<b>Bijsluiter</b>. De hyperlink naar het originele document werkt niet meer. Daarom laat Woogle de tekst zien die in dat document stond. Deze tekst kan vreemde foutieve woorden of zinnen bevatten en de opmaak kan verdwenen of veranderd zijn. Dit komt door het zwartlakken van vertrouwelijke informatie of doordat de tekst niet digitaal beschikbaar was en dus ingescand en vervolgens via OCR weer ingelezen is. Voor het originele document, neem contact op met de Woo-contactpersoon van het bestuursorgaan.<br><br>====================================================================== Pagina 1 ======================================================================

<pre>JKM330PP-72-A
310-330 Watt
                                                    (4BB)




                  KEY FEATURES
                                                                   4 Busbar Solar Cell:
                                                                   4 busbar solar cell adopts new technology to improve the efficiency of
                                                                   modules , offers a better aesthetic appearance, making it perfect for rooftop
                                                                   installation.

                                                                   High Power Output:
                                                Power
                                               Warranty
                                                                   Polycrystalline 72-cell module achieves a power output up to 330Wp.


                                                                   Anti-PID Guarantee:
                                                                   Limited power degradation of Eagle module caused by PID effect is
                                               PID-FREE
                                                                   guaranteed under 60℃/85% RH condition for mass production.


                                                                   Low-light Performance:
                                                                   Advanced glass and surface texturing allow for excellent performance in
                                      LOW LIGHT
                                                                   low-light environments.


                                                                   Severe Weather Resilience:
                                               2400 Pa
                                               5400 Pa             Certified to withstand: wind load (2400 Pascal) and snow load (5400 Pascal).


                                                                   Durability against extreme environmental conditions:
                                       RESISTANT                   High salt mist and ammonia resistance certified by TUV NORD.

                                                                   Temperature Coefficient:
                                                CLIMATE
                                                                   Improved temperature coefficient decreases power loss during high
                                               DURABILITY
                                                                   temperatures.



                                                LINEAR PERFORMANCE WARRANTY
                                                               10 Year Product Warranty          25 Year Linear Power Warranty




                                                                                                                       linear performance warranty
                                                       100%
                Guaranteed Power Performance




                                                       97.5%                   Add                                     Standard performance warranty
                                                                                   ition
                                                                                        al va
                                                            95.%                             lue f
                                                                                                  rom
                                                                                                        Jinko
                                                                                                                Sola
                                                            90.%                                                    r’s lin
                                                                                                                           ear w
                                                                                                                                arra
                                                                                                                                    nty


                                                       80.7%


                                                                                                                                                          years
                                                                   1           5                     12                                              25
</pre>

====================================================================== Einde pagina 1 =================================================================

<br><br>====================================================================== Pagina 2 ======================================================================

<pre>                                    992       40                                                                  942
                                                                                                                                                                            Current-Voltage & Power-Voltage
                                                             Ⅱ                                                                                                                       Curves (315W)
                                                                            Junction box




                                                                                                                              100
                                                                                       ＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸ




                                                                                 Ⅰ                                                                                12                                                    320
                                                             Ⅲ                                                                      Label                                  Cells temp = 25℃

                                                                       Installing Holes
                                                                                                                                                                  10       1000 W/m2                                    300




                                                                                                              L
                                                                                                                                                                           800 W/m2
 1956




                                                                    Ø
                                                                        4                                                                                         8                                                     250
                                                                  2-




                                                                                                                                                   1360
                                                                                                                                             860
                                                                  Grounding Holes                                                                                          600 W/m2
                                                                                                                                                                  6                                                     200


                                                                                                                                                                           400 W/m2
                                                                                                                                                                  4                                                     150
                                                                                     Cathode -                           + Anode
                                                                                                                  Connector                                                200 W/m2
                                                             A         A                                                                                          2                                                     100

                                                                                                                                                                                                                        50
                                                                                                                                                                  0                                                     0
                                                                                                                                                                       0               10      20     30   40      50




             ＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸＸ




                 Ⅰ                        Ⅲ

                                          9        5.5

                  55
                                                                                  40




                                                         5                                                        7.7
                                                    4.
                                3




                           8
        55




                                                    14




                                                                                                                                    35

                 Ⅱ




                                                                  JKM310PP-A                                                                 JKM315PP-A                          JKM320PP-A                 JKM325PP-A          JKM330PP-A

                                                                  STC                                         NOCT                           STC          NOCT                  STC           NOCT          STC         NOCT    STC    NOCT

                                                                 310Wp                                        231Wp                         315Wp         235Wp              320Wp            238Wp        325Wp 242Wp         330Wp 246Wp

                                                                 37.0V                                        33.9V                         37.2V         34.3V               37.4V           34.7V        37.6V    35.0V      37.8V   35.3V

                                                                 8.38A                                        6.81A                         8.48A         6.84A               8.56A           6.86A        8.66A    6.91A      8.74A   6.97A

                                                                 45.9V                                        42.7V                         46.2V         43.2V               46.4V           43.7V        46.7V    44.0V      46.9V   44.2V

                                                                 8.96A                                        7.26A                         9.01A         7.29A               9.05A           7.30A        9.10A    7.34A      9.14A   7.38A

                                                                            15.98%                                                                   16.23%                            16.49%                   16.75%            17.01%




Please send your enquiries to Australiasales@jinkosolar.com
                                                                                                                                                                                                                    AU-JKM-330PP-72-A_rev2016
</pre>

====================================================================== Einde pagina 2 =================================================================

<br><br>