<b>Bijsluiter</b>. De hyperlink naar het originele document werkt niet meer. Daarom laat Woogle de tekst zien die in dat document stond. Deze tekst kan vreemde foutieve woorden of zinnen bevatten en de opmaak kan verdwenen of veranderd zijn. Dit komt door het zwartlakken van vertrouwelijke informatie of doordat de tekst niet digitaal beschikbaar was en dus ingescand en vervolgens via OCR weer ingelezen is. Voor het originele document, neem contact op met de Woo-contactpersoon van het bestuursorgaan.<br><br>====================================================================== Pagina 1 ======================================================================

<pre>30141731
                                        Questionnaire
               for   collecting       data for the      drawing up of the
            BAT Reference Document (BREF) for Common
         Waste Gas Treatment in the Chemical Sector (the
                                         WGC BREF)
                                             July  2018
       European   IPPC Bureau
       JOINT RESEARCH CENTRE
       Directorate B -
                       Growth and Innovation
       Circular Economy and Industrial Leadership Unit
                                                                          0000000083
</pre>

====================================================================== Einde pagina 1 =================================================================

<br><br>====================================================================== Pagina 2 ======================================================================

<pre>30141731
      Drawing up    of the WGC BREF
                   Questionnaire for collecting data for the drawing up of the BAT
           Reference Document                     (BREF)     for Common Waste Gas Treatment in the
                                            Chemical Sector           (the  WGC      BREF)
          Please read the WGC BREF              questionnaire User's manual (separate document) and all the
          individual    questions   before    starting to collect data/information and fill in this questionnaire.
          This   questionnaire is designed for the collection of data for emissions to air from chemical
          installations   falling under the scope of the WGC BREF. The questionnaire also includes questions
          regarding     the  contextual information on techniques implemented and monitoring.
          This   questionnaire is    based     on  the outcome of the technical  working group (TWG)       Kick-off Meeting
          for the   drawing up of    the WGC BREF held in         September   2017 and the interim TWG       meeting held
          on   14-15 March 2018.
          The    questionnaire consists of the following set of sheets:
            1               Introductory notes
            J Installation identification and description
            rR Channelled emissions to air (sources)
             Ce
                      3.1   Periodic and/or continuous measurements
             ———
                      3.2 Contextual information        on  waste gas treatment   techniques
             ETRE
                      3.3   Process-specific      information
            .  NE
                           Diffuse emissions to air
             REE
                      4.1   Fugitive and    non-fugitive emissions
             pred
                      4.2 Mass balance exercise          (SMP)
            .               Endnotes
                                      Not all sheets of the     questionnaire are initially visible.
                       The relevant sheets will appear when data are entered in the appropriate cells.
              Macro options of Excel must be enabled. This template was designed with Excel 2010.
                                                       GENERAL WARNINGS:
            To make this       questionnaire as user-friendly as possible, many actions have been automated
            using    Excel's   programming functionalities (i.e. macros). These functionalities may only work
            within a precisely defined structure, which is that of the original questionnaire template
            provided by the European IPPC Bureau.
            Therefore, the original structure of this Excel template must not be changed, under any
            circumstances.
              In  particular,  do not:- fill in this questionnaire starting from any version other than the original
            blank template;
            -
               insert, delete, hide, unhide, modify the order or modify the names of a worksheet manually;
            -
               insert, delete, hide, unhide or modify a line or a yellow cell ofa worksheet manually;
            -
               modify the content, the format or any other property of a yellow cell;
            -
               insert a value or write text outside a white cell;
            -
               modify the format or any property, other than the content, of a white cell.You may:
            -
               enter information in the white cells using the required format (i.e. number, text or date).
                                                            Sheet 1. Introductory notes
                                                                                                                            0000000084
</pre>

====================================================================== Einde pagina 2 =================================================================

<br><br>====================================================================== Pagina 3 ======================================================================

<pre>30141731
         Savea non-confidential version of this questionnaire
                               Sheet 1.     Introductory     notes
                                                                   0000000085
</pre>

====================================================================== Einde pagina 3 =================================================================

<br><br>====================================================================== Pagina 4 ======================================================================

<pre>30141731
      Drawing up   of the WGC BREF
             [TU UE TINMEU IT DY TE  PETSUTT CUTTIPIELUITIY    UIE   UUESSLUUTITIIINE    UTT  DETIGIN   UT UTE  UPETAWUT  UT ITE
            neta llatinm-
            First  name    and  surname:
            Date of   completion:                                                        30/10/2018
            Job title:                                                          Environment coordinator
            E-mail
            Telephone:
                                                                               EEE               0   cao
            To be filled in   by the competent authority checking               the  quality   of the   questionnaire:
            Member State ¥                                                           Netherlands        (NL)
            Date of   quality  check:
            Organisation:
            First  name    and  surname:
            Job title:
            E-mail:
            Telephone:
                                       Only    to be used       by   MS     competent authorities
              Once the    questionnaire has been checked by the MS competent authorities, this                          button may
              be used to    automatically remove all information entered in the light red cells and                     save a non-
                                             confidential version of the questionnaire.
                                     Save a noncorficentiial version  of this questionnaire
                               J
            questionnaire:
            Industrial   organisation:
            Date of   completion:
            First  name    and  surname:
            Job title:
            E-mail:
            Telephone:
            To be filled in   by the TWG member(s)           from environmental NGOs               giving   assistance with
            completing     the questionnaire:
            Environmental NGO:
            Date of   completion:
            First  name    and  surname:
            Job title:
            E-mail:
            Telephone:
          In the event that you have doubts or difficulties when completing this questionnaire,                          please  do not
                                        hesitate to contact the European IPPC Bureau,
                                                                5.1.2e                      .         "
                                                                    512e51.2e517%
          Telephones:        ERR       5.1.2e       Tel. +34           EF               IEEE       IEEE:       Tel. +34  IEE
                                                            Sheet 1.      Introductory     notes
                                                                                                                                        0000000086
</pre>

====================================================================== Einde pagina 4 =================================================================

<br><br>====================================================================== Pagina 5 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Sheet 1. Introductory notes
                                                             0000000087
</pre>

====================================================================== Einde pagina 5 =================================================================

<br><br>====================================================================== Pagina 6 ======================================================================

<pre>30141731
      Drawing up   of the WGC BREF
                                         INFORMATION ABOUT THIS QUESTIONNAIRE
            Industrial Emissions Directive and BREFs
            The   Industrial Emissions Directive    (2010/75/EU) of 24 November 2010 (IED) replaced the Integrated
            Pollution Prevention and Control     (IPPC) Directive (2008/1/EC) and related legislation on industrial
            emissions. Under the IPPC Directive and now the IED, a Best Available Techniques (BAT) Reference
            document (BREF) is the vehicle through which BAT (and emerging techniques) are determined in a
            transparent manner, based on sound techno-economic information. The key elements of BREFs (i.e.
            'BAT conclusions') are adopted through a Committee procedure and are the reference for setting
            permit conditions of installations covered by the IED. Each BREF is the outcome ofa three- to four-
            year process involving numerous experts, representing industry, Member States, environmental NGOs
            and services of     the Commission.
            Information      exchange      under the IED for the      drawing up     of the Common Waste Gas
            Treatment in the Chemical Sector             (WGC)    BREF
            The  European IPPC Bureau (EIPPCB) is part of the Circular Economy and Industrial Leadership Unit
            of Directorate B    -
                                  Growth and Innovation. Directorate B is   one  of the scientific directorates of the
            European Commission's Joint Research Centre (JRC). It organises the exchange of information
            between Member States, the representatives of the industries concerned, environmental NGOs and
            the Commission, on the best available techniques (BAT) under Article 13(1) of the IED. The objective
            of the information exchange exercise is to draw up and review BREF documents. All the information in
            the context of the drawing up of this BREF is exchanged via an electronic system (BATIS), except for
            confidential and sensitive information. Only registered members and JRC staff are allowed to submit
            and view information. The BATIS privacy statement can be consulted on the EIPPCB website:
            hitp://eippcb.jrc.ec.europa.eu/batis/downloadPdf?name=Privacy Statement BATIS                   DPO-1586.pdf
            The  personal data requested about the persons who filled in or checked the questionnaire will only be
            used   so that they can be contacted if questions arise when the EIPPCB analyses the data. Should you
            have any queries concerning the processing of your personal data, please address them to the
            secretariat of the Circular Economy and Industrial Leadership Unit:
            IEEEFTIN
            The work       the
                                © curopa cu
                        on       drawing up ofthe WGC BREF officially started with the activation in September 2016
            of the  Technical   Working   Group (TWG) formed especially for this purpose. The Kick-off Meeting (KoM)
            of the TWG was held in Seville from 25 to 29 September 2017 (the KoM report is available on the
            EIPPCB website at http://eippcb.jrc.ec.europa.eu/reference/). The primary purpose of this
            questionnaire is to collect data and contextual information to derive the Best Available Technique
            (BAT) conclusions for the WGC BREF, regarding the emissions to air from chemical installations.
            Moreover, the data collected will be used to draw up the 'Current emission levels' and "Techniques to
            consider in the determination of BAT'     chapters  of the WGC BREF.
            Purpose      of this   questionnaire
            The purpose of this questionnaire is to obtain plant-specific information and data regarding the
            environmental performance of existing chemical installations in the scope of the WGC BREF. This
            questionnaire    is one  of the sources of information for the WGC BREF drawing-up process.
            Member States       are responsible, with the support of the industrial organisations, for collecting and
            checking the filled-in questionnaires so that the EIPPCB can have them all returned by the strict
            deadline of 21/12/2018.
            The  quality of the data provided is fundamental for deriving sound BAT conclusions. Therefore
            this questionnaire should be filled in very carefully and as exhaustively as possible.
            What    type of information is requested
            Please submit the information that you have available and/or that you         are able to collect. Please
            provide information and descriptions and plant-specific and process-specific data on emissions and
            consumption. You may attach additional supporting documents to provide other relevant information
            together with this questionnaire.
                                                          Sheet 1.   Introductory   notes
                                                                                                                         0000000088
</pre>

====================================================================== Einde pagina 6 =================================================================

<br><br>====================================================================== Pagina 7 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Sheet 1. Introductory notes
                                                             0000000089
</pre>

====================================================================== Einde pagina 7 =================================================================

<br><br>====================================================================== Pagina 8 ======================================================================

<pre>30141731
      Drawing up   of the WGC BREF
            Handling     confidential business information              (CBI)
            The  exchange     of information under the IED should not lead to the       breaching of either EU or national
            competition laws or other laws designed to protect legitimate economic interests. The information
            submitted by filling in this questionnaire will be used solely for the purpose of the drawing up ofthe
            WGC BREF. This questionnaire has been designed to focus on emission data that, in principle, should
            not be confidential.
            However, the TWG has decided that they will need to collect           some   contextual information   on the waste
            gas treatment techniques and specific processes/products. A small proportion of this information will be
            treated as confidential business information (CBI) and is to be reported in the light red cells.
            The  operator will:
            »
              send the full  questionnaire (containing CBI) to the Member State (MS) for checking;
            »
              send the process flow diagram(s) showing the waste gas treatment systems and any other supporting
            documents to the MS; the process flow diagrams and other supporting documents should not contain
            any CBI.
            The Member State        (MS) representative will:
            »
              check the  quality, completeness and consistency         of the information in the full questionnaire;
            »
              create and   save a    non-confidential version of the   questionnaire, using the button provided above;
            +
              post the non-confidential version of the questionnaire, and any other supporting documents onto
            BATIS, so that they will be shared with the whole TWG;
            «
              send the full version of the questionnaire (containing CBI) to the EIPPCB by email.
            The EIPPCB will:
            «
              anonymise the full questionnaires (containing CBI information) by allocating a CBI reference number
            to each  installation; this reference will be used to identify the installation whenever CBI is used as part
            of the data assessment and analysis;
            +
              store the full questionnaires, (containing CBI information) and the reference number information, in
            access-restricted and password-protected electronic folders; the information will only be used by the
            Head of the EIPPCB and the BREF authors for the purposes of producing the WGC BREF;
            +
              send each MS      a list of all the installation names  and CBI reference numbers for the installations in
            that MS; this will allow the MS to check        on the performance of their installations whenever anonymised
            information is used by the EIPPCB.
            The MS will:
            «
              inform each installation of their CBI reference       number; this will allow each installation to identify their
            data whenever      anonymised information is used by the EIPPCB.
                                                              Sheet 1. Introductory    notes
                                                                                                                                0000000090
</pre>

====================================================================== Einde pagina 8 =================================================================

<br><br>====================================================================== Pagina 9 ======================================================================

<pre>30141731
      Drawing up   of the WGC BREF
                                             SCOPE OF THE DATA COLLECTION
            The scope ofthis data collection covers channelled and diffuse emissions to air from
            chemical installations (Section 4 of Annex | to Directive 2010/75/EU) of the following
            (groups of) substances:
              (Groups of) Substances         included in the scope                       Comments
               1,3-Butadiene
              Ammonia (NH3)
              Benzene
              Carbon    disulphide (CS3)                               only  for viscose   production
              Carbon monoxide
              Chloromethane
              Dichloromethane
              Dust                                                     including PM       and PM25s data*
              Elementary     chlorine  (Ch)
              Ethylene dichloride (EDC)
              Ethylene oxide
              Formaldehyde
              Gaseous chlorides (expressed as HCI)                     including   HCI data”
              Gaseous fluorides (expressed as HF)
              Hydrogen cyanide (HCN)
              Hydrogen sulphide (H.S)                                  only  for viscose   production
              Lead and its compounds (as Pb)
              Nickel and its compounds (as Ni)
              Nitrogen oxides (NOx), expressed as NO;
              Nitrous oxide (N2O)
              PCDD/Fs      (dioxins +
                                       furans)                         as  |I-TEQ  or  WHO-TEQ*
              Propylene     oxide
              Sulphur   oxides   (SOx), expressed   as SO;
              Tetrachloromethane       (CCls)
              Toluene
              Trichloromethane
                                                                       if TVOC data     are not available then
              TVOC     (Total volatile organic compounds)              report  data   as NMVOC    (non-methane
                                                                       VOOQ).
              Vinyl  chloride  monomer     (VCM)
            *
               When such data      are  available.
            The scope     ofthis  data collection also covers channelled and diffuse emissions to air from:
            -
              chemical    plants which carry out the physical   purification and reconcentration of spent
            sulphuric   acid and do not use sulphur dioxide     as a feedstock, if they are co-
            located/integrated/associated with a process that is included in the scope of the WGC BREF;
            -
               reformers, if they are co-located/integrated/associated with a process that is included in the
            scope of the WGC BREF and standalone reformers;
            -
              the storage, transfer and handling of materials only where these are directly associated with
            the chemical production process. This includes the combined treatment of waste gases in
            those cases where a share of the pollutant load originates from the storage, transfer and
            handling of materials.
                                                       Sheet 1.  Introductory  notes
                                                                                                               0000000091
</pre>

====================================================================== Einde pagina 9 =================================================================

<br><br>====================================================================== Pagina 10 ======================================================================

<pre>30141731
      Drawing up  of the WGC BREF
                                 SCOPE OF THE DATA COLLECTION: EXCLUSIONS
            The  following emissions are excluded:
            1) Channelled and diffuse emissions from plants producing chlorine, hydrogen,            and
            sodium/potassium hydroxide by the electrolysis of brine (see CAK BREF).
            2) Channelled emissions from       plants producing the following organic chemicals in
            continuous processes where the total      production capacity of those chemicals exceeds     20 kt/yr
            (see LVOC BREF):
            -
              Lower olefins via the steam  cracking process;
            -
              Formaldehyde;
            -
              Ethylene oxide  and ethylene glycols;
            -
              Phenol from   cumene  oxidation;
            -
              Dinitrotoluene (DNT) from toluene, toluene diamine (TDA) from DNT, TDI from TDA,
            methylene diphenyl diamine (MDA) from aniline, MDI from MDA;
            -
              Ethylene dichloride (EDC) and vinyl chloride monomer (VCM);
            -
              Hydrogen peroxide,
            except for emissions of NOx from thermal oxidisers, which are included in the scope               of
            this data collection.
            NB: Diffuse emissions from the aforementioned            plants  are included in the scope of this
            data collection.
            3) Channelled and diffuse emissions from         plants producing   the following inorganic
            chemicals
            (see LVIC-AAF and LVIC-S BREFs):
            -
              Ammonia;
            -
              Calcium carbide;
            -
              Carbon black;
            -
              Hydrofluoric acid, phosphoric acid, nitric acid, sulphuric acid;
            -
              Inorganic phosphates;
            -
              Phosphorus-, nitrogen- or potassium-based fertilisers (simple or compound fertilisers);
            -
              Soda ash, calcium chloride and precipitated calcium carbonate;
            -
              Sodium chlorate;
            -
              Sodium silicate;
            -
              Synthetic amorphous silica (SAS);
            -
              Titanium dioxide, ferrous chloride and ferrous sulphate (copperas).
            4) Channelled and diffuse emissions from:
                     -
                       combustion  plants (see  LCP BREF and MCP        Directive), except  for process
            the chemical industry with  a total rated thermal input equal to   or greater than 1 MW,
            which   are  included in this data  collection;
              process furnaces/heaters with   a  total rated thermal  input below 1 MW;
            -
              process furnaces/heaters used in lower olefins and      ethylene dichloride  crackers.
            -
            5) Channelled and diffuse emisisons from waste incineration           plants (see  WI BREF).
            6) Channelled and diffuse emissions from indirect         cooling systems (see    ICS BREF).
                                                     Sheet 1.  Introductory  notes
                                                                                                                  0000000092
</pre>

====================================================================== Einde pagina 10 =================================================================

<br><br>====================================================================== Pagina 11 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
           2    Installation identification and          description
                                                                            MgO-Proces (wet-route)
                                                                                    Nedmag bv
                                            ¥|
                                Country           Netherands (NL)   |
                                       City                            Veendam                                      |
                               Name  o         hed files           |           Document description               |
                           NL_Nedmagbv_MgOprroces_1                     Diagram of the Magnesia process
                                                                                 UT UTE
                                                                      LESLIE                     id PTULESS TWiST
                                                                                         TMdaUITea
                           NL Nedmagbv MgOprroces         7                             rewaiteh
                           NL Nedmagbv MgOprroces 3                     Part of de  permit emissions part  1
                          NL_Nedmagbv_MgOPrroces          4             Part of de permit emissions part   2
                                                                         Sheet 2. Installation
                                                                                                                      0000000093
</pre>

====================================================================== Einde pagina 11 =================================================================

<br><br>====================================================================== Pagina 12 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
           3    Channelled emissions to air
                                                               Bl       -
                                                                   y
                                                                                               Teg
                                                                  other   inorganic compounds such as
                                                                     calcium    carbide, silicon, silicon
                                                                                     ic] rhide
                                                                          Magnesium compounds                      1 shaftkiln  (F3102}
                                                                                  Continuous
                                                                      24    hiday and        7 days/week.
                                                                                  = 100
                                                                                              000
                                                                   TZ E MON-TEEs, Metal URES or
                                                                  other inorganic compounds such as
                                                                     calcium carbide, silicon, silicon
                                                                                     rarhide
                                                                          Magnesium compounds                      1 shatftkiln (F3202)
                                                                                  Continuous
                                                                      24    hiiday and       7 days/week.
                                                                   a ZB
                                                                                  =
                                                                                      100 000
                                                                           TTUT=TTTSIa
                                                                                         le, TIE Tal DA RIE UT
                                                               |
                                                                  other   inorganic compounds such as
                                                                     calcium carbide, silicon, silicon
                                                                                     rarhide
                                                                          Magnesium compounds                       Dust fitter 33102
                                                                                  Continuous
                                                                      24    hi'day and 7 days/week.
                                                                   FZ
                                                                                  =
                                                                                      100 Tetdl
                                                                                              000 OEes OT
                                                                           MON-TETErs,
                                                               |
                                                                  other   inorganic compounds such as
                                                                     calcium carbide, silicon, silicon
                                                                                     £3 rhide
                                                                          Magnesium compounds                       Dust fitter 33202
                                                                                  Continuous
                                                                      24    hi'day and 7 days/week.
                                                                                  >=  100 000
                                                                   a £5    TUTTE      La ls,  TIE
                                                                                                  Lal UA Ress Ul
                                                                  other   inorganic compounds such as
                                                                     calcium carbide, silicon, silicon
                                                                                     rarhide
                                                                          Magnesium compounds                    Dustfiter DBM     $3117
                                                                                  Continuous
                                                                      24    hiiday and       7 days/week.
                                                                   FL €
                                                                                  =
                                                                                       100 TNETdl
                                                                                              000 TEES OT
                                                                           TIOT-TTETATS,
                                                               |
                                                                  other   inorganic compounds such as
                                                                     calcium carbide, silicon, silicon
                                                                                     rarhids
                                                                          Magnesium compounds                    Dustfiter DBM 53217
                                                                                  Continuous
                                                                      24    hi'day and 7       days/week.
                                                                                  =
                                                                                      100 000
                                                       =
                                      2
                                   TIOOO COT   Tapa Ty   |
                                          Type of process ¥
                                     recess operating time ¥
                                                 Fa CITE TTTET
                                                                                                                             Sheet 3. Channeled emissions
                                                                                                                                                          0000000094
</pre>

====================================================================== Einde pagina 12 =================================================================

<br><br>====================================================================== Pagina 13 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Sheet 3. Channeled emissions
                                                              0000000095
</pre>

====================================================================== Einde pagina 13 =================================================================

<br><br>====================================================================== Pagina 14 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                  Fro     Bera               je ¥
                                 (0k
                                  FICO
                                      U LOT (Tr AAI 0 SLY
                                            Capa
                                                      Sh {CUTORT
                                                                 1
                I                RE
                                 Process op
                                 nll LL     Le eA
                                                                hl
                                 ALARA                  CY LUV]
                                                                =
                                                                   Sheet 3. Channeled emissions
                                                                                                0000000096
</pre>

====================================================================== Einde pagina 14 =================================================================

<br><br>====================================================================== Pagina 15 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                                                                                _
                                                           IE
                                                                                  _
                                                         other inorganic compounds such as
                                                           calcium    carbide, silicon, silicon
                                                                          | rhide
                                                               Magnesium compounds                Calciner fumacs F3101
                                                                        Continuous
                                                             24 hrday and     7 days/week.
                                                                        =
                                                                           100 000
                                                          a LB  ITU-T
                                                                       labs,
                                                                               THE
                                                                                    Tal ARIES UT
                                                       |
                                                         other inorganic compounds such as
                                                           calcium carbide, silicon, silicon
                                                                          rarhide
                                                               Magnesium compounds                Calciner furmace F3201
                                                                        Continuous
                                                             24 hr'day and 7 days/week.
                                                                        =  100 000
                                                          = Ze  TTU-Meldls,    Tetldl Wiles oF
                                                       |
                                                         other inorganic compounds such as
                                                           calcium carbide, silicon, silicon
                                                                          rarhide
                                                               Magnesium compounds                    Shaftkiln F3102
                                                                        Continuous
                                                             24 hr'day and    7 days/week.
                                                                        = 100 000
                                                          TZ    MON-TETals, metal Danes or
                                                       |
                                                         other inorganic compounds such as
                                                           calcium carbide, silicon, silicon
                                                                          rarhide
                                                               Magnesium compounds                    Shatftkiln F3202
                                                                        Continuous
                                                             24 hr'day and 7    days/week.
                                                                        =  100000
                                 |
                                  [--               x
                                             Product v
                                      Type ofprocess  ¥|
                                                                                                              Sheet 3. Channeled emissions
                                                                                                                                           0000000097
</pre>

====================================================================== Einde pagina 15 =================================================================

<br><br>====================================================================== Pagina 16 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Sheet 3. Channeled emissions
                                                              0000000098
</pre>

====================================================================== Einde pagina 16 =================================================================

<br><br>====================================================================== Pagina 17 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                                    :
                                   Yes{Flease explain why)
                                                           who are changed regulary.
                                 |                                 of dust
                                                           Controle is based on
                                                                                     Sheet 3. Channeled emissions
                                                                                                                  0000000099
</pre>

====================================================================== Einde pagina 17 =================================================================

<br><br>====================================================================== Pagina 18 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.1   Channelled emissions to air monitored                               periodically       and associated waste gas treatment                           system                        Emission       point     ID   (custom):          $3104                       Emission       point   ID (automatic):
                                                                                                                                                                                                                                                                                                                      | P1
                                                                                                                                                                                                                                                                                                                           |
          1                   Information          on  waste gas
                                                                                                                       Indicate which (groups of) substances            are monitored                 ¥                                   Indicate which (groups of) substances     are  monitored
                                                                                                                    Cana       1,3-Butadiene                                                                                            HF        [Gaseous fluorides   (expressed   as  HF)
                                                                                                                    MH       Ammonia                                                                                                   HCM        Hydrogen cyanide
                                                                                                                    Cena      Benzene                                                                                                   Has       Hydrogen sulphide, (only for viscose production)
                                                                                                                              Carbon                         for viscose                                                                Pb        Lead and its
                                                                                                                    CS:                  disulphide, (only                  production)                                                                          compounds
                                                                                                                     CoO      Carbon monoxide                                                                                           Mi        Mickel and its   compounds
                                                                                                                   CHac       Chloromethane                                                                                            MO         [Nitrogen  oxides  (expressed  as  NOx
                                            .                        ;
                                                                                                                   CHzze        |Dichloromethane                                                                                       Maa        Mitrous oxide
                                      Monitored substances           in the waste gas                                            i
                                                                                                                                                                                                                                                    :
                                                                                                                                                                                                                                                                 g
                                                       calculated Please indicate if the                         PCDD/F       Dioxins and furans                                                                                      Caso        Propylene    oxide
                                 (measured         or
                                substance is                             if so, please fill in
                                                     monitored, and,                                                          Dust                                                                   Yes                               S04        Sulphur   oxides  (expressed  as  S03
                                       the associated lines        in  block    4 below.                                      Dust   -
                                                                                                                                       PMzs                                                                                            CCl,       Tetrachloromethane
                                                                                                                              Dust   -
                                                                                                                                       Pg                                                                                              Cra        Toluene
                                                                                                                     Ck       Elementary chlorine                                                                                     CHCl;       Trichloromethane
                                                                                                                   Cansciz    [Ethylene    dichloride   (EDC)                                                                         Cane        Win   chloride   monomer  (WVCM)
                                                                                                                    Caran     Ethylene     oxide                                                                                   MMWVOC           Mon-methane volatile  organic compounds
                                                                                                                    CHao      Formaldehyde                                                                                            TVOC        Total volatile organic compounds
                                                                                                                     HCI      (Gaseous chlorides       (expressed      as HC)
                                                           Comments
          2                   Information          on  waste gas treatment         system
                                                                                                                                                                                     Justification/frationale for using this technigue      or
                                                                                                     Waste gas treatment   technique ¥           Abatement /       Recovery   ¥                                                                                              Comments
                                                                                                                                                                                                  COHIbTSton sLLrb igus
                                                 ’                                         :
                                                                                                           un                 i
                                                                                                                                                                                                                              :     :
                                                                                                                                                                                                                                                    Hot air from the  DBM cooler is going through the   cyclone to
                                    1          Final abatement                  technique                Gravitational                                    Abatement                         To           dust form the
                                                                                                                                                                                                            AR
                                                                                                                                                                                                                         cooling  air
                                                                                                                                                             ]
                                                                    or recovery                                         separation                                                              remove
                                                                                                                                                                                                                                                                   remove  dust from  the cooling air
                                              Other abatement or recovery technigue
                                    2
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    3
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    4
                                              applied before final abatementirecovery
                                              Other abatement or recovery technigue
                                    5
                                              applied before final abatementirecovery
                                 What    are    the main factors which influence the                                                                                           ;                                         ;
                                                                                                                                                                                                                                               ii
                                                                                                                                                                        Compliance   ELV   (BREF    LVIC-S0 and    permit of Dutch authorities)
                                   deoanlopetaior ol he Shae                 ent    sysen
                               If there is     no   waste gas treatment         system   or  the
                                 generic techniques cannot be applied. please
                                                          explain why
          3                   Other information
                                                                                                  CMR 1A/1B
                                                                                                                              lacute toxicity]      Origin of
                                       Properties       of the midture/preparation:              Ty              CMR ¥ 2      |byinhalation |      hazardous                      Comments
                                                                                                                                     Y          substances W
                                                                                                       =
                                           If the group Dust is monitored:                       Mo            Mo
                                  If the group        TVOC   or NMVOC is monitored:              [No           Mo
                                                                                                      When the concentration of                                     below the quantification limit, what
                                                                                                                                    individual congeners
                                                                                                                             concentration
                                                                                                                                                                is the sum? ¥
                                                                                                                                                                                                                           CRE
                                                                                                                                                is  reported   in
                            |           If the group Dioxins is monitored:
                            |       Additional information        on   batch processes
                                  Specify      the reference conditions         as set in the
                               permit if they differ from the following conditions:
                                dry gas, temperature of 273.16 K a pressure of
                                                           101.3 kPa.
                            |              If relevant, reference Oz         coe)
                                                                                                                                                                                                                                                             Sheet 3.1. Measurement      (P1)
                                                                                                                                                                                                                                                                                                                             0000000100
</pre>

====================================================================== Einde pagina 18 =================================================================

<br><br>====================================================================== Pagina 19 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                                                                                             ence 0 content (a).
          lo                     —
                                               |
                                                        i
                                                                                              Other                                TTTee
                                                                                                                                   singe
                                   2018 Seu: |
                                                  Compliance
                                                  manitoring
                                                             Yearly           halthourly  | (Specifyin 53.10
                                                                                                                                 a
                                                                                            comments)
                                                        ;
                                                                                              Other                               Three
                                                                                                                                  singles
                                   2017
                                        Sa        Compliance
                                                  monitoring
                                                             Yearly           halfhourly  | (Specifyin 43.80
                                                                                            comments)                            eas rem
                                                                                                                                  Three
                                        EM 13284- Compliance
                                                                              halthourly      Other    44.00
                                                                                                                                  singles
                                   2016
                                        [oooh     Riis       Yearly
                                                                                            gry                                  ges
                                                                                                                                    ents
                                   2017
                                   2016
          |
                                   2015
                                   2017
                                   2016
                                   2075
            _
                                   2017
            g
                                   2016
                                   2075
                                   2017
                                   2016
                                   2015
                                   2017
                                   2016
                                   2075
                                                              Sheet 3.1. Measurement  (P1)
                                                                                                                                          0000000101
</pre>

====================================================================== Einde pagina 19 =================================================================

<br><br>====================================================================== Pagina 20 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                   ,
                                                           2017
              Formaldehyde    Hy
                                         mg/Nm?
                                               Tiel.
                                                         | 2016
                      (Cho                                 2015
                                 )                         2017
           Gaseous chlorides
                          3
                                       |mg/Nm?
                                            __
                                                       4
                                                         | 2016
                      (HCI)                                2015
                                                           2017
           a
           Gaseous fuoides | mom? |                        2076
                                                           2015
                ora                                        2017
           Hydrogen cyanide | nm                           2076
                    iil                   _
                                                           2015
           Hydrogen sulphide |              _
                                                           (—201C
                      {Rn                                  2015
                                                           2017
                 Lead and its                    Ch        =
                                         gi
            compounds (Pb)                                      ;
                 ST           LT                           2017
               Nickelandits                 |__|   NT
             compounds (Ni)            |                   a
             Nitrogen oxides |
                             2
                                               |
                                                  Nm?      =
                                                           2015
                                                           2017
           Mitrous oxide (Many           |mg/Mm?® |        2016
                                                           2015
             Propylene oxide
                      Cus
                                       |       }
                                                  Nm?      cu
                                                           2015
                    ;          i                           2017
              Sulphur       oxides
                                         |mgim? |
                                     *
                   i                                       2016
                      80,
                                                           2015
                          ]
                                                           2017
          Tetrachloromethane|                     ws       T5578
                      {CCl
                                                           2015
                                                           2017
              Talu ene (Corre            mg/Mm?            2016
                                                           2015
               ;                                           2017
            Trichloromethane | [ro        ___
                                                            rer
                    ore
                                                           2017
               Vimy chloride
            monomer          (VCM)     |mg/Nm*|            2016
                    (Canc                                  2015
               wa                                          2017
             volatile organic                     Nm       [2076
                 compounds
                                               3
                                                            :
                                                           2014
                  FINIYAN   aad
                                                           [2017
                Total volatile                       —
          organic compounds| mg/Nm* |                      2016
                   {TVOC)                                  2015
                                                                  Sheet 3.1. Measurement (P1)
                                                                                              0000000102
</pre>

====================================================================== Einde pagina 20 =================================================================

<br><br>====================================================================== Pagina 21 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Gravitational          separation
           1    Identification
              |       Technique    associated with   point of emission:                      P1
           2    Removed substances
                                                                Substance
                                                                                 Removal          Removal
                                                                               purpose ¥       [efficiency (%)
                Removed substance 1 ¥                              Dust        Abatement
                                                                                  primary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments
                Information    on  the gravitational separation equipment
                Type   ¥                                                        Cyclone
                Start of  operation (year)                                         1980
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                                    Sampling  and measurements
                Operating time of the equipment (h/yr)                             8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                no
                VWdsSTE  Uds TEAUITETIIS]  MTT Ta5T Ul
                                                                                    Fo
                Deriving method for removal efficiency                        Design   value
              |                  Comments
                Waste gas     properties  after the   gravitational separation equipment
                    Do the waste gas properties vary
                  significantly under normal operating              No
                               conditions? ¥
                Measurement       point number                       1               2                3                5           6         7 10 fi 12
                Flow  (Nm2/h)                                    12800.0
                Humidity (%)                                       3.40
                Temperature (°C)                                   315
                Comments
           5    Operational    data for  gravitational separation      -
                                                                         consumables
                                                                                                               Sheet 3.2. Gravit. sep. (P1)(1)
                                                                                                                                                        0000000103
</pre>

====================================================================== Einde pagina 21 =================================================================

<br><br>====================================================================== Pagina 22 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                    42
                                 04/2018
                                         Sheet 3.2. Gravit. sep. (P1)(1)
                                                                         0000000104
</pre>

====================================================================== Einde pagina 22 =================================================================

<br><br>====================================================================== Pagina 23 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.3   Process furnace/heater
                                                            Other  (Specify in comments)
                                                                  Magnesium oxide
                                        I   The furnace is  a shaftkiln for sintering the magnesiumoxide
                                        |
                                 /heate                             direct-heating
                                                                           Air
                                          Other (Specify in
                                             comments)
                                           Wet scrubbing
                                            with caustic
                                             Optimised
                                            combustion
                                              Wet dust
                                             scrubbing
                                                    Natural gas
                                        brkina packed    bed  (MgO Briquettes) shaftkiln with  dirct contact between the burners and the MgO briquettes
                                                                                                                                 Sheet 3.3. Process f-h (P1)(1)
                                                                                                                                                                0000000105
</pre>

====================================================================== Einde pagina 23 =================================================================

<br><br>====================================================================== Pagina 24 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.1   Channelled emissions to air monitored                            periodically      and associated waste gas treatment                      system                       Emission        point   ID  (custom):          [$3204                      Emission        point  ID (automatic):
                                                                                                                                                                                                                                                                                                          | P2
                                                                                                                                                                                                                                                                                                               |
          1                 Information         on  waste gas
                                                                                                                   Indicate which (groups of) substances       are monitored                ¥                                 Indicate which (groups of) substances     are  monitored
                                                                                                                Cana       1,3-Butadiene                                                                                    HF        [Gaseous fluorides   (expressed   as  HF)
                                                                                                                MH       Ammonia                                                                                           HCM        Hydrogen cyanide
                                                                                                                Cena      Benzene                                                                                           Has       Hydrogen sulphide, (only for viscose production)
                                                                                                                          Carbon                       for viscose                                                          Pb        Lead and its
                                                                                                                CS:                disulphide, (only               production)                                                                       compounds
                                                                                                                 CoO      Carbon monoxide                                                                                   Mi        Mickel and its   compounds
                                                                                                               CHac       Chloromethane                                                                                    MO         [Nitrogen  oxides  (expressed  as  NOx
                                          .                       ;
                                                                                                               CHzze        |Dichloromethane                                                                               Maa        Mitrous oxide
                                    Monitored substances          in the waste gas                                           i                                                                                                                       g
                                                    calculated Please indicate if the                        PCDD/F       Dioxins and furans                                                                              Caso        Propylene    oxide
                               (measured        or
                              substance is                            if so, please fill in
                                                   monitored, and,                                                        Dust                                                             Yes                             S04        Sulphur   oxides  (expressed  as  S03
                                     the associated lines       in  block    4 below.                                     Dust  -
                                                                                                                                  PMzs                                                                                     CCl,       Tetrachloromethane
                                                                                                                          Dust  -
                                                                                                                                  PMiq                                                                                     Cra        Toluene
                                                                                                                 Ck       Elementary chlorine                                                                             CHCl;       Trichloromethane
                                                                                                               Cansciz    [Ethylene  dichloride   (EDC)                                                                   Cane        Win   chloride   monomer  (WVCM)
                                                                                                                Caran     Ethylene   oxide                                                                              MMWVOC          Mon-methane volatile  organic compounds
                                                                                                                CHao      Formaldehyde                                                                                   TVOC         Total volatile organic compounds
                                                                                                                 HCI      (Gaseous chlorides     (expressed   as HC)
                                                        Comments
          2                 Information         on  waste gas treatment         system
                                                                                                                              ;
                                                                                                                                                                            Justification/rationale for using this technigue    or
                                                                                                 Waste gas treatment   technique ¥          Abatement /   Recovery   ¥                                                                                           Comments
                                                                                                                                                                                        COHIbTSton sLLrb igus
                                                                                                                                                                                                                                        Hotairfeme DEM                           trough the cydone io
                                  1          Final abatement     or recovery technigue               Gravitational  separation                      Abatement                      to remove dust from the    cooling air                                      id
                                            Dther abatement or recovery technigue
                                  2
                                            applied before final abatement/fre covery
                                            Other abatement or recovery technigue
                                  3
                                            applied before final abatementfe covery
                                            Other abatement or recovery technigue
                                  4
                                            applied before final abatement/re covery
                                            Other abatement or recovery technigue
                                  5
                                            applied before final abatement/re covery
                               What    are    the main factors which influence the                                                                                     i                                        ;                 _
                                                                                                                                                                 Compliance  ELV   (BREF   LMC-50 and     permit Dutch authorities)
                                 dosaninalor LIL: Shale                   SED SuF on)
                             If there is     no  waste gas treatment         system   or the
                               generic technigues cannot be applied. please
                                                       explain why
         k]                 Other information
                                                 )
                                                                                              CMR 1AMB
                                                                                                                          lAcute toxicity]    Origin of
                                                                                  i
                                     Properties      of the midture/preparation:                   =
                                                                                                             CMR ¥ 2      |byinhalation |    hazardous                   Comments   ;
                                                                                                                                 Y         substances W
                                                                                                   =
                                         If the group Dust is monitored:                     Mo            Mo
                                If the group TVOC or NMVOC is monitored:                     [No           Mo
                                                                                                  When the concentration of individual congeners is below the quantification limit, what
                                                                                                                                      3                 ;
                                                                                                                                                                                                               Comments
                                                                                                                         concentration is reported in the sum? ¥
                                      If the group Dioxins is monitored:
                                  Additional information       on   batch processes
                                Specify      the reference conditions        as set in the
                             permit if they differ from the following conditions:
                              dry gas, temperature of 273.16 K a pressure of
                                                        101.3 kPa.
                                         If relevant, reference Oz        mee)
                                                                                                                                                                                                                                                 Sheet 3.1. Measurement      (P2)
                                                                                                                                                                                                                                                                                                                 0000000106
</pre>

====================================================================== Einde pagina 24 =================================================================

<br><br>====================================================================== Pagina 25 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                                                                                                                             remni
                                                                                                                                                    Three
                                               ,                      —
                                                                                                                Other                                on
                                       wa
                                            Film 0.3000 35.0000
                                                                ls eg      Yes Yearly           halfhourly                 3160  | 33.30 | 3550    Singes
                                                                                                              Seri                                  ments
                                                                                                                Other                               Three
                                       Wir
                                            EL   0.3000 35.0000
                                                                Seg        Yes Yearly           halthourly                 4460  | 44.90 | 44.00   Sings
                                                                                                              Sky                                   ments
                                                                      i
                                                                                                                Other                               Thize
                                       mis
                                            Bla  0.3000 35.0000
                                                                Somelizncy
                                                                monitoring
                                                                           Yes
                                                                               Yearly           halfhourly  | OTs)
                                                                                                              (Specifyin | 37.50 | 32.30
                                                                                                                                         | 39.60    sings,
                                                                                                                                                   maAsuay
                                       2017
                                     |
          |
              Dust-PMs         mgm     2076
                                       2015
                                       2017
               ust
                   -    PM       ng!
                                       2016
                                       2015
                             |         2017
                            hh
                                       2016
                                       2015
                           —
                                       2017
                      So
                                       2016
                               |       2015
                                       2017
                               | ng    2016
                               |       2015
                                                                                Sheet 3.1. Measurement  (F2)
                                                                                                                                                           0000000107
</pre>

====================================================================== Einde pagina 25 =================================================================

<br><br>====================================================================== Pagina 26 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                   ,
                                                           2017
              Formaldehyde    Hy
                                         mg/Nm?
                                               Tiel.
                                                         | 2016
                      (Cho                                 2015
                                 )                         2017
           Gaseous chlorides
                          3
                                       |mg/Nm?
                                            __
                                                       4
                                                         | 2016
                      (HCI)                                2015
                                                           2017
           a
           Gaseous fuoides | mom? |                        2076
                                                           2015
                ora                                        2017
           Hydrogen cyanide | nm                           2076
                    iil                   _
                                                           2015
           Hydrogen sulphide |              _
                                                           (—201C
                      {Rn                                  2015
                                                           2017
                 Lead and its                    Ch        =
                                         gi
            compounds (Pb)                                      ;
                 ST           LT                           2017
               Nickelandits                 |__|   NT
             compounds (Ni)            |                   a
             Nitrogen oxides |
                             2
                                               |
                                                  Nm?      =
                                                           2015
                                                           2017
           Mitrous oxide (Many           |mg/Mm?® |        2016
                                                           2015
             Propylene oxide
                      Cus
                                       |       }
                                                  Nm?      cu
                                                           2015
                    ;          i                           2017
              Sulphur       oxides
                                         |mgim? |
                                     *
                   i                                       2016
                      80,
                                                           2015
                          ]
                                                           2017
          Tetrachloromethane|                     ws       T5578
                      {CCl
                                                           2015
                                                           2017
              Talu ene (Corre            mg/Mm?            2016
                                                           2015
               ;                                           2017
            Trichloromethane | [ro        ___
                                                            rer
                    ore
                                                           2017
               Vimy chloride
            monomer          (VCM)     |mg/Nm*|            2016
                    (Canc                                  2015
               wa                                          2017
             volatile organic                     Nm       [2076
                 compounds
                                               3
                                                            :
                                                           2014
                  FINIYAN   aad
                                                           [2017
                Total volatile                       —
          organic compounds| mg/Nm* |                      2016
                   {TVOC)                                  2015
                                                                  Sheet 3.1. Measurement (P2)
                                                                                              0000000108
</pre>

====================================================================== Einde pagina 26 =================================================================

<br><br>====================================================================== Pagina 27 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Gravitational          separation
           1    Identification
              |       Technique    associated with   point of emission:                      P2
           2    Removed substances
                                                                Substance
                                                                                 Removal          Removal
                                                                               purpose ¥       [efficiency (%)
                Removed substance 1 ¥                              Dust        Abatement
                                                                                  primary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments
                Information    on  the gravitational separation equipment
                Type   ¥                                                        Cyclone
                Start of  operation (year)                                         1980
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                                    Sampling  and measurements
                Operating time of the equipment (h/yr)                             8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                no
                VWdsSTE  Uds TEAUITETIIS]  MTT Ta5T Ul
                                                                                    Fo
                Deriving method for removal efficiency                        Design   value
              |                  Comments
                Waste gas     properties  after the   gravitational separation equipment
                    Do the waste gas properties vary
                  significantly under normal operating              No
                               conditions? ¥
                Measurement       point number                       1               2                3                5           6         7 10 fi 12
                Flow  (Nm2/h)                                    14787.0
                Humidity (%)                                       3.80
                Temperature (°C)                                   200
                Comments
           5    Operational    data for  gravitational separation      -
                                                                         consumables
                                                                                                               Sheet 3.2. Gravit. sep. (P2)(1)
                                                                                                                                                        0000000109
</pre>

====================================================================== Einde pagina 27 =================================================================

<br><br>====================================================================== Pagina 28 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                    12
                                 10/2018
                                         Sheet 3.2. Gravit. sep. (P2)(1)
                                                                         0000000110
</pre>

====================================================================== Einde pagina 28 =================================================================

<br><br>====================================================================== Pagina 29 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.3   Process furnace/heater
                                                                 Other  (Specify in comments)
                                                                       Magnesium oxide
                                           I   The furmace is    a shaftkiln for sintering the Magnesiumoxide
                                           |
                                    /heate                               direct-heating
                                                                               Air
                                                                                                        Max NOX
                                                           on
                                                                                                       emission is
                                             Other   (Specify in
                                                                                                     assHion: Tnx
                                               GOmMeits)                                              NOx kg/tonne
                                                                                                      MgO  per year
                                              Wet   scrubbing                                         no Sulphur  in
                                               with caustic                                            natural gas
                                                Optimised
                                               combustion
                                                 Wet dust
                                                 scrubbing
                                 —
                               —   BD      |
                                                         Natural  gas
                           [  NE                               7                   \ |
                                            york is an  packed   bed (MgO briquettes)    shaft kiln, with direct contact between burners and MgO briquettes.
                                                                                                                                        Sheet 3.3. Process f-h (P2)(1)
                                                                                                                                                                       0000000111
</pre>

====================================================================== Einde pagina 29 =================================================================

<br><br>====================================================================== Pagina 30 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.1   Channelled emissions to air monitored                               periodically     and associated waste gas treatment                         system                        Emission       point      ID (custom):        $3102                       Emission       point ID (automatic):
                                                                                                                                                                                                                                                                                                             | P3
                                                                                                                                                                                                                                                                                                                  |
          1                   Information         on  waste gas
                                                                                                                    Indicate which (groups of) substances           are monitored                 ¥                                Indicate which (groups of) substances     are  monitored
                                                                                                                 Cana       1,3-Butadiene                                                                                        HF        [Gaseous fluorides   (expressed   as  HF)
                                                                                                                 MH        Ammonia                                                                                              HCM        Hydrogen cyanide
                                                                                                                 Cena       Benzene                                                                                              Has       Hydrogen sulphide, (only for viscose production)
                                                                                                                            Carbon                        for viscose                                                            Pb        Lead and its
                                                                                                                 CS:                  disulphide, (only                 production)                                                                       compounds
                                                                                                                  CoO       Carbon monoxide                                                                                      Mi        Mickel and its   compounds
                                                                                                                CHac        Chloromethane                                                                                       MO         [Nitrogen  oxides  (expressed  as  NOx
                                            .                       ;
                                                                                                                CHzze        |Dichloromethane                                                                                   Maa        Mitrous oxide
                                      Monitored substances          in the waste gas                                          i
                                                                                                                                                                                                                                             :
                                                                                                                                                                                                                                                          g
                                                      calculated Please indicate if the                        PCDD/F       Dioxins and furans                                                                                 Caso        Propylene    oxide
                                 (measured        or
                                substance is                            if so, please fill in
                                                    monitored, and,                                                         Dust                                                                 Yes                            S04        Sulphur   oxides  (expressed  as  S03
                                       the associated lines       in  block    4 below.                                     Dust  -
                                                                                                                                    PMzs                                                                                        CCl,       Tetrachloromethane
                                                                                                                            Dust  -
                                                                                                                                    Pg                                                                                          Cra        Toluene
                                                                                                                  Ck        Elementary chlorine                                                                                CHCl;       Trichloromethane
                                                                                                                Cansciz     [Ethylene   dichloride   (EDC)                                                                     Cane        Win   chloride   monomer  (WVCM)
                                                                                                                 Caran      Ethylene    oxide                                                                                 MMWVOC         Mon-methane volatile  organic compounds
                                                                                                                 CHao       Formaldehyde                                                                                       TVOC        Total volatile organic compounds
                                                                                                                  HCI       (Gaseous chlorides      (expressed     as HC)
                                                          Comments
          2                   Information         on  waste gas treatment         system
                                                                                                                                                                                 Justification/frationale for using this technigue   or
                                                                                                   Waste gas treatment   technique ¥          Abatement /      Recovery   ¥                                                                                           Comments
                                                                                                                                                                                              COHIbTSton sLLrb igus
                                    1          Final abatement     or recovery technigue                      Filtration                      Abatement and recovery                       Removal and recovery of dust
                                              Other abatement or recovery technigue
                                    2
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    3
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    4
                                              applied before final abatementirecovery
                                              Other abatement or recovery technigue
                                    5
                                              applied before final abatementirecovery
                                 What    are    the main factors which influence the                                                                                       ;                                          y                 ai
                                                                                                                                                                    Compliance   ELV   { BREF LVIC-S0 and       permit of Dutch Autorties)
                                   dosaninalor LIL: Shale                   SED    SuF on)
                               If there is     no  waste gas treatment         system   or the
                                 generic techniques cannot be applied. please
                                                         explain why
          3                   Other information
                                                                                                CMR 1A/1B
                                                                                                                           lacute toxicity]      Origin of
                                       Properties      of the midture/preparation:             Ty             CMR ¥ 2      |byinhalation |      hazardous                     Comments
                                                                                                                                  Y          substances W
                                                                                                     =
                                           If the group Dust is monitored:                     Mo           Mo
                                  If the group       TVOC   or NMVOC is monitored:             [No          Mo
                                                                                                    When the concentration of                                   below the quantification limit, what
                                                                                                                                 individual congeners
                                                                                                                           concentration
                                                                                                                                                            is the sum? ¥
                                                                                                                                                                                                                     CRE
                                                                                                                                             is  reported  in
                            |           If the group Dioxins is monitored:
                            |       Additional information       on   batch processes
                                  Specify      the reference conditions        as set in the
                               permit if they differ from the following conditions:
                                dry gas, temperature of 273.16 K a pressure of
                                                          101.3 kPa.
                            |              If relevant, reference Oz        coe)
                                                                                                                                                                                                                                                      Sheet 3.1. Measurement      (P3)
                                                                                                                                                                                                                                                                                                                    0000000112
</pre>

====================================================================== Einde pagina 30 =================================================================

<br><br>====================================================================== Pagina 31 ======================================================================

<pre>30141731
      Drawing   up of the WGC BREF
                                                                                                                                                     remni
                                                                             ”
                                                                                                                     Representati
                                       2018 Seu:      0.300No  20.0000 Compliance Yes Yearly           halthouly     |veemission|   430  | 370   | 260
                                                                       monitoring                                        level
                                                                              ;
                                                                                                                     Representati
                                                               20.0000                                 halthourly                        |       |
                   C               .   wo             0.3000
                                                                       panhsncs   Yes Yearly                         ve
                                                                                                                        erision     490    210     650
                                            EN 13284-                  Compliance                                    Representati
                                       2006           0.300MNa 20.0000     ji     Yes Yearly           half-hourly  |ve emission | 20.20 | 19.20 | 19.00
                                            12001
                                             [7
                                                                       monitoring                                        Weed)
                                       2017
                Dust-PMzs
                              [
                              |   mg   2016
                                ]
                                       2075
          |
                                       2017
          |
                Dust-PMy,         |mgn 2016
                                       2015
                                       2017
            —              —
            Ele       faa
                      Re
                                       2016
                                       2015
                                       2017
                                       2016
                                       2075
          _                —
                                       2017
          Bae
                                       2016
                         :
          |
                                       2015
                                                                                       Sheet 3.1. Measurement   (F3)
                                                                                                                                                           0000000113
</pre>

====================================================================== Einde pagina 31 =================================================================

<br><br>====================================================================== Pagina 32 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                   ,
                                                           2017
              Formaldehyde    Hy
                                         mg/Nm?
                                               Tiel.
                                                         | 2016
                      (Cho                                 2015
                                 )                         2017
           Gaseous chlorides
                          3
                                       |mg/Nm?
                                            __
                                                       4
                                                         | 2016
                      (HCI)                                2015
                                                           2017
           a
           Gaseous fuoides | mom? |                        2076
                                                           2015
                ora                                        2017
           Hydrogen cyanide | nm                           2076
                    iil                   _
                                                           2015
           Hydrogen sulphide |              _
                                                           (—201C
                      {Rn                                  2015
                                                           2017
                 Lead and its                    Ch        =
                                         gi
            compounds (Pb)                                      ;
                 ST           LT                           2017
               Nickelandits                 |__|   NT
             compounds (Ni)            |                   a
             Nitrogen oxides |
                             2
                                               |
                                                  Nm?      =
                                                           2015
                                                           2017
           Mitrous oxide (Many           |mg/Mm?® |        2016
                                                           2015
             Propylene oxide
                      Cus
                                       |       }
                                                  Nm?      cu
                                                           2015
                    ;          i                           2017
              Sulphur       oxides
                                         |mgim? |
                                     *
                   i                                       2016
                      80,
                                                           2015
                          ]
                                                           2017
          Tetrachloromethane|                     ws       T5578
                      {CCl
                                                           2015
                                                           2017
              Talu ene (Corre            mg/Mm?            2016
                                                           2015
               ;                                           2017
            Trichloromethane | [ro        ___
                                                            rer
                    ore
                                                           2017
               Vimy chloride
            monomer          (VCM)     |mg/Nm*|            2016
                    (Canc                                  2015
               wa                                          2017
             volatile organic                     Nm       [2076
                 compounds
                                               3
                                                            :
                                                           2014
                  FINIYAN   aad
                                                           [2017
                Total volatile                       —
          organic compounds| mg/Nm* |                      2016
                   {TVOC)                                  2015
                                                                  Sheet 3.1. Measurement (P3)
                                                                                              0000000114
</pre>

====================================================================== Einde pagina 32 =================================================================

<br><br>====================================================================== Pagina 33 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Filtration
           1    Identification
              |       Technique    associated with      point of emission:                     P3
           2    Removed substances
                                                                   Substance
                                                                                   Removal           Removal
                                                                                 purpose ¥       [efficiency (%)
                Removed substance 1 ¥                                 Dust       Abatement
                                                                                  secondary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments
                Information    on  the filtration   equipment
                Type   V¥                                                  Fabric filter / Bag filter
                Start of  operation (year)                                           1980
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                              atch system, periodic measurements,      visual ( controle
                Operating time of the equipment (h/yr)                              8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                  no
                VWasSIlE Uds UEJUIIETILS]   ITT TASTE Ul
                                                                                      no
                Deriving method for removal efficiency                          Design   value
              |                  Comments
                Waste gas     properties   after the filtration    equipment
                    Do the waste gas properties vary
                  significantly under normal operating                 No
                               conditions? ¥
                Measurement       point number                          1                                                                                10 11 12
                Flow  (Nm3/h)                                       32130.0
                Humidity (%)                                          3.20
                Temperature (°C)                                      104
                Comments
           9    Operational    data for filtration    -
                                                         consumables
                                                                                                                           Sheet 3.2. Filtration (P3)(1)
                                                                                                                                                                  0000000115
</pre>

====================================================================== Einde pagina 33 =================================================================

<br><br>====================================================================== Pagina 34 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                   24
                                 09/2017
                                         Sheet 3.2. Filtration (P3)(1)
                                                                       0000000116
</pre>

====================================================================== Einde pagina 34 =================================================================

<br><br>====================================================================== Pagina 35 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.1   Channelled emissions to air monitored                               periodically     and associated waste gas treatment                         system                        Emission       point    ID  (custom):           $3202                        Emission       point ID (automatic):
                                                                                                                                                                                                                                                                                                                | P4
                                                                                                                                                                                                                                                                                                                     |
          1                   Information         on  waste gas
                                                                                                                    Indicate which (groups of) substances           are monitored                 ¥                                Indicate which (groups of) substances        are  monitored
                                                                                                                 Cana       1,3-Butadiene                                                                                        HF           [Gaseous fluorides   (expressed   as  HF)
                                                                                                                 MH        Ammonia                                                                                              HCM           Hydrogen cyanide
                                                                                                                 Cena       Benzene                                                                                              Has          Hydrogen sulphide, (only for viscose production)
                                                                                                                            Carbon                        for viscose                                                            Pb           Lead and its
                                                                                                                 CS:                  disulphide, (only                 production)                                                                          compounds
                                                                                                                  CoO       Carbon monoxide                                                                                       Mi          Mickel and its   compounds
                                                                                                                CHac        Chloromethane                                                                                       MO            [Nitrogen  oxides  (expressed  as  NOx
                                            .                       ;
                                                                                                                CHzze        |Dichloromethane                                                                                    Maa          Mitrous oxide
                                      Monitored substances          in the waste gas                                          i
                                                                                                                                                                                                                                               :
                                                                                                                                                                                                                                                             g
                                                      calculated Please indicate if the                        PCDD/F       Dioxins and furans                                                                                  Caso          Propylene    oxide
                                 (measured        or
                                substance is                            if so, please fill in
                                                    monitored, and,                                                         Dust                                                                 Yes                            S04           Sulphur   oxides  (expressed  as  S03
                                       the associated lines       in  block    4 below.                                     Dust  -
                                                                                                                                    PMzs                                                                                        CCl,          Tetrachloromethane
                                                                                                                            Dust  -
                                                                                                                                    Pg                                                                                          Cra           Toluene
                                                                                                                  Ck        Elementary chlorine                                                                                CHCl;          Trichloromethane
                                                                                                                Cansciz     [Ethylene   dichloride   (EDC)                                                                      Cane          Win   chloride   monomer  (WVCM)
                                                                                                                 Caran      Ethylene    oxide                                                                                 MMWVOC           Mon-methane volatile   organic compounds
                                                                                                                 CHao       Formaldehyde                                                                                       TVOC           Total volatile organic compounds
                                                                                                                  HCI       (Gaseous chlorides      (expressed     as HC)
                                                          Comments
          2                   Information         on  waste gas treatment         system
                                                                                                                                                                                 Justification/frationale for using this technigue   or
                                                                                                   Waste gas treatment   technique ¥          Abatement /      Recovery   ¥                                                                                              Comments
                                                                                                                                                                                              COHIbTSton sLLrb igus
                                    1          Final abatement     or recovery technigue                      Filtration                      Abatement and recovery             Recovery and     removal of dust,  Compliance     ELV
                                              Other abatement or recovery technigue
                                    2
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    3
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    4
                                              applied before final abatementirecovery
                                              Other abatement or recovery technigue
                                    5
                                              applied before final abatementirecovery
                                 What    are    the main factors which influence the                                                                                        :
                                                                                                                                                                                                                      i                his
                                                                                                                                                                      Compliance   ELV  (BREF    LVIC-So and    permit Dutch   auth oritie 5)
                                   dosaninalor LIL: Shale                   SED    SuF on)
                               If there is     no  waste gas treatment         system   or the
                                 generic techniques cannot be applied. please
                                                         explain why
          3                   Other information
                                                                                                CMR 1A/1B
                                                                                                                           lacute toxicity]      Origin of
                                       Properties      of the midture/preparation:             Ty             CMR ¥ 2      |byinhalation |      hazardous                     Comments
                                                                                                                                  Y          substances W
                                                                                                     =
                                           If the group Dust is monitored:                     Mo           Mo
                                  If the group       TVOC   or NMVOC is monitored:             [No          Mo
                                                                                                    When the concentration of                                   below the quantification limit, what
                                                                                                                                 individual congeners
                                                                                                                           concentration
                                                                                                                                                            is the sum? ¥
                                                                                                                                                                                                                     CRE
                                                                                                                                             is  reported  in
                            |           If the group Dioxins is monitored:
                            |       Additional information       on   batch processes
                                  Specify      the reference conditions        as set in the
                               permit if they differ from the following conditions:
                                dry gas, temperature of 273.16 K a pressure of
                                                          101.3 kPa.
                            |              If relevant, reference Oz        coe)
                                                                                                                                                                                                                                                         Sheet 3.1. Measurement      (P4)
                                                                                                                                                                                                                                                                                                                       0000000117
</pre>

====================================================================== Einde pagina 35 =================================================================

<br><br>====================================================================== Pagina 36 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                                                                                                                                        remni
                                                                                   ”
                                                                                                                           Representati
                                             2018 Seu:      0.300No  20.0000 Compliance Yes Yearly           halthouly     |veemission|  360  | 5.90 | 250
                                                                             monitoring                                        level
                                                                                    ;
                                                                                                                           Representati
                                                                     20.0000                                 halthourly                       |      |
                        C                .   wo             0.3000
                                                                             panhsncs   Yes Yearly                         ve
                                                                                                                              erision    1180   100    550
                                             2006
                                                  EN 13284-
                                                            0.300MNa 20.0000 Compliance
                                                                                 ji     Yes Yearly           half-hourly   Representati
                                                                                                                            |veemission| 3.10   2.40   250
                                                  12001
                                                   [7
                                                                             monitoring                                        Weed)
                                             2017
                  Dust-        PM.s
                                    [
                                    |   mg   2016
                                      ]
                                             2075
          |
                                             2017
          |
                  Dust-PMy,             |mgn 2016
                                             2015
                                             2017
             —                 —
             Ele          faa
                          Re
                                             2016
                                             2015
                                             2017
                                             2076
                                             2075
          _                     —
                                             2017
          [|
                 =              TE
                                             2016
                             :
          |
                                             2015
                                                                                             Sheet 3.1. Measurement   (P4)
                                                                                                                                                              0000000118
</pre>

====================================================================== Einde pagina 36 =================================================================

<br><br>====================================================================== Pagina 37 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                   ,
                                                           2017
              Formaldehyde    Hy
                                         mg/Nm?
                                               Tiel.
                                                         | 2016
                      (Cho                                 2015
                                 )                         2017
           Gaseous chlorides
                          3
                                       |mg/Nm?
                                            __
                                                       4
                                                         | 2016
                      (HCI)                                2015
                                                           2017
           a
           Gaseous fuoides | mom? |                        2076
                                                           2015
                ora                                        2017
           Hydrogen cyanide | nm                           2076
                    iil                   _
                                                           2015
           Hydrogen sulphide |              _
                                                           (—201C
                      {Rn                                  2015
                                                           2017
                 Lead and its                    Ch        =
                                         gi
            compounds (Pb)                                      ;
                 ST           LT                           2017
               Nickelandits                 |__|   NT
             compounds (Ni)            |                   a
             Nitrogen oxides |
                             2
                                               |
                                                  Nm?      =
                                                           2015
                                                           2017
           Mitrous oxide (Many           |mg/Mm?® |        2016
                                                           2015
             Propylene oxide
                      Cus
                                       |       }
                                                  Nm?      cu
                                                           2015
                    ;          i                           2017
              Sulphur       oxides
                                         |mgim? |
                                     *
                   i                                       2016
                      80,
                                                           2015
                          ]
                                                           2017
          Tetrachloromethane|                     ws       T5578
                      {CCl
                                                           2015
                                                           2017
              Talu ene (Corre            mg/Mm?            2016
                                                           2015
               ;                                           2017
            Trichloromethane | [ro        ___
                                                            rer
                    ore
                                                           2017
               Vimy chloride
            monomer          (VCM)     |mg/Nm*|            2016
                    (Canc                                  2015
               wa                                          2017
             volatile organic                     Nm       [2076
                 compounds
                                               3
                                                            :
                                                           2014
                  FINIYAN   aad
                                                           [2017
                Total volatile                       —
          organic compounds| mg/Nm* |                      2016
                   {TVOC)                                  2015
                                                                  Sheet 3.1. Measurement (P4)
                                                                                              0000000119
</pre>

====================================================================== Einde pagina 37 =================================================================

<br><br>====================================================================== Pagina 38 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Filtration
           1    Identification
              |       Technique    associated with     point of emission:                      P4
           2    Removed substances
                                                                  Substance
                                                                                 Removal             Removal
                                                                                purpose ¥        [efficiency (%)
                Removed substance 1 ¥                                Dust       Abatement
                                                                                secondary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments
                Information    on  the filtration  equipment
                Type   V¥                                                 Fabric filter / Bag  filter
                Start of  operation (year)                                          1980
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                             atch system, periodic measurement,        visual c¢ ontrole
                Operating time of the equipment (h/yr)                             8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                 no
                VWdsSTE  Uds TEAUITETIIS]   MTT Ta5T Ul
                                                                                     Fo
                Deriving method for removal efficiency                         Design    value
              |                  Comments
                Waste gas     properties   after the filtration   equipment
                    Do the waste gas properties vary
                  significantly under normal operating                No
                               conditions? ¥
                Measurement       point number                         1               2                3                 ol       5            6          10 11 12
                Flow  (Nm3/h)                                      32331.0
                Humidity (%)                                         3.80
                Temperature (°C)                                      83
                Comments
           9    Operational    data for filtration   -
                                                        consumables
                                                                                                                             Sheet 3.2. Filtration (P4)(1)
                                                                                                                                                                    0000000120
</pre>

====================================================================== Einde pagina 38 =================================================================

<br><br>====================================================================== Pagina 39 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                   24
                                 09/2018
                                         Sheet 3.2. Filtration (P4)(1)
                                                                       0000000121
</pre>

====================================================================== Einde pagina 39 =================================================================

<br><br>====================================================================== Pagina 40 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.1   Channelled emissions to air monitored                               periodically     and associated waste gas treatment                         system                        Emission       point    ID  (custom):         $3117                          Emission         point ID (automatic):
                                                                                                                                                                                                                                                                                                                  | P5
                                                                                                                                                                                                                                                                                                                       |
          1                   Information         on  waste gas
                                                                                                                    Indicate which (groups of) substances           are monitored                 ¥                                Indicate which (groups of) substances         are  monitored
                                                                                                                 Cana       1,3-Butadiene                                                                                        HF         [Gaseous fluorides    (expressed     as  HF)
                                                                                                                 MH        Ammonia                                                                                              HCM         Hydrogen cyanide
                                                                                                                 Cena       Benzene                                                                                              Has        Hydrogen sulphide, (only for viscose production)
                                                                                                                            Carbon                        for viscose                                                             Pb        Lead and its
                                                                                                                 CS:                  disulphide, (only                 production)                                                                        compounds
                                                                                                                  CoO       Carbon monoxide                                                                                       Mi        Mickel and its   compounds
                                                                                                                CHac        Chloromethane                                                                                        MO         [Nitrogen  oxides  (expressed     as  NOx
                                            .                       ;
                                                                                                                CHzze        |Dichloromethane                                                                                    Maa        Mitrous oxide
                                      Monitored substances          in the waste gas                                          i
                                                                                                                                                                                                                                             :
                                                                                                                                                                                                                                                           g
                                                      calculated Please indicate if the                        PCDD/F       Dioxins and furans                                                                                  Caso        Propylene    oxide
                                 (measured        or
                                substance is                            if so, please fill in
                                                    monitored, and,                                                         Dust                                                                 Yes                             S04        Sulphur   oxides  (expressed     as  S03
                                       the associated lines       in  block    4 below.                                     Dust  -
                                                                                                                                    PMzs                                                                                        CCl,        Tetrachloromethane
                                                                                                                            Dust  -
                                                                                                                                    Pg                                                                                           Cra        Toluene
                                                                                                                  Ck        Elementary chlorine                                                                                CHCl;        Trichloromethane
                                                                                                                Cansciz     [Ethylene   dichloride   (EDC)                                                                      Cane        Win   chloride   monomer    (WVCM)
                                                                                                                 Caran      Ethylene    oxide                                                                                 MMWVOC         Mon-methane volatile    organic compounds
                                                                                                                 CHao       Formaldehyde                                                                                       TVOC         Total volatile organic compounds
                                                                                                                  HCI       (Gaseous chlorides      (expressed     as HC)
                                                          Comments
          2                   Information         on  waste gas treatment         system
                                                                                                                                                                                 Justification/frationale for using this technigue   or
                                                                                                   Waste gas treatment   technique ¥          Abatement /      Recovery   ¥                                                                                               Comments
                                                                                                                                                                                              COHIbTSton sLLrb igus
                                    1          Final abatement     or recovery technigue                      Filtration                               Abatement                                   Removal of dust                                            Dust filtering  system, bag filters
                                              Other abatement or recovery technigue
                                    2
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    3
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    4
                                              applied before final abatementirecovery
                                              Other abatement or recovery technigue
                                    5
                                              applied before final abatementirecovery
                                 What    are    the main factors which influence the                                                                                        :                                         3                 a;
                                                                                                                                                                      Compliance   ELV  (BREF-LVIC-50       and permit Dutch authorities)
                                   dosaninalor LIL: Shale                   SED    SuF on)
                               If there is     no  waste gas treatment         system   or the
                                 generic techniques cannot be applied. please
                                                         explain why
          3                   Other information
                                                                                                CMR 1A/1B
                                                                                                                           lacute toxicity]      Origin of
                                       Properties      of the midture/preparation:             Ty             CMR ¥ 2      |byinhalation |      hazardous                     Comments
                                                                                                                                  Y          substances W
                                                                                                     =
                                           If the group Dust is monitored:                     Mo           Mo
                                  If the group       TVOC   or NMVOC is monitored:             [No          Mo
                                                                                                    When the concentration of                                   below the quantification limit, what
                                                                                                                                 individual congeners
                                                                                                                           concentration
                                                                                                                                                            is the sum? ¥
                                                                                                                                                                                                                     CRE
                                                                                                                                             is  reported  in
                            |           If the group Dioxins is monitored:
                            |       Additional information       on   batch processes                                                                                 Compliance   ELV  (BREF    LVIC-S0 and    permit  Dutch  authorities)
                                  Specify      the reference conditions        as set in the
                               permit if they differ from the following conditions:
                                dry gas, temperature of 273.16 K a pressure of
                                                          101.3 kPa.
                            |              If relevant, reference Oz        coe)
                                                                                                                                                                                                                                                       Sheet 3.1. Measurement         (P23)
                                                                                                                                                                                                                                                                                                                         0000000122
</pre>

====================================================================== Einde pagina 40 =================================================================

<br><br>====================================================================== Pagina 41 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                                                                                                                                     remni
                                                                                                                                 i                           Three
                                         ,                        Cr                                                  Representati                             iz
                                 wa
                                      Film 0.300No 20.0000 ls eg      Designvalue]  Yes Yearly           halfhourly   ve
                                                                                                                          mason      090  | 090  | 0.90
                                                                                                                                                           Singles
                                                                                                                                                               ents
                                                                                                                                   .
                                                                                                                                                             Three
                                                                 :
                                                                                                                      Representati                            i
                                 Wir
                                      EL   0.3000  20.0000 Seg        Designvalug]  Yes Yearly           halthourly   ve
                                                                                                                         emision
                                                                                                                           i
                                                                                                                                     100  | 100  | 1.00
                                                                                                                                                           [Sides
                                                                                                                                                               ents
                                                                  .
                                                                                                                      Representati                           Thre
                                                                                                                                                            Singles
                                 mis
                                      Bla  0.300No 20.0000 Compliance
                                                           manitoring
                                                                      Design value| Yes Yearly           halthourly   |veemission|
                                                                                                                          lave |
                                                                                                                                     7.00 | 5.00 | 6.50
                                                                                                                                                           measurem
                                                                                                                                                               ents
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                                                                         Sheet 3.1. Measurement  (P5)
                                                                                                                                                                    0000000123
</pre>

====================================================================== Einde pagina 41 =================================================================

<br><br>====================================================================== Pagina 42 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                   ,
                                                           2017
              Formaldehyde    Hy
                                         mg/Nm?
                                               Tiel.
                                                         | 2016
                      (Cho                                 2015
                                 )                         2017
           Gaseous chlorides
                          3
                                       |mg/Nm?
                                            __
                                                       4
                                                         | 2016
                      (HCI)                                2015
                                                           2017
           a
           Gaseous fuoides | mom? |                        2076
                                                           2015
                ora                                        2017
           Hydrogen cyanide | nm                           2076
                    iil                   _
                                                           2015
           Hydrogen sulphide |              _
                                                           (—201C
                      {Rn                                  2015
                                                           2017
                 Lead and its                    Ch        =
                                         gi
            compounds (Pb)                                      ;
                 ST           LT                           2017
               Nickelandits                 |__|   NT
             compounds (Ni)            |                   a
             Nitrogen oxides |
                             2
                                               |
                                                  Nm?      =
                                                           2015
                                                           2017
           Mitrous oxide (Many           |mg/Mm?® |        2016
                                                           2015
             Propylene oxide
                      Cus
                                       |       }
                                                  Nm?      cu
                                                           2015
                    ;          i                           2017
              Sulphur       oxides
                                         |mgim? |
                                     *
                   i                                       2016
                      80,
                                                           2015
                          ]
                                                           2017
          Tetrachloromethane|                     ws       T5578
                      {CCl
                                                           2015
                                                           2017
              Talu ene (Corre            mg/Mm?            2016
                                                           2015
               ;                                           2017
            Trichloromethane | [ro        ___
                                                            rer
                    ore
                                                           2017
               Vimy chloride
            monomer          (VCM)     |mg/Nm*|            2016
                    (Canc                                  2015
               wa                                          2017
             volatile organic                     Nm       [2076
                 compounds
                                               3
                                                            :
                                                           2014
                  FINIYAN   aad
                                                           [2017
                Total volatile                       —
          organic compounds| mg/Nm* |                      2016
                   {TVOC)                                  2015
                                                                  Sheet 3.1. Measurement (P23)
                                                                                               0000000124
</pre>

====================================================================== Einde pagina 42 =================================================================

<br><br>====================================================================== Pagina 43 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Filtration
           1    Identification
              |       Technique    associated with     point of emission:                       P5
           2    Removed substances
                                                                  Substance
                                                                                   Removal            Removal
                                                                                  purpose ¥       [efficiency (%)
                Removed substance 1 ¥                                Dust         Abatement
                                                                                  secondary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments                      Re moval   by extraction for recovery and environment
                Information    on  the filtration  equipment
                Type   V¥                                                  Fabric filter / Bag  filter
                Start of  operation (year)                                           1980
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                             , perdiodic changing   the filters  periodic samp ling and  measuring
                Operating time of the equipment (h/yr)                              8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                  no
                VWdsSTE  Uds TEAUITETIIS]   MTT Ta5T Ul
                                                                                      Fo
                Deriving method for removal efficiency                          Design    value
              |                  Comments
                Waste gas     properties   after the filtration   equipment
                    Do the waste gas properties vary
                  significantly under normal operating                No
                               conditions? ¥
                Measurement       point number                         1                2                3              ol          5            6          10 11 12
                Flow  (Nm3/h)                                       7226.0
                Humidity (%)                                         3.90
                Temperature (°C)                                      40
                Comments
           9    Operational    data for filtration   -
                                                        consumables
                                                                                                                              Sheet 3.2. Filtration (P5)(1)
                                                                                                                                                                     0000000125
</pre>

====================================================================== Einde pagina 43 =================================================================

<br><br>====================================================================== Pagina 44 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                    42
                                 04/2018
                                         Sheet 3.2. Filtration (P5)(1)
                                                                       0000000126
</pre>

====================================================================== Einde pagina 44 =================================================================

<br><br>====================================================================== Pagina 45 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.1   Channelled emissions to air monitored                              periodically      and associated waste gas treatment                         system                        Emission       point     ID (custom):         $3217                       Emission       point   ID (automatic):
                                                                                                                                                                                                                                                                                                               | P6
                                                                                                                                                                                                                                                                                                                    |
          1                   Information         on  waste gas
                                                                                                                    Indicate which (groups of) substances           are monitored                 ¥                                Indicate which (groups of) substances     are  monitored
                                                                                                                 Cana       1,3-Butadiene                                                                                        HF        [Gaseous fluorides   (expressed   as  HF)
                                                                                                                 MH        Ammonia                                                                                              HCM        Hydrogen cyanide
                                                                                                                 Cena       Benzene                                                                                              Has       Hydrogen sulphide, (only for viscose production)
                                                                                                                            Carbon                        for viscose                                                            Pb        Lead and its
                                                                                                                 CS:                  disulphide, (only                 production)                                                                       compounds
                                                                                                                  CoO       Carbon monoxide                                                                                      Mi        Mickel and its   compounds
                                                                                                                CHac        Chloromethane                                                                                       MO         [Nitrogen  oxides  (expressed  as  NOx
                                            .                       ;
                                                                                                                CHzze        |Dichloromethane                                                                                   Maa        Mitrous oxide
                                      Monitored substances          in the waste gas                                          i
                                                                                                                                                                                                                                             :
                                                                                                                                                                                                                                                          g
                                                      calculated Please indicate if the                        PCDD/F       Dioxins and furans                                                                                 Caso        Propylene    oxide
                                 (measured        or
                                substance is                            if so, please fill in
                                                    monitored, and,                                                         Dust                                                                 Yes                            S04        Sulphur   oxides  (expressed  as  S03
                                       the associated lines       in  block    4 below.                                     Dust  -
                                                                                                                                    PMzs                                                                                        CCl,       Tetrachloromethane
                                                                                                                            Dust  -
                                                                                                                                    Pg                                                                                          Cra        Toluene
                                                                                                                  Ck        Elementary chlorine                                                                                CHCl;       Trichloromethane
                                                                                                                Cansciz     [Ethylene   dichloride   (EDC)                                                                     Cane        Win   chloride   monomer  (WVCM)
                                                                                                                 Caran      Ethylene    oxide                                                                                 MMWVOC         Mon-methane volatile  organic compounds
                                                                                                                 CHao       Formaldehyde                                                                                       TVOC        Total volatile organic compounds
                                                                                                                  HCI       (Gaseous chlorides      (expressed     as HC)
                                                          Comments
          2                   Information         on  waste gas treatment         system
                                                                                                                                                                                 Justification/frationale for using this technigue   or
                                                                                                   Waste gas treatment   technique ¥          Abatement /      Recovery   ¥                                                                                           Comments
                                                                                                                                                                                              COHIbTSton sLLrb igus
                                    1          Final abatement     or recovery technigue                      Filtration                               Abatement                                   Removal of dust                                          Dust removal   system, bag filters
                                              Other abatement or recovery technigue
                                    2
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    3
                                              applied before final abatementfrecovery
                                              Other abatement or recovery technigue
                                    4
                                              applied before final abatementirecovery
                                              Other abatement or recovery technigue
                                    5
                                              applied before final abatementirecovery
                                 What    are    the main factors which influence the                                                                                       ;                                         ;
                                                                                                                                                                                                                                        ii
                                                                                                                                                                    Compliance   ELV   (BREF    LVIC-S0 and    permit of Dutch authorities)
                                   deoanlopetaior ol he Shae                ent    sysen
                               If there is     no  waste gas treatment         system   or the
                                 generic techniques cannot be applied. please
                                                         explain why
          3                   Other information
                                                                                                CMR 1A/1B
                                                                                                                           lacute toxicity]      Origin of
                                       Properties      of the midture/preparation:             Ty             CMR ¥ 2      |byinhalation |      hazardous                     Comments
                                                                                                                                  Y          substances W
                                                                                                     =
                                           If the group Dust is monitored:                     Mo           Mo
                                  If the group       TVOC   or NMVOC is monitored:             [No          Mo
                                                                                                    When the concentration of                                   below the quantification limit, what
                                                                                                                                 individual congeners
                                                                                                                           concentration
                                                                                                                                                            is the sum? ¥
                                                                                                                                                                                                                       CRE
                                                                                                                                             is  reported  in
                            |           If the group Dioxins is monitored:
                            |       Additional information       on   batch processes
                                  Specify      the reference conditions        as set in the
                               permit if they differ from the following conditions:
                                dry gas, temperature of 273.16 K a pressure of
                                                          101.3 kPa.
                            |              If relevant, reference Oz        coe)
                                                                                                                                                                                                                                                      Sheet 3.1. Measurement      (PG)
                                                                                                                                                                                                                                                                                                                      0000000127
</pre>

====================================================================== Einde pagina 45 =================================================================

<br><br>====================================================================== Pagina 46 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                                                                                                                                     remni
                                                                                                                                  i                          Three
                                         ,                        Tari                                                 Representati                            Si
                                 wa
                                      Film 0.300No 20.0000 ls eg       Designvalue]  Yes Yearly           halfhourly   ve
                                                                                                                           mason      510 | 550  | 570
                                                                                                                                                           Singels
                                                                                                                                                               ents
                                                                                                                                    .
                                                                                                                                                             Three
                                                                 :
                                                                                                                       Representati                           i
                                 Wir
                                      EL   0.3000  20.0000 Seg         Designvalug]  Yes Yearly           halthourly   ve
                                                                                                                          emision
                                                                                                                            i
                                                                                                                                      100 | 100  | 1.00
                                                                                                                                                           JSngs
                                                                                                                                                               ents
                                                                  .
                                                                                                                       Representati                          Three
                                                                                                                                                            Singels
                                 mis
                                      Bla  0.300No 20.0000 Compliance
                                                           manitoring
                                                                       Design value| Yes Yearly           halthourly   |veemission|
                                                                                                                           lave |
                                                                                                                                      100 | 1.00 | 1.00
                                                                                                                                                           measurem
                                                                                                                                                               ents
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                 2017
                                 2016
                                 2015
                                                                                          Sheet 3.1. Measurement  (PG)
                                                                                                                                                                    0000000128
</pre>

====================================================================== Einde pagina 46 =================================================================

<br><br>====================================================================== Pagina 47 ======================================================================

<pre>30141731
      Drawing     up of the WGC BREF
                                   ,
                                                           2017
              Formaldehyde    Hy
                                         mg/Nm?
                                               Tiel.
                                                         | 2016
                      (Cho                                 2015
                                 )                         2017
           Gaseous chlorides
                          3
                                       |mg/Nm?
                                            __
                                                       4
                                                         | 2016
                      (HCI)                                2015
                                                           2017
           a
           Gaseous fuoides | mom? |                        2076
                                                           2015
                ora                                        2017
           Hydrogen cyanide | nm                           2076
                    iil                   _
                                                           2015
           Hydrogen sulphide |              _
                                                           (—201C
                      {Rn                                  2015
                                                           2017
                 Lead and its                    Ch        =
                                         gi
            compounds (Pb)                                      ;
                 ST           LT                           2017
               Nickelandits                 |__|   NT
             compounds (Ni)            |                   a
             Nitrogen oxides |
                             2
                                               |
                                                  Nm?      =
                                                           2015
                                                           2017
           Mitrous oxide (Many           |mg/Mm?® |        2016
                                                           2015
             Propylene oxide
                      Cus
                                       |       }
                                                  Nm?      cu
                                                           2015
                    ;          i                           2017
              Sulphur       oxides
                                         |mgim? |
                                     *
                   i                                       2016
                      80,
                                                           2015
                          ]
                                                           2017
          Tetrachloromethane|                     ws       T5578
                      {CCl
                                                           2015
                                                           2017
              Talu ene (Corre            mg/Mm?            2016
                                                           2015
               ;                                           2017
            Trichloromethane | [ro        ___
                                                            rer
                    ore
                                                           2017
               Vimy chloride
            monomer          (VCM)     |mg/Nm*|            2016
                    (Canc                                  2015
               wa                                          2017
             volatile organic                     Nm       [2076
                 compounds
                                               3
                                                            :
                                                           2014
                  FINIYAN   aad
                                                           [2017
                Total volatile                       —
          organic compounds| mg/Nm* |                      2016
                   {TVOC)                                  2015
                                                                  Sheet 3.1. Measurement (PG)
                                                                                              0000000129
</pre>

====================================================================== Einde pagina 47 =================================================================

<br><br>====================================================================== Pagina 48 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Filtration
           1    Identification
              |       Technique    associated with      point of emission:                      P6
           2    Removed substances
                                                                   Substance
                                                                                    Removal           Removal
                                                                                   purpose ¥      [efficiency (%)
                Removed substance 1 ¥                                 Dust         Abatement
                                                                                   secondary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments                       Re moval   by extraction for recovery and environment
                Information    on  the filtration   equipment
                Type   V¥                                                   Fabric filter / Bag filter
                Start of  operation (year)                                            1980
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                              stem, periodoc changing the filters, periodic 1 measurements
                Operating time of the equipment (h/yr)                               8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                   no
                VWasSIlE Uds UEJUIIETILS]   ITT TASTE Ul
                                                                                       no
                Deriving method for removal efficiency                           Design   value
              |                  Comments
                Waste gas     properties   after the filtration    equipment
                    Do the waste gas properties vary
                  significantly under normal operating                 No
                               conditions? ¥
                Measurement       point number                          1                                                                               10 11 12
                Flow  (Nm3/h)                                       10643.0
                Humidity (%)                                          1.80
                Temperature (°C)                                       40
                Comments
           9    Operational    data for filtration    -
                                                         consumables
                                                                                                                          Sheet 3.2. Filtration (P6)(1)
                                                                                                                                                                 0000000130
</pre>

====================================================================== Einde pagina 48 =================================================================

<br><br>====================================================================== Pagina 49 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                    42
                                 01/2018
                                         Sheet 3.2. Filtration (P6)(1)
                                                                       0000000131
</pre>

====================================================================== Einde pagina 49 =================================================================

<br><br>====================================================================== Pagina 50 ======================================================================

<pre>30141731
            up of the
      Drawing         WGC BREF
        3.1  Channelled emissions to air monitored periodically or continuously and associated waste gas treatment      sy  Emission point        ID (custom):   53101         Emission point ID (automatic): lcP1
                                                                                                                                                                                                   |
                                                                                                                                                                                                           |
                                                                                                                            on     12
                                                                                                                                      LK    teh
                                                                                                                  Dust (MgO) is removed  by EGF far recaveryand
                                                                                          AbakEment recovery
                                                                                                   and                        environmental  ressons
                                                                                               Compliance ELV (BREF LVIC-3D and permit Duich authorities) and recovery
                                                                                                                                                                   of MgD dust
                                                                                                                                                                                                                   Sheet 3.1.
                                                                                                                                                                                                                              Measurement (GFT)
                                                                                                                                                                                                                                                0000000132
</pre>

====================================================================== Einde pagina 50 =================================================================

<br><br>====================================================================== Pagina 51 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 aig EN
                                     Fs
                                        ozse.2017 0.400No  2000.0000  Lionglisnis
                                                                      she    my
                                                                                  “es earthy ha hour Fareeenon|
                                                                                                          ori:
                                                                                                                   21100     [204.00 208.00
                                     5            0.400Ne  2000.0000f fo ig       Yes Yearly haithouty
                                                                                                       |vesmisson|
                                                                                                                   1051.00   [871.00 750.00
                                     EY           0.400 Mo 000.0000)  Sie dig     “ez Yearly halEhoury                     |        | 480
                                                                                                       veamisson    450       500
                                     EY wrians    p.200Ne             Iie ig      Yes Yearly halthouty
                                                                                                       |vesmisson|
                                                                                                                   10100     105.00  102.00
                                     5.  A        p.200Ne             Son ing     Yes Yearly haithouty
                                                                                                       |vesmisson|
                                                                                                                   10800     102.00  102.00
                                     _            0.200Me              ee Ging    Yes Yearly ralhouty
                                                                                                       |ieemisson|
                                                                                                                   11400     |11400  122.00
                                                                                                                                            Shest3d.1. Measurement (CPT)
                                                                                                                                                                         0000000133
</pre>

====================================================================== Einde pagina 51 =================================================================

<br><br>====================================================================== Pagina 52 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Shest3d.1. Measurement (CPT)
                                                              0000000134
</pre>

====================================================================== Einde pagina 52 =================================================================

<br><br>====================================================================== Pagina 53 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Shest3d.1. Measurement (CPT)
                                                              0000000135
</pre>

====================================================================== Einde pagina 53 =================================================================

<br><br>====================================================================== Pagina 54 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Electrostatic          precipitation (ESP)
           1    Identification
              |       Technique    associated with   point of emission:                            CP1
           2    Removed substances
                                                                Substance
                                                                                   Removal               Removal
                                                                                  purpose ¥           [efficiency (%)
                Removed substance 1 ¥                               Dust          Abatement
                                                                                     primary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                                             DUSL TEMOVAI    Dy   ESF     ITIAITNY  1017 TECOVETY  O1  MIU UUSL,
                                 Comments                    It mle     senriramee ms mte lo ees    me
                                                                                                 meses
                Information    on  the electrostatic   precipitation (esp) equipment
                Type   ¥                                                      Dry     wire    plate
                Start of  operation (year)                                             1980
                Last retrofit (year)                                                  2002
                Aim of the retrofit                                            replacement
                Control parameters                             Dust FilterWatch       system, measurements
                Operating time of the equipment (h/yr)                                8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                   none
                VWdsSTE  Uds TEAUITETIIS]  MTT Ta5T Ul
                                                                                       none
                Deriving method for removal efficiency                         Design       value
              |                  Comments
                Waste gas     properties  after the electrostatic     precipitation (esp) equipment
                    Do the waste gas properties vary
                  significantly under normal operating               No
                               conditions? ¥
                Measurement       point number                        1                  2                   3                            5           6         7  10 11 12
                Flow  (Nm3/h)                                     31808.0
                Humidity (%)                                       43.00
                Temperature (°C)                                    160
                Comments                                     ‘nts  on whether the      pre-dryer is active (160       °C) or not (400°C).
           9    Operational    data for electrostatic    precipitation (esp)    -
                                                                                   consumables
                                                                                                                                 Sheet 3.2. Elec. precip. (CP1)(1)
                                                                                                                                                                            0000000136
</pre>

====================================================================== Einde pagina 54 =================================================================

<br><br>====================================================================== Pagina 55 ======================================================================

<pre>30141731
      Drawing up  of the WGC BREF
              SOs consumption (if injected to reduce
                                                                                0                kg/1  000    Nm?
              particle resistivity)
              NH: consumption (if injected to reduce
                                                                                0                kg/1  000  Nm?
              particle resistivity)
              Water   consumption (wet ESP)                                     0                m1 000 Nm?
              Energy consumption                                                3)               kWh/1 000       Nm?
              Other   operational    information on  electrostatic  precipitation (esp)
              Turnaround interval                                              12                months
              Last turnaround                                               04/2018              month/year (MM/YYYY)
              Number of    stages                                               3
                                                                            Stage   1                     Stage   2  (if relevant)               Stage 3 (if relevant)
                                                           Average or       Minimum     Maximum | Average    or     |Minimum |Maximum
                                                                                                                                            po        Minimum [Maximum
                                                          typical value       value      value    typical value   |   value       value
                                                                                                                                             kim       value        value
              Residence time in the electrical field  (s)
              Upstream cooling      '¥                                         No
              Water injection    ¥                                             No
                               Comments
                                                                                                           Sheet 3.2. Elec.      precip. (CP1)(1)
                                                                                                                                                                          0000000137
</pre>

====================================================================== Einde pagina 55 =================================================================

<br><br>====================================================================== Pagina 56 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.3   Process furnace/heater
                                                              Other (Specify in comments)
                                                                   Magnesium oxide
                                                                                              RR
                                                                                              temperature in
                                                                                             the furnace isn't
                                                                                                          SO
                                            Other (Specify
                                              comments)
                                                           in
                                                                                               very High,oo
                                                                                             concentration is
                                                                                               not high also.
                                                                                                Optimaised
                                       —
                                                                                                combustion
                                          |                                                     Not present
                                               Optimised
                                         |
                                              combustion
                                            Other (Specify in                                   Removal of
                                              comments)
                            y
                                        |             Natural  gas            |
                                         Is heated by   natural gas with low /zero contants of Nitrogen and   np sulphur
                                                                                  Sheet 3.3. Process f-h  (CP1)(1)
                                                                                                                         0000000138
</pre>

====================================================================== Einde pagina 56 =================================================================

<br><br>====================================================================== Pagina 57 ======================================================================

<pre>30141731
            up of the
      Drawing         WGC BREF
        3.1  Channelled emissions to air monitored periodically or continuously and associated waste gas treatment      sy  Emission point        ID (custom):   53202          Emission point ID (automatic): lcP2]|
                                                                                                                                                                                                    |
                                                                                                                                                                                                            |
                                                                                                                            on     12
                                                                                                                                      LK    teh
                                                                                                                  Dust (MgO) is removed  by EGF far recaveryand
                                                                                          AbakEment recovery
                                                                                                   and                        environmental  ressons
                                                                                               Compliance ELY (BREF-LVIG-50 and   permit Dutch authorities)
                                                                                                                                                         and recovery
                                                                                                                                                                    of MgO dust
                                                                                                                                                                                                                      Shest3.1. Measurement (CF)
                                                                                                                                                                                                                                                 0000000139
</pre>

====================================================================== Einde pagina 57 =================================================================

<br><br>====================================================================== Pagina 58 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 2018 EX     0.400  2000.0000  paises  “es earthy ha hour
                                         ces
                                                                                             vesmisson 10400   [108.00  [114.00
                                      5      0.400  2000.0000) fo ig   Yes Yearly halthoury  meson     g9.00
                                                                                                             | 3900 | 34.00
                                      EY     0.400) 000.0000)  Sie dig “ez Yearly halEhoury                  |         | 200
                                                                                             veamisson  sx      530
                                      ES ST  0.200             Iie ig  Yes Yearly halEhourhy
                                                                                             9 208
                                                                                                    J  11000   [115.00  [112.00
                                      fo     0.200             Son ing Yes Yearhy halEhourhy
                                                                                             “es Sgn
                                                                                                       10450   [107.00  [108.50
                                      EY sin 0.200              Se deg Yes Yearly halthoury
                                                                                             emesen    2030     |=s30|sm
                                                                                                                                Shest3.1. Measurement (CF)
                                                                                                                                                           0000000140
</pre>

====================================================================== Einde pagina 58 =================================================================

<br><br>====================================================================== Pagina 59 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Shest3.1. Measurement (CF)
                                                            0000000141
</pre>

====================================================================== Einde pagina 59 =================================================================

<br><br>====================================================================== Pagina 60 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Shest3.1. Measurement (CF)
                                                            0000000142
</pre>

====================================================================== Einde pagina 60 =================================================================

<br><br>====================================================================== Pagina 61 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Electrostatic          precipitation (ESP)
           1    Identification
              |       Technique    associated with   point of emission:                         CPZ
           2    Removed substances
                                                                Substance
                                                                                    Removal              Removal
                                                                                   purpose ¥          [efficiency (%)
                Removed substance 1 ¥                               Dust           Abatement
                                                                                     primary
                Removed substance 2 ¥
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                                             DUSL TEMOVAI     Dy   ESF  ITIAITNY    107  TECOVETY  OT UUSL [IVIOU)
                                 Comments                    mpm] mle   Fe      Irs stm]
                                                                            meg
                                                                                             ees om ems ee
                Information    on  the electrostatic   precipitation (esp) equipment
                Type   ¥                                                       Dry   wire  plate
                Start of  operation (year)                                            1980
                Last retrofit (year)                                                  2002
                Aim of the retrofit                                             replacement
                Control parameters                              Dust filter watch    system, measurements
                Operating time of the equipment (h/yr)                                8000
                Minimum operating time (h/yr)
                Bypass    conditions                                                  none
                VWdsSTE  Uds TEAUITETIIS]  MTT Ta5T Ul
                                                                                      none
                Deriving method for removal efficiency                          Design    value
              |                  Comments
                Waste gas     properties  after the electrostatic     precipitation (esp) equipment
                    Do the waste gas properties vary
                  significantly under normal operating               No
                               conditions? ¥
                Measurement       point number                        1                 2                    3                           5           6         7  10 11 12
                Flow  (Nm3/h)                                     331230
                Humidity (%)                                       38.00
                Temperature (°C)                                    160
                Comments                                     bets  on whether the     pre-dryer is active       (150°C) or not  (400°C)
           9    Operational    data for electrostatic    precipitation (esp)     -
                                                                                    consumables
                                                                                                                                Sheet 3.2. Elec. precip. (CP2)(1)
                                                                                                                                                                           0000000143
</pre>

====================================================================== Einde pagina 61 =================================================================

<br><br>====================================================================== Pagina 62 ======================================================================

<pre>30141731
      Drawing up  of the WGC BREF
              SOs consumption (if injected to reduce
                                                                                0                kg/1  000    Nm?
              particle resistivity)
              NH: consumption (if injected to reduce
                                                                                0                kg/1  000  Nm?
              particle resistivity)
              Water   consumption (wet ESP)                                     0                m1 000 Nm?
              Energy consumption                                                3)               kWh/1 000       Nm?
              Other   operational    information on  electrostatic  precipitation (esp)
              Turnaround interval                                              12                months
              Last turnaround                                               10/2018              month/year (MM/YYYY)
              Number of    stages                                               3
                                                                            Stage   1                     Stage   2  (if relevant)               Stage 3 (if relevant)
                                                           Average or       Minimum     Maximum | Average    or     |Minimum |Maximum
                                                                                                                                            po        Minimum [Maximum
                                                          typical value       value      value    typical value   |   value       value
                                                                                                                                             kim       value        value
              Residence time in the electrical field  (s)
              Upstream cooling      '¥                                         No
              Water injection    ¥                                             No
                               Comments
                                                                                                           Sheet 3.2. Elec.      precip. (CP2)(1)
                                                                                                                                                                          0000000144
</pre>

====================================================================== Einde pagina 62 =================================================================

<br><br>====================================================================== Pagina 63 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.3   Process furnace/heater
                                                                       Other (Specify in comments)
                                                                            Magnesium oxide
                                                                              direct-heating
                                                                                    Air
                                                                         z                          :
                                                                               7
                                                                                    5    EE
                                                                                                      |
                                                                                               -
                                                                                          Tm
                                                                           chhnique           gue
                                                                                    £
                                                                                                   a
                                                                                                      [Temperature of]
                                                                                                          d the furnace
                                                                                                        isn't high so the
                                                    Other  (Specify in                                         NOx
                                                       comments)                                         concentration
                                                                                                        isn't high either.
                                                                                                            Optimised
                                               |
                                                                                                           combustion
                                                  |                                                        not present
                                                        Optimised
                                                |
                                                 |     combustion
                                                           (Specify in                                     Removal of
                                                  Other
                                                  |
                                                       comments)                                          dust by ESP
                             —   |
                                               l               Natural gas
                                       ifreleva]             3.00%
                                                 E   is heated  by Natural gas with low/zero contants of    nitrogen and   ho Sulphur
                                                                                           Sheet 3.3. Process f-h     (CP2)(1)
                                                                                                                                      0000000145
</pre>

====================================================================== Einde pagina 63 =================================================================

<br><br>====================================================================== Pagina 64 ======================================================================

<pre>30141731
            up of the
      Drawing         WGC BREF
        3.1  Channelled emissions to air monitored periodically or continuously and associated waste gas treatment   sy  Emission point     ID (custom):        531 10 Emission point ID (automatic): cpa]
                                                                                                                                                                                         |
                                                                                                                                                                                        ]
                                                                                                                                                                                        [
                                                                                                                                                                                        Jamis
                                                                                                                                                                                        |
                                                                                                                                                                                                   |
                                                                                                                                                                                        |
                                                                                                                                                                                         |
                                                                                                                                                                                         |
                                                                                                                                                                                       dustand 502
                                                                                                                      PFeductonof dust, HO and 302,
                                                                                                       Compliance ELV
                                                                                                                      (BREF LVIC-50 and permit of Dutch authori bes)
                                                                                                                                                                                                           Sheet 3.1.
                                                                                                                                                                                                                      Measurement (CFI)
                                                                                                                                                                                                                                        0000000146
</pre>

====================================================================== Einde pagina 64 =================================================================

<br><br>====================================================================== Pagina 65 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 2018 Th         0.300    50.0000) vy                              Yaz Yearly halthourhy
                                                                                                                          ve emission    5440    [110.00   [110.10
                                                                                                                                     ti
                                 2017 3     Joe. 0.300    50.0000) [Einesil                        Yaz Yearly halthourty  |veemizsion|
                                                                                                                             level
                                                                                                                                         55.30    [5810  | 55.00
                                                                                                                                     ti
                                         Ey Pie  0.200No  £0.0000  Ho ig                           Ves Yearly halEhoury
                                 018
                                   TF
                                                                                                                          veamisson      um       |zvoo     |=
                                      3
                                      i)
                                      i]
                                      ]
                                      3
                                     =
                                     i]
                                     T
                                     ]
                                     i}
                                   MT
                                     i]
                                   iE
                                                                                       Mezsuredica
                                                                                                                      hy [Reprasantat]
                                         »
                                 ws
                                         Eas     0.400MNo 20.0000  one
                                                                             ~
                                                                               | 2000
                                                                                         culated   Yes Yearly a
                                                                                                                                         os    |  oso    | oso
                                                                                          value                              level
                                                                         0
                                                                                       Mezsurediza                                   ti
                                 #5
                                         Bons    0.4000   20.0000) i             2000    Ioulsted  Yes Yearly halthoudy   |vesmissen|    280
                                                                                                                                               |  450
                                                                                                                                                         |  430
                                                                   menitanin              value                              level
                                                                         i
                                                                                       Mezsurediza                                   iti
                                 ae
                                         Flison  0.40000  30.0000  fk ig         5000
                                                                                      | ulated     Yes Yearly halthoury   [veemisson|     130
                                                                                                                                               |  2.50
                                                                                                                                                         | 440
                                                                                          value                              level
                                 2017
                                 iE
                                 iE
                                 017
                                 TE
                                    E
                                 017
                                 THE
                                 THE
                                 2017
                                 THE
                                 TE
                                 2017
                                 TE
                                 TE
                                 2017
                                 TE
                                 TE
                                 2017
                                                                                                                                                                   Shest3.1. Measurement (CFI)
                                                                                                                                                                                               0000000147
</pre>

====================================================================== Einde pagina 65 =================================================================

<br><br>====================================================================== Pagina 66 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 MNEM-EM-14151
                                 HEM-EN 14181
                                 MNEMN-EM 14181
                                                Sheet 3.1.
                                                           Measurement (CPI)
                                                                             0000000148
</pre>

====================================================================== Einde pagina 66 =================================================================

<br><br>====================================================================== Pagina 67 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                        [Complisnoe    Emission limit
                                        nonitoring    | 82  Kg  NOoo'ton
                                        IC omplizn ce  [Emnizd sion limit
                                        monitoring    |3,82 kg NCeeton
                                                        emission limit
                                        [Camplisnoe
                                        monitoring    3,82  kg  NCreoton
                                 20000  [Foiepitas    MEM-EM-14181
                                 20000) i             NEN-EN-14181
                                 20000       i        MEM-EN-14181
                                                                          Sheet 3.1.
                                                                                     Measurement (CPI)
                                                                                                       0000000149
</pre>

====================================================================== Einde pagina 67 =================================================================

<br><br>====================================================================== Pagina 68 ======================================================================

<pre>30141731
      Drawing up      of   the WGC BREF
          3.2 Dust           scrubbing
           1    Identification
              |           Technique    associated with    point of emission:                 CP3
           2    Removed substances
                                                                      Substance
                                                                                    Removal         Removal
                                                                                   purpose ¥     [efficiency (%)
                Removed substance 1 ¥                                    Dust      Abatement          95.00
                                                                                     primary
                                                                    Suphuroxiaes
                Removed substance 2 ¥
                                                                        (SOX)
                                                                                   Aoslement
                                                                                     primary
                                                                                                      95.00
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                     Comments                     |
                Information        on  the dust    scrubbing eq uipment
                Type       ¥                                                    Venturi scrubber
                Start of      operation (year)                                        2006
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                                                Measurement
                Operating time of the equipment (h/yr)                                8000
                Minimum operating time (h/yr)
                Bypass conditions                                                      no
                VWdSIE       Uds UEdUTIETINS])  ITT Cade Ul
                                                                                       no
                |= IF
                       Py ff
                Deriving method for removal efficiency                          Estimated value
              |                      Comments                     placed (2006)  because further  reducing  of the dust and
                Waste gas         properties   after the dust    scrubbing equipment
                      Do the waste gas properties vary
                   significantly under normal operating                   No
                                   conditions? ¥
                Measurement           point number                         1            2               3                                                   10 11 12
                Flow       (Nm?/h)                                     10414.0
                Humidity (%)                                            30.00
                Temperature (°C)                                          75
                Comments
                                                                                                                         Sheet 3.2. Dust scrubbing (CP3)(1)
                                                                                                                                                                     0000000150
</pre>

====================================================================== Einde pagina 68 =================================================================

<br><br>====================================================================== Pagina 69 ======================================================================

<pre>30141731
      Drawing up  of the WGC BREF
           9  Operational   data for dust scrubbing  -
                                                       consumables
              Scrubbing   water consumption                                           m3/1 000Nm?
              Energy consumption                                                      kWh/1 000 Nm?
           6  Other   operational information on  dust  scrubbing
              Turnaround interval                                                     months
              Last turnaround                                                         month/year (MM/YYYY)
              Operating temperature (°C)
                                                         Average or   Minimum Maximum
                                                        typical value  value   value
              Volume of   scrubbing water used to
              treat the waste gases  (m?®
                             Comments
                                                                                             Sheet 3.2. Dust scrubbing (CP3)(1)
                                                                                                                                0000000151
</pre>

====================================================================== Einde pagina 69 =================================================================

<br><br>====================================================================== Pagina 70 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.3   Process furnace/heater
                                                       Other (Specify in comments)
                                                            Magnesium oxide
                                                              direct-heating
                                                                    Air
                                                                                        NOx is reduced
                                                                                         by optimizing
                                                                                         the proces of
                                                                                          the furnace
                                       Wet scrubbing
                                        with caustic
                                         Optimised
                                        combustion
                                         Wet dust
                                         scrubbing
                                 |
                                                                       |
                                                Natural gas
                                                Naturalgas contains  no  nitrogen en sulphur
                                                                                                       Sheet 3.3. Process f-h (CP3)(1)
                                                                                                                                       0000000152
</pre>

====================================================================== Einde pagina 70 =================================================================

<br><br>====================================================================== Pagina 71 ======================================================================

<pre>30141731
            up of the
      Drawing         WGC BREF
        3.1  Channelled emissions to air monitored periodically or continuously and associated waste gas treatment   sy   Emission point        ID (custom):        53210                     Emission     point ID (automatic): |cP4]|
                                                                                                                                                                                                                    In         |
                                                                                                                                                                    Byinjection ofwater and Mg(O HZ r=d uction ofdust, 502 and
                                                                                                                                                                                                     ->
                                                                                                                       PFeducton of: dust, HCl and 502                                    decressing the pH
                                                                                                        compliance ELV
                                                                                                                        (BREF LVIC-S0   and
                                                                                                                                             permit Dutch authorities)
                                                                                                                                                                                                                                        Sheet 3.1.
                                                                                                                                                                                                                                                   Measurement (CP4)
                                                                                                                                                                                                                                                                     0000000153
</pre>

====================================================================== Einde pagina 71 =================================================================

<br><br>====================================================================== Pagina 72 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 2018 Th         0.300    50.0000) vy                              Yaz Yearly halthourhy
                                                                                                                          ve emission    3240   [40103730
                                                                                                                                     ti
                                 2017 3     Joe. 0.300    50.0000) [Einesil                        Yaz Yearly halthourty  |veemizsion|
                                                                                                                             level
                                                                                                                                         S120   [5500 | 53s
                                                                                                                                     ti
                                         Ey Pie  0.200No  £0.0000  Ho ig                           Ves Yearly halEhoury                       | 1250 | 2470
                                 018
                                   TF
                                                                                                                          veamisson      200
                                      3
                                      i)
                                      i]
                                      ]
                                      3
                                     =
                                     i]
                                     T
                                     ]
                                     i}
                                   MT
                                     i]
                                   iE
                                                                                       Mezsuredica
                                                                                                                      hy [Reprasantat]
                                         »
                                 ws
                                         Eas     0.400MNo 20.0000  one
                                                                             ~
                                                                               | 2000
                                                                                         culated   Yes Yearly a
                                                                                                                                          182 | om |    om
                                                                                          value                              level
                                                                         0
                                                                                       Mezsurediza                                   ti
                                 #5
                                         Bons    0.4000   20.0000) i             2000    Ioulsted  Yes Yearly halthoudy   |vesmissen|    280
                                                                                                                                              | 830
                                                                                                                                                      | sa0
                                                                   menitanin              value                              level
                                                                         i
                                                                                       Mezsurediza                                   iti
                                 ae
                                         Flison  0.40000  30.0000  fk ig         5000
                                                                                      | ulated     Yes Yearly halthoury   [veemisson|    2.10   |3040
                                                                                                                                                      | 670
                                                                                          value                              level
                                 2017
                                 iE
                                 iE
                                 017
                                 TE
                                    E
                                 017
                                 THE
                                 THE
                                 2017
                                 THE
                                 TE
                                 2017
                                 TE
                                 TE
                                 2017
                                 TE
                                 TE
                                 2017
                                                                                                                                                            Shest3.1. Measurement (CP4)
                                                                                                                                                                                        0000000154
</pre>

====================================================================== Einde pagina 72 =================================================================

<br><br>====================================================================== Pagina 73 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 MNEM-EM-14151
                                 MNEM-EM-14151
                                 MNEM-EM-14151
                                               Shest3.1. Measurement (CP4)
                                                                           0000000155
</pre>

====================================================================== Einde pagina 73 =================================================================

<br><br>====================================================================== Pagina 74 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                       TET            ai
                                       (mening       3.82 bg Noxon
                                       IC omplizn ce  emission limit
                                       [ranting      3.82 bg Noxon
                                                      emission limit
                                       IC omplizn ce
                                       [reriating    3.82 bg Noxon
                                 20004 [Compliance   MEM-EN-14181
                                                             ]
                                            hts
                                 20000 ompliznce     MEN-EM-14151
                                 20004 a             MEN-EM-14181
                                                                     Sheet 3.1.
                                                                                Measurement (CP4)
                                                                                                  0000000156
</pre>

====================================================================== Einde pagina 74 =================================================================

<br><br>====================================================================== Pagina 75 ======================================================================

<pre>30141731
      Drawing up   of  the WGC BREF
          3.2 Dust      scrubbing
           1    Identification
              |       Technique    associated with    point of emission:                    CP4
           2    Removed substances
                                                                    Substance
                                                                                  Removal         Removal
                                                                                 purpose ¥     [efficiency (%)
                Removed substance 1 ¥                                   Dust     Abatement
                                                                                   primary
                                                                                                    95.00
                                                                  Suphuroxiaes
                Removed substance 2 ¥
                                                                      (SOX)
                                                                                 Aoslement
                                                                                   primary
                                                                                                    95.00
                Removed substance 3 ¥
                Removed substance 4 ¥
                Removed substance 5 ¥
                                 Comments                       |
                Information    on  the dust    scrubbing equipment
                Type   ¥                                                      Venturi scrubber
                Start of operation (year)                                           2006
                Last retrofit (year)
                Aim of the retrofit
                Control parameters                                              measurement
                Operating time of the equipment (h/yr)                              8000
                Minimum operating time (h/yr)
                Bypass conditions                                                    no
                             HedUTIelIls])  IMT CdsE Ul
                ISIE                                                                 no
                                                              *
                Deriving method for removal efficiency                        Estimated value
              |                  Comments                       placed (2006)  because  offurther   reduction of the dust
                Waste gas     properties   after the dust    scrubbing equipment
                    Do the waste gas properties vary
                  significantly under normal operating                   No
                               conditions? ¥
                Measurement       point number                            1           2               3                                                   10 11 12
                Flow (N  m3/h)                                        9725.0
                Humidity (%)                                           32.00
                Temperature (°C)                                         73
                Comments
                                                                                                                       Sheet 3.2. Dust scrubbing (CP4)(1)
                                                                                                                                                                   0000000157
</pre>

====================================================================== Einde pagina 75 =================================================================

<br><br>====================================================================== Pagina 76 ======================================================================

<pre>30141731
      Drawing up  of the WGC BREF
           9  Operational   data for dust scrubbing  -
                                                       consumables
              Scrubbing   water consumption                                           m3/1 000Nm?
              Energy consumption                                                      kWh/1 000 Nm?
           6  Other   operational information on  dust  scrubbing
              Turnaround interval                                                     months
              Last turnaround                                                         month/year (MM/YYYY)
              Operating temperature (°C)
                                                         Average or   Minimum Maximum
                                                        typical value  value   value
              Volume of   scrubbing water used to
              treat the waste gases  (m?®
                             Comments
                                                                                             Sheet 3.2. Dust scrubbing (CP4)(1)
                                                                                                                                0000000158
</pre>

====================================================================== Einde pagina 76 =================================================================

<br><br>====================================================================== Pagina 77 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
          3.3   Process furnace/heater
                                                        Other (Specify in comments)
                                                             Magnesium oxide
                                                               direct-heating
                                                                     Air
                                                                      3                 NOX
                                                                                              TS
                                                                                                 TeaUcas
                                                                                         by optimizing
                                                                                          the furnace
                                                                                            nroces
                                       Wet scrubbing
                                        with caustic
                                         Optimised
                                        combustion
                                         Wet dust
                                         scrubbing
                           |
                             2                   Natural gas
                                 input
                                                      7
                                                Natural gas contains no  nitrogen and sulphur
                                                                                                         Sheet 3.3. Process f-h (CP4)(1)
                                                                                                                                         0000000159
</pre>

====================================================================== Einde pagina 77 =================================================================

<br><br>====================================================================== Pagina 78 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
           4   Diffuse emissions to air
                                         Type of process '¥
                                   Process operating time '¥
                                 Production capacity t/vr) ¥
                                                             Sheet 4. Diffuse emissions
                                                                                        0000000160
</pre>

====================================================================== Einde pagina 78 =================================================================

<br><br>====================================================================== Pagina 79 ======================================================================

<pre>30141731
         Sheet 4. Diffuse emissions
                                    0000000161
</pre>

====================================================================== Einde pagina 79 =================================================================

<br><br>====================================================================== Pagina 80 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Sheet 4. Diffuse emissions
                                                            0000000162
</pre>

====================================================================== Einde pagina 80 =================================================================

<br><br>====================================================================== Pagina 81 ======================================================================

<pre>30141731
      Drawing up of the WGC BREF
                                 Year of reference ¥
                                                     Sheet 4. Diffuse emissions
                                                                                0000000163
</pre>

====================================================================== Einde pagina 81 =================================================================

<br><br>====================================================================== Pagina 82 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                              ENDNOTES
                                                                                        1. Introductory    notes
                                       Information           on the person completing or checking the questionnaire. This person may be
                                                                                                                                                              |Backte      |
          To be filled in   by the                                                                                                                             worksheet
                                       contacted if further information or clarification is needed. This will usually be an employee of
         person completing the
                                       the company that is the             operator of the installation   or a   consultant    working   for the operator
      questionnaire on behalf of
           the operator of the         of the installation.
                installation
                                       Total rated thermal           input: permitted    total rated thermal    input  of all process furnaces/heaters
     the chemical      industry with
                                       connected to the stack where emissions                  occur.
      a  total rated thermal     input
      equal    to or  greater than 1
                     MW,
                                                                                             2. Installation
                                       If several installations are operated by the same company, please
                                                                                                                                                              |Backte      |
        Name of the installation
                                                                                                                               provide a different   name      worksheet
                                       for every installation, in order to differentiate between the different                 questionnaires.
                                       Name of the company operating the plant. This is the legal entity which holds the
         Name of the company
                                       environmental permit for the plant and which is named on the permit.
      Hypedink to the permit (if If an electronic version of the permit is publicly available on the Internet, please provide the
            publicly available)        hyperlink to it.
        Start of operation (year) Start of operation of the plant according to the IED permit or other permit issued prior to the
                                       Substantial change as defined in the IED (i.e. changes in the nature or functioning, or an
     Substantial changes in the
          installation having a        extension, of an installation which may have significant negative effects on human health or
                                       the environment) or as defined by the competent authority.
           significant effect on
             emissions to air
          Please                       Please provide a flow diagram/layout showing the sources of the waste gases, the waste
                   provide a flow
     diagram showing        the  waste gas     flows, the waste gas treatment systems and emission points. It should be a block
         gas treatment systems         diagram, e.g. according to ISO 10628:1997 Flow diagrams for process plants General                    -
                                        palm =
                                                                                      3. Channelled emissions
                                       Periodic measurement               means    the determination of     a  measurement       (particular quantity
                                                                                                                                                              |Backte      |
                                                                                                                                                               worksheet
          Channelled emission          subject      to     measurement)     at  specified  time intervals  using    manual    or  automated methods.
      sources to air where only For periodic measurements, the result of                         a measurement may be         an  average    over the
       periodic measurement is sampling period, preferably as agreed by                         the  TWG, i.e. 30 minutes for       measurements of
                    used               emissions to air.
          Channelled emission
                                       Continuous measurement                means a     measurement with       an   automated     measuring system
      sources     to air where    only
                                       (AMS) permanently              installed  on  site for continuous   monitoring     of emissions,    according to    EN
      continuous measurement
                                       14181:2004.
                   is used
          Channelled emission
                                       Emission           source  where the determination of the       measure      is realised   through periodic
      sources     to air where both
                                       measurement for             some   parameters and through continuous            measurement for       others, as
       periodic    and continuous
                                       described above.
       measurements        are  used
        Process     operating time     The time           during which the production process is operating and waste gases are generated.
                                       Production           capacity for the given IED activity connected to the emission point. The aim of
      Production      capacity (t/yr) this field is to differentiate between small-, medium-, large- and very large-scale processes.
                                       The exact production capacity is not requested.
                                       Select the chemical            activity specified   in the environmental      permit using the drop-down       list
                                       (which      is taken from Annex | to Directive           2010/75/EU).     In the  case   of stand-alone waste gas
         Main chemical      activity   treatment                  that      not                  chemical                    indicate the chemical
                                                           plants      are       permitted   as            installations,
                                       acitvity     of the main contributor to the waste gas flow.
                                       If there     are     other chemical activities carried out in the       same    installation and   emitting through
        Other chemical                 the same emission point as the main chemical activity, please specify the most important
                            activity
                                       other chemical activity using the drop-down list (which is taken from Annex | to Directive
                                         Fo
                                              on  J ll
                                                 Wr    | el IY
                                       If there     are     non-chemical activities carried out in the        same installation and emitting through
          Other   (non-chemical)       the same emission             point as the other chemical activities, please specify the most important
                   activity            other non-chemical            activity using the drop-down list (which is taken from Annex | to Directive
                                         gl
                                             pe  pp
                                       If the waste gas treatment system treats emissions from the production of polyolefins, PVC,
                                       solution-polymerised rubbers or viscose, please indicate which one by using the drop-down
            Particular  polymer        list. This will generate a specific worksheet (numbered 3.3). The generic information about
                production             the measurement of emission recovery techniques, abatement techniques and monitoring of
                                       emissions should be reported using the generic worksheets (numbered 3.1 and 3.2).
                                                                                         Sheet 5. Endnotes
                                                                                                                                                                         0000000164
</pre>

====================================================================== Einde pagina 82 =================================================================

<br><br>====================================================================== Pagina 83 ======================================================================

<pre>30141731
     Drawing up ofthe WGC BREF
                               Sheet 5. Endnotes
                                                 0000000165
</pre>

====================================================================== Einde pagina 83 =================================================================

<br><br>====================================================================== Pagina 84 ======================================================================

<pre>30141731
     Drawing      up of the WGC BREF
                                                                                                                  3.1. Measurement        (P)                                               Back ¢
                                                 Selecting           a  substance                 as a  "Yes' in the    drop-down     menu    generates a corresponding line in           worksheet
      Indicate which                             block 4 for           filing          in measurement           data. If the substance is not monitored, select ‘No’ or leave
                            (groups of)
      substances        are   monitored [he cell empty. The                                   reasons    why   the substance is not monitored may be            explained     in
                                                 Comments’.
          Waste gas treatment                    [Selecting a technique                          in the  drop-down       menu    generates the corresponding worksheet
                   technique                     (Worksheet 3.2).
                                                 Please         report here if TVOC                     or dusts contain substances classified           as carcinogenic,
                 CMR 1A/1B                       mutagenic or toxic for reproduction (CMR)                                  of  category 1A, 1B under Part 3 of Annex IV to
                                                 Regulation (EC) No 1272/2008.
                                                 Please         report here if TVOC                     or dusts contain substances classified           as carcinogenic,
                     CMR 2
                                                 mutagenic             or   toxic for            reproduction (CMR)         of  category 2 under Part 3 of Annex IV to
                                                 Please report here if TVOC                             or dusts contain substances classified           as acutely J toxic b y
     Acute    toxicity by         inhalation!                 o.oo"
                                                 inhalation.
                     of hazardous                Please select from the                           drop-down      list. If you choose "other"     please specify    in the comments
           Origin
                                                 cell.
                 substances
            Final abatement            or        Please         specify the final waste gas treatment, before the gas stream                              is emitted into the    air,
                                                 using       the    drop-down menu (which is taken from the CWW BREF).
           recovery technique
                                                 Please specify the other waste gas treatments that are used, using the drop-down menu
              |
                                            :    (which is taken from the CWW BREF). Box 2 should be used for the technique before the
     ra                mien                      final technique. Box 3 should be used for the technique before the technique described in
                                                 box 2 etc.
                 before final
                                                 Recovery comprises for example the                                   removal of utilisable individual    compounds, such as
           abatement/recovery                    starting materials, products, solvents                               or catalysts,  or material conversion with       subsequent
                                                 suhstance            recovery
             oo               ]
                                                 Please describe                      why       these  techniques       are  used and   why they    are used in   a  particular  order.
                                                                                                                                                                                         Back    -
      Justification/rationale for |For example: Absorption using a caustic scrubber to remove acid gases followed by                                                                      worksheet
        using this technique or |ata|ytic oxidation to destroy VOCs. Acid gases must be removed first because they would
     combination of         techniques poison                  the                           in the              oxidiser.
                                                                       catalyst                      catalytic
                                }
                                                 In many cases the main factor will be compliance with emission limit values (ELVs) specified
      What                main      factors jn
                are the                               European or national legislation. Other factors might be, for example: the recovery of an
                                      the
           which influence                  the
                                                 expensive solvent for reuse in the process; or compliance with an ELV which is lower than
        design/operation of                      he value           specified                in legislation   in order to    protect  a sensitive local habitat; or     secondary
           abatement system?                     filtration       using a HEPA filter to ensure                        removal of active     pharmaceutical ingredients.
        If there is
       treatment
                       no  waste gas
                       system or the
                                                 £2the                                                                    minor mass Tow       mit specifiedin national
                                                                                                                                                     P
                                                 leqislati
                                                  egisiation.
     generic techniques cannot
      be applied, please explain
                      why
                                                 Please provide data for 3 years of reference                                  (select from   drop-down menu).        [f available,
              Reference year
                                                 these should be the data for the last 3 years                                 2017, 2016 and 2015.
                                                 The     published or documented procedure for using the monitoring approach and technique
                                                 (i.e. analytical principle, such as infrared absorption, chemiluminescence, isokinetic
                                                 sampling followed by gravimetry, sorbent tube followed by gas chromatography), so that
          Standard      monitoring               comparable results can be obtained when the monitoring is carried out at different times or
                    method                       by different organisations. Please select, from a drop-down list, the appropriate CEN, ISO or
                                                 other standard. For further information on monitoring methods see the JRC Reference
                                                 Report on Monitoring of emissions from IED installations (the ROM REF) (Published
                                                 version 07/2018) at eippcb.jrc.ec.europa.eu/reference.
      Measurement                                [otandard uncertainty as specified in the measurement                                     report. The standard uncertainty is
                           uncertainty
                         in the                  the result of            a   measurement                expressed       as a  standard deviation     (see  1SO  20988:2007).
        (expressed                    same
      unit   as the measurement)
                            :
                                                 Select 'No' if the value                         reported   in this   row  is obtained   directly from the calibrated
     Has the
                  uncertainty 2isatly measurement device.
      been taken into account?
                                                                                                  Otherwise, indicate if the reported values have been calculated by
                                                 |   hia     cting      or    adding            the  uncertainty.
                                                 The limit of detection is the lowest concentration at which the presence of the substance can
              oo                    ]
                                                 be confirmed. So if a substance is not detected it may be absent or it may be present at a
             Limit of detection                  concentration below the limit of detection. If the measured value is below the detection                                         limit,
                                                 then the detection limit of the                          monitoring      method should be      reported.
                                                 The limit of quantification is the lowest concentration at which the amount of                                      a  substance
         oo                   .         .
                                                 can     be determined with                        an  acceptable level of accuracy and precision. The limit of
         Limit    of quantification
                                                |, ,antification will always be equal to or higher than the limit of detection. If the measured
                                                 value is below the quantification limit, then the quantification limit of the monitoring method
                                                   Looms olin] Dm om pom om pom pode pm, pm]
                                                 Please                                                                                                                                   Back to
           oo         oo
                                          |
                                                                report the emission limit values (ELVs)                           as set in your  permit. Where relevant, please
      Emission       limit value (ELV) report
       in the permit(in mg/Nm3)
                                                              the ELVs              as       concentration and/or         as mass    flow (in the next  column).                         worksheet
                                                                                                                    Sheet 5. Endnotes
                                                                                                                                                                                                    0000000166
</pre>

====================================================================== Einde pagina 84 =================================================================

<br><br>====================================================================== Pagina 85 ======================================================================

<pre>30141731
     Drawing  up of the WGC BREF
                                  Please   explain    the reason    for monitoring   the substance: e.g. compliance monitoring,
        Purpose   of monitoring   operator self-monitoring, operational control, Other regulation (e.g. health and safety).
                                  Provide the overall removal         efficiency of all combined waste gas treatment units. If the
       Removal    efficiency (%)  waste gas treatment       system is only made up of       one step, then report the efficiency of this
           Deriving   method      Please select from      a drop-down list for specifying the method for deriving the removal
                                  Data   can   be  reported for three reference years (to be selected between 2008 and 2017 by
                                  the drop-down menu).
                                  Emission data should refer to dry gas, a temperature of 273.15 K, a pressure of 101.3
                                  kPa and if relevant the reference O, content. If the measured value is below the detection
                                  limit, the detection limit of the monitoring method should be reported and information given
                                  in the  corresponding ‘Additional information’ cell (last column).
       MeasurementEmission
                                  Data should be       reported for normal operating conditions (NOC) only. As an indication, for
       data should refer to dry
                                  the purpose of the drawing up of the WGC BREF, other than normal operating conditions
         gas, a temperature of
       273.15 K, a pressure of
                                  (ONTOC) can include:
                                  +
                                    start-up and shutdown operations of the production plant (excluding routine fluctuations,
      101.3 kPa and if relevant,
                                  e.g. product changeover for individual production lines);
      the reference O2 content    +
                                    waste water treatment plant start-up (especially for seasonal operations);
                   (%)            +
                                    failure/unavailability of abatement equipment;
                                  +
                                    failure/unavailability of monitoring equipment;
                                  *
                                    major accidental spillages of liquids;
                                    emergency operations or actions taken for critical safety issues;
                                  *
                                  +
                                    definitive cessation of production operations.
                                  Please   specify by using     the   drop-down menu: spot sample in special case, occasional (once      |  Back to
                                                                                                                                           worksheet
                                  per year 12 times per year),          frequently (once per month once per week). The specified
                                             -                                                        -
                                  time intervals may be regular         (e.g. once every month) or irregular. Measurements are
                                  usually made using portable equipment for typically less than 24 h. The data reported here
                                  should refer only to the normal operating conditions of the chemical activity (see ‘endnotes’
                                  for definition of the main chemical activity) during the reference year. Although values
     Frequency    of measurement obtained during other years may also be representative of the current plant operation,
                                  please provide only data obtained during the reference year. Since the purpose of this
                                  questionnaire is to collect information on plant performance and not on compliance with
                                  requirements imposed by the competent authority, please report the shortest term average
                                  type which is available at the plant level (e.g. if half hourly averages and daily averages are
                                  available, report only half hourly averages, regardless of what is actually reported to the
                                  competent authority).
           Averaging period       Period of time     over  which the    sample   is taken.
                                  In many cases the emissions from batch processes vary considerably at different times in
                                  the batch cycle. For each KEI, please explain how the emissions vary during the batch
      Additional information   on cycle, how     you ensure that the periodic sampling complies with the ELVs specified in the
           batch processes        permit and     how you can use the measurements to calculate total or average emissions. You
                                  may include the information here or attach additional information, such as graphs of
                                  emissions, as an annex to the questionnaire and report the file name here.
                                  According     to EN   15259,  measurement        planning shall consider plant-specific conditions. A
                                  check shall be made        as to  whether, in view of the   measurement    objective, the necessary
                                  measuring      conditions   are  satisfied.
                                  For batch processes in particular the timing of the emission measurements shall take these
       Measurement      planning  circumstances into account sufficiently. Especially in the case of very short-term emission
                                  events,   a  check shall be made        as to whether several similar emission events     can be
                                  combined in      one  sampling    in order to enable evaluation of the   operating  state.
                                                                               Sheet 5. Endnotes
                                                                                                                                                     0000000167
</pre>

====================================================================== Einde pagina 85 =================================================================

<br><br>====================================================================== Pagina 86 ======================================================================

<pre>30141731
     Drawing     up of the WGC BREF
                                                                                        3.1. Measurement          (C)
                                        Selecting     a  substance       as a  "Yes' in the   drop-down      menu    generates a corresponding line in
                                                                                                                                                                |Backte      |
                                                                                                                                                                 worksheet
      Indicate which                    block 4 for     filing in measurement         data. If the substance is not monitored, select ‘No’ or leave
                           (groups of)
      substances       are  monitored the cell     empty. The reasons why the              substance is not monitored may be          explained     in
                                        Comments’.
          Waste gas treatment           Selecting a technique           in the  drop-down      menu     generates the corresponding worksheet
                  technique             (Worksheet 3.2).
                                        Please     report here if TVOC         or dusts contain substances classified           as carcinogenic,
                CMR 1A/1B               mutagenic or toxic for reproduction (CMR)                  of  category 1A, 1B under Part 3 of Annex IV to
                                        Regulation (EC) No 1272/2008.
                                        Please     report here if TVOC         or dusts contain substances classified           as carcinogenic,
                    CMR 2
                                        mutagenic       or   toxic for  reproduction (CMR)         of category 2 under Part 3 of Annex [V to
                                        Please     report here if TVOC         or dusts contain substances classified           as acutely   toxic  by
     Acute    toxicity by    inhalation
                                        inhalation.
                     of hazardous       Please select from the           drop-down     list. If you choose "other"       please specify  in the comments
           Origin
                substances              cell.
            Final abatement      or     Please     specify the final waste gas treatment, before the gas stream                  is emitted into the    air,
                                        using    the drop-down menu (which is taken from the CWW BREF).
           recovery     technique
                                        Please specify the other waste gas treatments                    that are used, using the drop-down menu
           Other abatement       or     (which is taken from the CWW BREF). Box 2 should be used for the technique before the
                                        final technique. Box 3 should be used for the technique before the technique described in
     recovery technique applied
                                        box 2 etc. Recovery comprises for example the removal of utilisable individual compounds,
                before final
                                        such as starting materials, products, solvents or catalysts, or material conversion with
           abatement/recovery
                                        subsequent substance recovery.
                                        Please describe          why these techniques are used and why they are used in a particular order.
      Justification/rationale for       For   example: Absorption using a caustic scrubber to remove acid gases followed by
        using this technique or catalytic oxidation to destroy VOCs. Acid gases must be removed first because they would
     combination of techniques
                                        poison the catalyst in the catalytic oxidiser.
                                        In many cases the main factor will be compliance with emission limit values (ELVs) specified
      What     are  the main factors in
                                            European or national legislation. Other factors might be, for example: the recovery of an                             Back to
           which influence the
                                        expensive solvent for reuse in the process; or compliance with an ELV which is lower than                                worksheet
        design/operation of the the value specified in legislation in order to protect a sensitive local habitat; or secondary
           abatement system?            filtration            a HEPA filter to ensure removal of active
                                                    using                                                           pharmaceutical ingredients.
                                        For   example,       in some cases a      waste gas treatment         system is    not required because      the
        If there is    no waste gas
                                        mass     flow of the substance is below the minor                mass   flow limit specified in national
       treatment system orthe
                                        legislation.
     generic techniques cannot
      be applied, please explain
                      why
                                        Data    can be reported for three reference years (to be selected between 2008                       and 2017     by
        MeasurementEmission
                                        the   drop-down menu).
        data should refer to      dry   Emission data should refer to dry gas, a temperature of 273.15 K, a pressure                         of 101.3 kPa
         gas,   a  temperature of       and if relevant the reference O2 content. If the measured value is below the detection
        273.15                                                                                                                                         limit,
                   K, a pressure of
                                        the detection limit of the         monitoring    method should be         reported   and information    given  in the
       101.3   kPa and if relevant,
                                        corresponding          ‘Additional information’ cell      (last column).
       the reference O2 content
                      (%).
                                        Please provide data for 3 years of reference                  (select  from  drop-down menu).       If available,
              Reference year
                                        these should be the data for the last 3 years                 2017, 2016 and 2015.
                                        The    published or documented procedure for using the monitoring approach and technique
                                        (i.e. analytical principle, such as infrared absorption, chemiluminescence, isokinetic
                                        sampling followed by gravimetry, sorbent tube followed by gas chromatography), so that
          Standard      monitoring      comparable results can be obtained when the monitoring is carried out at different times or
                    method              by different organisations. Please select, from a drop-down list, the appropriate CEN, ISO or
                                        other standard. For further information on monitoring methods see the JRC Reference
                                        Report on Monitoring of emissions from IED installations (the ROM REF) (Published
                                        version 07/2018) at eippchb.irc.ec.europa.eu/reference.
      Measurement                       Standard uncertainty as specified in the measurement                      report. The standard uncertainty is
                          uncertainty
                                        the result of      a  measurement       expressed      as a   standard deviation     (see  1SO  20988:2007).
        (expressed in the same
      unit as the measurement)
                                        Select 'No' if the value         reported   in this  row   is obtained    directly from the calibrated
     Has the     uncertainty already measurement              device.    Otherwise, indicate if the reported values have been calculated by
      been taken into account?                                         the
                                        subtracting      or   adding        uncertainty.
                                        The limit of detection is the lowest concentration at which the presence of the substance can
                                        be confirmed. So if a substance is not detected it may be absent or it may be present at a
             Limit of detection         concentration below the limit of detection. If the measured value is below the detection                         limit,
                                        then the detection limit of the          monitoring     method should be        reported.
                                                                                          Sheet 5. Endnotes
                                                                                                                                                                           0000000168
</pre>

====================================================================== Einde pagina 86 =================================================================

<br><br>====================================================================== Pagina 87 ======================================================================

<pre>30141731
     Drawing up ofthe WGC BREF
                               Sheet 5. Endnotes
                                                 0000000169
</pre>

====================================================================== Einde pagina 87 =================================================================

<br><br>====================================================================== Pagina 88 ======================================================================

<pre>30141731
     Drawing up of the WGC BREF
                                Please   explain  the  reason  for monitoring    the substance: e.g.   compliance monitoring,
       Purpose  of monitoring   operator self-monitoring, operational control, Other regulation (e.g. health and safety).
                                                                                                                                       Back to
                                Provide the overall removal      efficiency of all combined waste gas treatment units. If the         worksheet
       Removal   efficiency (%) waste gas treatment      system is only made up of one step, then report the efficiency of this
          Deriving  method      Please select from     a drop-down    list for specifying the method for   deriving the removal
                                As  part of the validation procedure, the outliers (defined      as  results which deviate
                                significantly from the other values in a measurement series) should be excluded before
                                reporting the 95th percentiles and the 97th percentiles. Furthermore, since the data reported
          95th Percentiles      here should refer only to normal operating conditions, any data refering to other than normal
                                operating conditions, as well as periods when the plant was not operational, should be
                                excluded if possible. If the measured value is below the detection limit report the detection
                                 imit nf the measurement method in the Comments cell
                                As  part of the validation procedure, the outliers (defined as a results which deviate
                                significantly from the other values in a measurement series) should be excluded before
                                reporting the 95th percentiles and the 97th percentiles. Furthermore, since the data reported
          97th Percentiles      here should refer only to normal operating conditions, any data refering to other-than-normal
                                operating conditions, as well as periods when the plant was not operational, should be
                                excluded if possible. If the measured value is below             detection limit report the detection
                                 imit of the measurement methodin the Comments               the
                                                                                            ce
                                The average value of the valid      daily averages (hourly     ne half-houlry) recorded during    a
           Yearly average       period of one year. Hourly and      half-hourly averages are     valid when other than normal
                                operating   conditions and   plant  shut down data     are excluded from the dataset.
                                Specify   the cases   of other than normal     operating conditions (OTNOC) which are included
                                and how emissions to air      during OTNOC are regulated. In the case of continuous
                                measurements please provide more insight into some specific conditions. You may include
                                the information here or attach additional information, such as graphs of emissions or a copy
                                of the permit, as an annex to the questionnaire and report the file name here.
                                As an indication, for the purpose of the drawing up of the WGC BREF, OTNOC can include:
                                +
                                  start-up and shutdown operations of the production plant (excluding routine fluctuations,
                the         of  e.g. product changeover for individual production lines);
        Specify      cases
                                +
                                  waste water treatment plant start-up (especially for seasonal operations);
     OTNOC which are included
                                +
                                  failure/unavailability of abatement equipment;
                                +
                                  failure/unavailability of monitoring equipment;
                                *
                                  major accidental spillages of liquids;
                                  emergency operations or actions taken for critical safety issues;
                                *
                                +
                                  definitive cessation of production operations.
                                                                           Sheet 5. Endnotes
                                                                                                                                                0000000170
</pre>

====================================================================== Einde pagina 88 =================================================================

<br><br>====================================================================== Pagina 89 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                         3.1. Measurement          (CP)                                     Back ¢
                                             Selecting    a  substance      as a  "Yes' in the   drop-down     menu   generates a corresponding line in    worksheet
      Indicate which                         Plock 4 for    filing  in measurement       data. If the substance is not monitored, select ‘No’ or leave
                            (groups of)
      substances        are  monitored the cell empty. The             reasons     why  the substance is not monitored may be         explained    in
                                             Comments’.
          Waste gas treatment                [Selecting a technique        in the  drop-down      menu    generates the corresponding worksheet
                 technique                   (Worksheet 3.2).
                                             Please    report here if TVOC        or dusts contain substances classified       as  carcinogenic,
                CMR 1A/1B                    mutagenic or toxic for reproduction (CMR)               of  category 1A, 1B under Part 3 of Annex IV to
                                             Regulation (EC) No 1272/2008.
                                             Please    report here if TVOC        or dusts contain substances classified       as  carcinogenic,
                    CMR 2
                                             mutagenic      or toxic for   reproduction (CMR)        of category 2 under Part 3 of Annex [V to
                  Sagi           :         .
                                             [Please   report here if TVOC        or dusts contain substances classified       as  acutely  toxic by
     Acute    toxicity by        inhalation,
                                             +o
                    of hazardous             Please select from the         drop-down     list. If you choose "other"    please specify in the comments
           Origin
                                             cell.
                substances
            Final abatement           or     Please    specify the final waste gas treatment, before the gas stream              is emitted into the  air,
                                             using   the drop-down menu (which is taken from the CWW BREF).
           recovery      technique
                                             Please specify the other waste gas treatments                 that are used, using the drop-down menu
           Other abatement             or    (which is taken from the CWW BREF). Box 2 should be used for the technique before the
                                             final technique. Box 3 should be used for the technique before the technique described in
     recovery technique applied
                                             box 2 etc. Recovery comprises for example the removal of utilisable individual compounds,
                before final
                                             such as starting materials, products, solvents or catalysts, or material conversion with
           abatement/recovery                subsequent substance recovery.
             oo               ]
                                             Please describe       why these techniques are used and why they are used in a particular order.
      Justification/rationale for            |For  example: Absorption using a caustic scrubber to remove acid gases followed by
        using this technique or ata ytic oxidation to destroy VOCs. Acid gases must be removed first because they would
     combination of techniques
                                             poison the catalyst in the catalytic oxidiser.
                               }
                                             In many    cases the main factor will be compliance with emission limit values (ELVs) specified
      What are the main factors      the
                                             jn European or national legislation. Other factors might be, for example: the recovery of an
           which influence                   expensive solvent for reuse in the process; or compliance with an ELV which is lower than
        design/operation of the              he value specified in legislation in order to protect a sensitive local habitat; or secondary
           abatement system?                 filtration using a HEPA filter to ensure removal of active pharmaceutical ingredients.
                                             For   example,    in some cases a waste gas treatment system is not required because the
        If there is    no  waste gas
                                                     flow of the substance is below the minor mass flow limit specified in national
       treat nent      system        or  the
                                             mass
                                             legisiation.
     generic techniques cannot                                                                                                                              Back to
      be applied, please explain                                                                                                                           worksheet
                      why
                                             Data   can be reported for three reference years (to be selected between 2008 and 2017 by
                                             the   drop-down menu).Emission data should refer to dry gas, a temperature of 273.15 K, a
                                             pressure of 101.3 kPa and if relevant the reference O2 content. If the measured value is
                                             below the detection limit, the detection limit of the monitoring method should be reported
                                               nd information      given in the corresponding ‘Additional information’ cell (last column).Data
                                               hould be    reported for normal operating conditions (NOC) only. As an indication, for the
        MeasurementEmission
        data should refer to                   urpose of the drawing up of the WGC BREF, other than normal operating conditions
                                        dry
                                        of    ONTOC) can include:* start-up and shutdown operations of the production plant (excluding
         gas,   a temperature                 outine fluctuations, e.g. product changeover for individual production lines);* waste water
        273.15    K,   a pressure of          reatment plant start-up (especially for seasonal operations);* failure/unavailability of
       101.3 kPa and if           relevant,    batement equipment;« failure/unavailability of monitoring equipment;+ major accidental
       the reference O2 content
                                               pillages ofliquids;« emergency operations or actions taken for critical safety issues;
                       (%)-                    efinitive cessation of production operations.
                                    hese
                                             Data   can be reported for three reference years (to be selected between 2008 and 2017 by
        Se                            ar      he   drop-down menu).Emission data should refer to dry gas, a temperature of 273.15 K, a
                                               ressure   of 101.3 kPa and if relevant the reference O2 content. If the measured value is
         gas,   a temperature           of
                                               elow the detection       limit, the detection limit of the monitoring method should be reported
        273.15 K,      a pressure of
                                               nd information
       101.3 KPa     ald    if relevant,                           given in the corresponding ‘Additional information’ cell (last column).
       the reference O2 content
                       (%).
                                             Please provide data for 3 years of reference               (select  from drop-down menu).     [f available,
              Reference year
                                             these should be the data for the last 3 years              2017, 2016 and 2015.
                                                                                             Sheet 5. Endnotes
                                                                                                                                                                     0000000171
</pre>

====================================================================== Einde pagina 89 =================================================================

<br><br>====================================================================== Pagina 90 ======================================================================

<pre>30141731
     Drawing up ofthe WGC BREF
                               Sheet 5. Endnotes
                                                 0000000172
</pre>

====================================================================== Einde pagina 90 =================================================================

<br><br>====================================================================== Pagina 91 ======================================================================

<pre>30141731
     Drawing   up of the WGC BREF
                                       Please    explain    the  reason  for  monitoring    the substance: e.g.       compliance monitoring,
        Purpose     of  monitoring     Pperator self-monitoring, operational control, Other regulation (e.g. health and safety).
                       Fast      3
                                       Provide the overall removal          efficiency  of all combined waste gas treatment units. If the
       Removal      efficiency (%)
                                      |, ate gas treatment system is only made up of               one step, then report the efficiency of this
            Deriving     method        Please select from        a drop-down list for specifying the method for deriving the removal
                                       Data   can    be  reported for three reference years (to be selected between 2008 and 2017 by
                                       the   drop-down menu).Emission data should refer to dry gas, a temperature of 273.15 K, a
                                       pressure of 101.3 kPa and if relevant the reference O2 content. If the measured value is
                                       below the detection limit, the detection limit of the monitoring method should be reported
                                         nd information      given in the corresponding ‘Additional information’ cell (last column).Data
                             Ce          hould be     reported for normal operating conditions (NOC) only. As an indication, for the
       MeasuremeniEmission
           a  should     refer
                              to dry |
                                         urpose of the drawing up of the WGC BREF, other than normal operating conditions
                                                      can
                                         ny 160) ) can include» start-up
                                                                                                                  of
         gas,  a temperature     of        N               include:+ start-up and and shutdown
                                                                                       shutd            tions
                                                                                                  operations      of the     production plan
                                                                                                                     the production      plant (excluding
                                                                                                                                                   (exclu
       273.15 K,     a  pressure of
                                        outine fluctuations, e.g.
                                                                      product changeover for individual production lines); wasteofwater
      101   3 kPa and if relevant       reatment plant start-up (especially for seasonal operations); failure/unavailability
                                         batement equipment; failure/unavailability of monitoring equipment;* major accidental
      the  reference 02 content
                  |
                                         pillages ofliquids;* emergency operations or actions taken for critical safety issues;+
                      o)
                     (%).                efinitive cessation of production operations.
                                       Please    specify by using     the   drop-down menu: spot sample in special case, occasional (once
                                         er  year 12 times per year),         frequently (once per month once per week). The specified
                                                   -                                                             -
                                        ime intervals may be regular          (e.g. once every month) or irregular. Measurements are
                                         sually made using portable equipment for typically less than 24 h. The data reported here
                                       should refer only to the normal operating conditions of the chemical activity (see ‘endnotes’
                                          r definition of the main chemical activity) during the reference year. Although values
     Frequency      of  measurement btained during other years may also be representative of the current plant operation,
                                         lease provide only data obtained during the reference year. Since the purpose of this
                                         uestionnaire is to collect information on plant performance and not on compliance with
                                        equirements imposed by the competent authority, please report the shortest term average
                                        ype which is available at the plant level (e.g. if half hourly averages and daily averages are
                                         vailable, report only half hourly averages, regardless of what is actually reported to the
                                       competent authority).
                                       Period of                 which the             is taken.                                                           Back to
           Averaging period                          time  over               sample
                                                                                                                                                          worksheet
                                       In many cases the emissions from batch processes vary considerably at different times in
                                       the batch cycle. For each KEI, please explain how the emissions vary during the batch
      Additional information       on  cycle, how      you ensure that the periodic sampling complies with the ELVs specified in the
            batch processes            permit and      how you can use the measurements to calculate total or average emissions. You
                                       may include the information here or attach additional information, such as graphs of
                                       emissions, as an annex to the questionnaire and report the file name here.
                                       As   part of the validation procedure, the outliers (defined as results which deviate
                                       significantly from the other values in a measurement series) should be excluded before
                                       reporting the 95th percentiles and the 97th percentiles. Furthermore, since the data reported
            95th Percentiles           here should refer only to normal operating conditions, any data refering to other than normal
                                       operating conditions, as well as periods when the plant was not operational, should be
                                       excluded if possible. If the measured value is below the detection limit report the detection
                                        imit of the   m                                                       l
                                       As   part of the validation procedure, the outliers (defined             as a  results which deviate
                                       significantly from the other values in a measurement series) should be excluded before
                                       reporting the 95th percentiles and the 97th percentiles. Furthermore, since the data reported
            97th Percentiles           here should refer only to normal operating conditions, any data refering to other-than-normal
                                       operating conditions, as well as periods when the plant was not operational, should be
                                       excluded if possible. If the measured value is below the detection limit report the detection
                                        imit of the measurement         method in the Comments cell
                                       The average value of the valid daily averages (hourly and half-houlry) recorded during                        a
                                       period   of  one   year. Hourly and half-hourly averages are valid when other than normal
             Yearly average
                                       operating     conditions and    plant   shut down data     are excluded from the dataset.
                                                                                     Sheet 5. Endnotes
                                                                                                                                                                    0000000173
</pre>

====================================================================== Einde pagina 91 =================================================================

<br><br>====================================================================== Pagina 92 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                         pecify the    cases   of other than normal           operating conditions (OTNOC) which are included
                                        nd how emissions to air         during OTNOC are regulated. In the case of continuous
                                         easurements please provide more insight into some specific conditions. You may include
                                       he information here or attach additional information, such as graphs of emissions or a copy
                                        fthe permit, as an annex to the questionnaire and report the file name here. As an
                                       ndication, for the purpose of the drawing up ofthe WGC BREF, OTNOC can include: start-
                                        p and shutdown operations of the production plant (excluding routine fluctuations, e.g.
                                        roduct changeover for individual production lines); waste water treatment plant start-up
         Specify    the cases   of
                                       especially     for seasonal operations);+ failure/unavailability of abatement equipment;
     OTNOC which are included
                                         ilure/unavailability of monitoring equipment;+ major accidental spillages of liquids;+
                                      emergency operations or actions taken for critical safety issues;s definitive cessation of
                                      production operations.
                                      According      to EN   15259,    measurement            planning  shall consider    plant-specific conditions. A
                                      check shall be made          as to  whether, in view of the         measurement       objective, the necessary
                                      measuring conditions are satisfied.For batch processes in particular the timing of the
                                      emission measurements shall take these circumstances into account sufficiently. Especially
        Measurement       planning
                                      in the  case of very short-term emission events, a check shall be made as to whether several
                                      similar emission events can be combined in one sampling in order to enable evaluation of
                                      the operating state.
                                                                                            3.2.  Absorption
                                      Please indicate               the                            which pollutant(s) are removed by the technique.
                                                                                                                                                            |Backte     |
                Substance                                   using       drop-down         menu
                                                                                                                                                             worksheet
                                      Please indicate       using   the drop-down         menu if the main goal of the technique is to remove the
           Removal purpose            associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                      remove this substance but partial removal of the substance occurs all the same (abatement
                                      Please select from the drop-down               menu       (the options  are  generally   taken from the CWW
                   Type               BREF).     If other, please provide information in the Comments cell.
           Last retrofit   (year)     According      to the IED    permit   or  substantial       changes granted by the IED permit.
                                      Please describe how the           operator     ensures      that the technique is running under        normal
          Control    parameters       operating     conditions and that       no   significant pollution is caused.
                                      Conditions of the IED         permit under which the treatment equipment                 may be     bypassed (e.g.
           Bypass    conditions
                                      when the lower        explosion limit threshold is exceeded).
      Waste gas     treatment(s)   in When the technique is bypassed, please explain which                       treatment(s)    are  applied  to the waste
             case  of  bypass         gases. If no treatment is applied, indicate "none".
                                      Please    provide    the removal      efficiency      of the  technique   for each substance. This       can  be the
        Removal     efficiency (%)    design   value.
                     method for       Please select from        a  drop-down      list for    specifying  the method for     deriving   the removal
          Deriving
           removal    efficiency      efficiency.
                                      Turnaround        means a    unit  or plant    shutdown       required  for maintenance      or  modifications of the
          Turmaround interval         unit  or plant.    Please describe the turnaround interval and/or intervals for routine
                                      maintenance        activities, which    can    include     periodic inspections     and the   replacement    of
                                      Turnaround        means    a unit  or plant    shutdown       required  for maintenance      or  modifications to the
             Last turnaround          unit  or plant.    Please describe the        month/year of the last turnaround           interval and/or intervals
                                      for routine maintenance activities.
                                      If the IED    permit   sets   a minimum       operating      time  requirement    for the  technique, please
       Minimum     operating    time
                                      indicate in hours per year (e.g. for a continuous process 24/365, the IED                        permit might
                   (hiyr)             require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                      This should be the time that the waste gas system is operating, e.g. a process may be shut
                                      down at weekends but the equipment continues to operate because if it were switched off
         Operating time of the
                                      there would be       problems restarting         it the   following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                      may be    operated occasionally for a             few hours     only, for example in the case ofparticular
                                        Pa Pl CrTET TPle
            Do the waste gas          Typically,    the waste gas properties may vary in the case of multipurpose productions, batch
             properties vary          processes. Waste gas properties may also vary when an emission point receives emissions
                                      from both batch and continuous processes. In this case, select Yes' to report upto 12
      significantly under normal
                                      measurement values.
        operating conditions?
                                      The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)          temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                      (i.e. HzO content).      In the  case    of continuous        monitoring   of the  flow, please report the 95th
                                        ercentile
                                      Water vapour content emitted to atmosphere from ducts and stacks (see EN                              14790).  In the
               Humidity (%)           case of continuous monitoring of humidity, please report the 95th percentile.
                                      Temperature of the         waste gas. If the        temperature is monitored continuously, please report
            Temperature (°C)          the 95th percentile.
     Operating temperature (°C) Temperature              at which the    equipment         is  designed to operate.
                                                                                        Sheet 5. Endnotes
                                                                                                                                                                      0000000174
</pre>

====================================================================== Einde pagina 92 =================================================================

<br><br>====================================================================== Pagina 93 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                                  3.2. Adsorption
                Substance            Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                 |Backte      |
                                                                                                                                                                  worksheet
                                     Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type              BREF).       If other, please provide information in the Comments cell.
           Last retrofit  (year)     According         to the IED       permit     or substantial       changes granted by the IED permit.
                                     Please describe how the                  operator      ensures      that the technique is running under      normal
          Control   parameters       operating       conditions        and that no significant pollution is caused.
                                     Conditions of the IED               permit under which the treatment equipment                 may be     bypassed (e.g.
           Bypass    conditions
                                     when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                              treatment(s)   are  applied to the waste
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please      provide      the removal          efficiency     of the   technique  for each substance. This      can  be the
        Removal     efficiency (%)   design      value.
                     method for      Please select from             a   drop-down        list for   specifying  the method for    deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround          means a        unit    or plant   shutdown        required for maintenance     or  modifications of the
          Turnaround interval        unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                            include     periodic inspections   and the   replacement    of
                                     maintenance activities, which                   can
                                     Turnaroundmeans                 a  unit    or plant   shutdown        required for maintenance     or  modifications to the
             Last turnaround         unit  or   plant.    Please describe the              month/year of the last turnaround         interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED      permit     sets     a  minimum       operating       time requirement   for the  technique, please
       Minimum     operating   time
                                     indicate in hours per year (e.g. for a continuous process 24/365, the IED                              permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the    down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                     there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be                      occasionally for a            few hours only, for example in the case of particular
                                       mem
                                           lm     operatedpm
                                               mignon)     Dm    me
                                                                    gm mm  mg
                                                                              gm
            Do the waste gas         Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas                  properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to                              report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                    Ce
                                     Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)          case     of continuous         monitoring        of  humidity, please report       the 95th   percentile.
                                     Temperature of the waste $ gas. If the temperature               P         is monitored continuously, $:ip please report
                                                                                                                                                           P
            Temperature (°C)               bP
                                     the 95th percentile.
     Operating temperature (°C) Temperature               at which the           equipment       is  designed to operate.
                                                                                               Sheet 5. Endnotes
                                                                                                                                                                            0000000175
</pre>

====================================================================== Einde pagina 93 =================================================================

<br><br>====================================================================== Pagina 94 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                                  3.2. Bioprocess
                Substance            Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                 |Backte      |
                                                                                                                                                                  worksheet
                                     Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type              BREF).       If other, please provide information in the Comments cell.
           Last retrofit  (year)     According         to the IED       permit     or substantial       changes granted by the IED permit.
                                     Please describe how the                  operator      ensures      that the technique is running under      normal
          Control   parameters       operating       conditions        and that no significant pollution is caused.
                                     Conditions of the IED               permit under which the treatment equipment                 may be     bypassed (e.g.
           Bypass    conditions
                                     when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                              treatment(s)   are  applied to the waste
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please      provide      the removal          efficiency     of the   technique  for each substance. This      can  be the
        Removal     efficiency (%)   design      value.
                     method for      Please select from             a   drop-down        list for   specifying  the method for    deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround          means a        unit    or plant   shutdown        required for maintenance     or  modifications of the
          Turnaround interval        unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                            include     periodic inspections   and the   replacement    of
                                     maintenance activities, which                   can
                                     Turnaroundmeans                 a  unit    or plant   shutdown        required for maintenance     or  modifications to the
             Last turnaround         unit  or   plant.    Please describe the              month/year of the last turnaround         interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED      permit     sets     a  minimum       operating       time requirement   for the  technique, please
       Minimum     operating   time
                                     indicate in hours per year (e.g. for a continuous process 24/365, the IED                              permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the    down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                     there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be                      occasionally for a            few hours only, for example in the case of particular
                                       mem
                                           lm     operatedpm
                                               mignon)     Dm    me
                                                                    gm mm  mg
                                                                              gm
            Do the waste gas         Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas                  properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to                              report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                    Ce
                                     Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)          case     of continuous         monitoring        of  humidity, please report       the 95th   percentile.
                                     Temperature of the waste $ gas. If the temperature               P         is monitored continuously, $:ip please report
                                                                                                                                                           P
            Temperature (°C)               bP
                                     the 95th percentile.
                                     Examples          of organic filtering         material: root       wood,  tree bark, peat, compost,      coconut fibre
              Filter material                   mixtures of these.
                                     i
                                                                                               Sheet 5. Endnotes
                                                                                                                                                                            0000000176
</pre>

====================================================================== Einde pagina 94 =================================================================

<br><br>====================================================================== Pagina 95 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                               3.2. Cold oxidation
                Substance            Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                |Backte      |
                                                                                                                                                                 worksheet
                                     Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type              BREF).       If other, please provide information in the Comments cell.
           Last retrofit  (year)     According         to the IED       permit     or substantial      changes granted by the IED permit.
                                     Please describe how the                  operator      ensures    that the technique is running under       normal
          Control   parameters       operating       conditions        and that no significant pollution is caused.
                                     Conditions of the IED               permit under which the treatment equipment                may be     bypassed (e.g.
           Bypass    conditions
                                     when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                             treatment(s)   are  applied to the waste
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please      provide      the removal          efficiency     of the  technique  for each substance. This      can  be the
        Removal     efficiency (%)   design      value.
                     method for      Please select from             a   drop-down        list for  specifying  the method for    deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround          means a        unit    or plant   shutdown       required for maintenance     or  modifications of the
          Turnaround interval        unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                            include   periodic inspections    and the   replacement    of
                                     maintenance activities, which                   can
                                     Turnaroundmeans                 a  unit    or plant   shutdown       required for maintenance     or  modifications to the
             Last turnaround         unit  or   plant.    Please describe the              month/year of the last turnaround        interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED      permit     sets     a  minimum       operating      time requirement   for the  technique, please
       Minimum     operating   time
                                     indicate in hours per year (e.g. for a continuous process 24/365, the IED                             permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the    down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                     there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be                      occasionally for a            few hours only, for example in the case of particular
                                       mem
                                           lm     operatedpm
                                               mignon)     Dm    me
                                                                    gm mm  mg
                                                                              gm
            Do the waste gas         Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas                  properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to                             report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                                     Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)          case     of continuous         monitoring        of  humidity, please report      the 95th   percentile.
                                     Temperature of the              waste gas. If the           temperature is monitored continuously, please report
            Temperature (°C)         the 95th percentile.
                                                                                               Sheet 5. Endnotes
                                                                                                                                                                           0000000177
</pre>

====================================================================== Einde pagina 95 =================================================================

<br><br>====================================================================== Pagina 96 ======================================================================

<pre>30141731
     Drawing      up of the WGC BREF
                                                                                          J.2. Condensation
                                                                                                                                                           Back ¢
                  Substance              Please indicate      using  the  drop-down menu which pollutant(s) are removed by the technique.                 worksheet
                                         Please indicate      using  the drop-down menu if the main goal of the technique is to remove the
             Removal purpose             associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                         remove this substance but partial removal of the substance occurs all the same (abatement
                                         Please select from the drop-down              menu (the options are generally taken from the CWW
                     Type                BREF).     If other, please provide information in the Comments cell.
             Last retrofit   (year)      According      to the IED  permit    or substantial     changes granted by the IED permit.
                                         Please describe how the          operator     ensures   that the technique is running under       normal
            Control   parameters         operating     conditions   and that no significant pollution is caused.
                                         Conditions of the IED       permit under which the treatment equipment              may be     bypassed (e.g.
             Bypass    conditions
                                         when the lower       explosion limit threshold is exceeded).
      Waste gas       treatment(s)    in [When the technique is bypassed, please explain which                  treatment(s)   are  applied to the waste
               case  of  bypass          gases. If no treatment is applied, indicate "none".
                                         Please    provide   the removal      efficiency    of the  technique  for each substance. This      can  be the
        Removal       efficiency (%)     design    value.
                       method for        Please select from      a  drop-down       list for specifying  the method for    deriving   the removal
            Deriving
             removal    efficiency       efficiency.
                                         Turnaround       means a    unit  or plant   shutdown      required for maintenance     or  modifications of the
            Turnaround interval          unit  or plant.   Please describe the turnaround interval and/or intervals for routine
                                                                                       include  periodic inspections    and the   replacement    of
                                         maintenance activities, which          can
                                         Turnaroundmeans          a  unit  or plant   shutdown      required for maintenance     or  modifications to the
               Last turnaround           unit  or plant.   Please describe the        month/year of the last turnaround       interval and/or intervals
                                         for routine maintenance activities.
         LC                   .     .
                                         If the IED    permit  sets  a minimum       operating     time requirement   for the  technique, please
       Minimum       operating     time
                                         j, icate in hours per year (e.g. for a continuous process 24/365, the IED                   permit might
                     (hiyr)              require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                         This should be the time that the waste gas system is operating, e.g. a process may be shut
                        time of the      down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                         there would be problems restarting it the following week. Or, on the contrary, the equipment
              equipment (hiyr)
                                         may be operated occasionally for a few hours only, for example in the case of particular
              Do the waste gas           Typically, theWaste gas properties may vary in the                case  of multipurpose productions,      batch
               properties vary           processes. Waste gas properties may also vary when an emission point receives emissions
                                         [fom both batch and continuous processes. In this case, select 'Yes' to report upto 12
      significantly under normal
                                         The measured volume flow rate of the waste gas converted to standard conditions at a
                Flow   (Nm3/h)           temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                         (i.e. H20 content). In the       case   of continuous monitoring of the flow, please report the 95th
                                         Water    vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
                 Humidity (%)            case   of continuous     monitoring     of  humidity, please report     the 95th   percentile.
                                         Temperature of the       waste gas. If the       temperature is monitored continuously, please report
              Temperature (°C)           the 95th percentile.
       Type     of cooling    medium     [Specify   the medium used in the condenser               (primary cooling curcuit) using the drop-down
                        of the           [f there is   an  evaporative cooling water system (as the primary or secondary circuit) enter
     Temperature                 cooling
                 medium                  the total   cooling water consumption (evaporative losses + blowdown).
                            (°C)
                                                                                         Sheet 5. Endnotes
                                                                                                                                                                    0000000178
</pre>

====================================================================== Einde pagina 96 =================================================================

<br><br>====================================================================== Pagina 97 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                               3.2. Dust scrubbing
                Substance            Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                 |Backte      |
                                                                                                                                                                  worksheet
                                     Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type              BREF).       If other, please provide information in the Comments cell.
           Last retrofit  (year)     According         to the IED       permit     or substantial       changes granted by the IED permit.
                                     Please describe how the                  operator      ensures      that the technique is running under      normal
          Control   parameters       operating       conditions        and that no significant pollution is caused.
                                     Conditions of the IED               permit under which the treatment equipment                 may be     bypassed (e.g.
           Bypass    conditions
                                     when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                              treatment(s)   are  applied to the waste
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please      provide      the removal          efficiency     of the   technique  for each substance. This      can  be the
        Removal     efficiency (%)   design      value.
                     method for      Please select from             a   drop-down        list for   specifying  the method for    deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround          means a        unit    or plant   shutdown        required for maintenance     or  modifications of the
          Turnaround interval        unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                            include     periodic inspections   and the   replacement    of
                                     maintenance activities, which                   can
                                     Turnaroundmeans                 a  unit    or plant   shutdown        required for maintenance     or  modifications to the
             Last turnaround         unit  or   plant.    Please describe the              month/year of the last turnaround         interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED      permit     sets     a  minimum       operating       time requirement   for the  technique, please
       Minimum     operating   time
                                     indicate in hours per year (e.g. for a continuous process 24/365, the IED                              permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the    down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                     there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be                      occasionally for a            few hours only, for example in the case of particular
                                       mem
                                           lm     operatedpm
                                               mignon)     Dm    me
                                                                    gm mm  mg
                                                                              gm
            Do the waste gas         Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas                  properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to                              report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                    Ce
                                     Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)          case     of continuous         monitoring        of  humidity, please report       the 95th   percentile.
                                     Temperature of the waste $ gas. If the temperature               P         is monitored continuously, $:ip please report
                                                                                                                                                           P
            Temperature (°C)               bP
                                     the 95th percentile.
     Operating temperature (°C) Temperature               at which the           equipment       is  designed to operate.
                                                                                               Sheet 5. Endnotes
                                                                                                                                                                            0000000179
</pre>

====================================================================== Einde pagina 97 =================================================================

<br><br>====================================================================== Pagina 98 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                                 3.2. Elec. precip.
                Substance            Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                |Backte      |
                                                                                                                                                                 worksheet
                                     Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type              BREF).       If other, please provide information in the Comments cell.
           Last retrofit  (year)     According         to the IED       permit     or substantial      changes granted by the IED permit.
                                     Please describe how the                  operator      ensures    that the technique is running under       normal
          Control   parameters       operating       conditions        and that no significant pollution is caused.
                                     Conditions of the IED               permit under which the treatment equipment                may be     bypassed (e.g.
           Bypass    conditions
                                     when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                             treatment(s)   are  applied to the waste
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please      provide      the removal          efficiency     of the  technique  for each substance. This      can  be the
        Removal     efficiency (%)   design      value.
                     method for      Please select from             a   drop-down        list for  specifying  the method for    deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround          means a        unit    or plant   shutdown       required for maintenance     or  modifications of the
          Turnaround interval        unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                            include   periodic inspections    and the   replacement    of
                                     maintenance activities, which                   can
                                     Turnaroundmeans                 a  unit    or plant   shutdown       required for maintenance     or  modifications to the
             Last turnaround         unit  or   plant.    Please describe the              month/year of the last turnaround        interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED      permit     sets     a  minimum       operating      time requirement   for the  technique, please
       Minimum     operating   time
                                     indicate in hours per year (e.g. for a continuous process 24/365, the IED                             permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the    down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                     there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be                      occasionally for a            few hours only, for example in the case of particular
                                       mem
                                           lm     operatedpm
                                               mignon)     Dm    me
                                                                    gm mm  mg
                                                                              gm
            Do the waste gas         Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas                  properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to                             report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                                     Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)          case     of continuous         monitoring        of  humidity, please report      the 95th   percentile.
                                     Temperature of the              waste gas. If the           temperature is monitored continuously, please report
            Temperature (°C)         the 95th percentile.
                                                                                               Sheet 5. Endnotes
                                                                                                                                                                           0000000180
</pre>

====================================================================== Einde pagina 98 =================================================================

<br><br>====================================================================== Pagina 99 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                                    3.2. Filtration
                Substance            Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                 |Backte      |
                                                                                                                                                                  worksheet
                                     Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type              BREF).       If other, please provide information in the Comments cell.
           Last retrofit  (year)     According         to the IED       permit     or substantial       changes granted by the IED permit.
                                     Please describe how the                  operator      ensures      that the technique is running under      normal
          Control   parameters       operating       conditions        and that no significant pollution is caused.
                                     Conditions of the IED               permit under which the treatment equipment                 may be     bypassed (e.g.
           Bypass    conditions
                                     when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                              treatment(s)   are  applied to the waste
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please      provide      the removal          efficiency     of the   technique  for each substance. This      can  be the
        Removal     efficiency (%)   design      value.
                     method for      Please select from             a   drop-down        list for   specifying  the method for    deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround          means a        unit    or plant   shutdown        required for maintenance     or  modifications of the
          Turnaround interval        unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                            include     periodic inspections   and the   replacement    of
                                     maintenance activities, which                   can
                                     Turnaroundmeans                 a  unit    or plant   shutdown        required for maintenance     or  modifications to the
             Last turnaround         unit  or   plant.    Please describe the              month/year of the last turnaround         interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED      permit     sets     a  minimum       operating       time requirement   for the  technique, please
       Minimum     operating   time
                                     indicate in hours per year (e.g. for a continuous process 24/365, the IED                              permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the    down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                     there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be                      occasionally for a            few hours only, for example in the case of particular
                                       mem
                                           lm     operatedpm
                                               mignon)     Dm    me
                                                                    gm mm  mg
                                                                              gm
            Do the waste gas         Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas                  properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to                              report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                    Ce
                                     Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)          case     of continuous         monitoring        of  humidity, please report       the 95th   percentile.
                                     Temperature of the waste $ gas. If the temperature               P         is monitored continuously, $:ip please report
                                                                                                                                                           P
            Temperature (°C)               bP
                                     the 95th percentile.
     Operating temperature (°C) Temperature               at which the           equipment       is  designed to operate.
                                                                                               Sheet 5. Endnotes
                                                                                                                                                                            0000000181
</pre>

====================================================================== Einde pagina 99 =================================================================

<br><br>====================================================================== Pagina 100 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                             3.2. Gravit. sep.
                Substance            Please indicate           using   the drop-down        menu     which pollutant(s)   are  removed      by the technique.
                                                                                                                                                              |Backte      |
                                                                                                                                                               worksheet
                                     Please indicate           using   the drop-down        menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                  menu       (the options  are  generally  taken from the CWW
                   Type              BREF).          If other, please provide information in the Comments cell.
           Last retrofit  (year)     According           to the IED   permit   or substantial       changes granted by the IED permit.
                                     Please describe how the               operator    ensures      that the technique is running under normal
          Control   parameters       operating conditions and that no significant pollution is caused.
                                     Conditions of the IED permit under which the treatment equipment may be bypassed (e.g.
           Bypass    conditions
                                     when the lower explosion limit threshold is exceeded).
      Waste gas                   in When the technique is bypassed, please explain which treatment(s) are applied to the waste
                    treatment(s)
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please         provide   the removal      efficiency     of the  technique   for each substance. This       can  be the
        Removal     efficiency (%)   design        value.
                     method for      Please select from            a  drop-down     list for    specifying  the method for    deriving    the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround            means a    unit  or plant   shutdown       required  for maintenance       or modifications of the
          Turnaround interval        unit    or   plant.    Please describe the turnaround interval and/or intervals for routine
                                     maintenance            activities, which    can   include     periodic inspections    and the     replacement   of
                                     Turnaround            means a unit     or plant   shutdown       required  for maintenance       or modifications to the
             Last turnaround         unit    or   plant.    Please describe the       month/year of the last turnaround          interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED         permit   sets  a minimum      operating      time  requirement   for the  technique, please
       Minimum     operating   time  indicate in hours per year (e.g. for a continuous process 24/365, the IED                           permit might
                   (hiyr)            require that the technique should work 90% of the time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                                     down at weekends but the equipment continues to operate because if it were switched off
         Operating time of the
                                     there would be           problems restarting        it the   following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be          operated occasionally for a          few hours     only, for example in the case ofparticular
                                             ln
                                         dom
                                                 emp emmlymd mam
            Do the waste gas         Typically,         the waste gas properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e.   H20        content).  In the  case   of continuous        monitoring  of the  flow, please report the 95th
                                     Water        vapour
                                                      P      content emitted to      atmosphere from ducts and stacks             ( (see EN 14790).) In the
               Humidity (%)          case       of continuous       monitoring    of           Pp
                                                                                     humidity, please report        the 95th   percentile.
                                     Temperature of the             waste gas. If the       temperature is monitored       continuously, please report
            Temperature (°C)         the 95th percentile.
                                                            at which the                     is  designed to operate.
     Operating temperature (°C) Temperature                                 equipment
                                                                                          Sheet 5. Endnotes
                                                                                                                                                                         0000000182
</pre>

====================================================================== Einde pagina 100 =================================================================

<br><br>====================================================================== Pagina 101 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                         3.2. Membrane sep.
                Substance            Please indicate          using   the drop-down        menu which pollutant(s)      are  removed     by the technique.
                                                                                                                                                            |Backte      |
                                                                                                                                                             worksheet
                                     Please indicate          using   the drop-down        menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select from the drop-down                 menu     (the options   are  generally  taken from the CWW
                   Type              BREF).         If other, please provide information in the Comments cell.
           Last retrofit  (year)     According          to the IED   permit   or substantial     changes granted by the IED permit.
                                     Please describe how the              operator    ensures     that the technique is running under normal
          Control   parameters       operating conditions and that no significant pollution is caused.
                                     Conditions of the IED permit under which the treatment equipment may be bypassed (e.g.
           Bypass    conditions
                                     when the lower explosion limit threshold is exceeded).
      Waste gas                   in When the technique is bypassed, please explain which treatment(s) are applied to the waste
                    treatment(s)
             case  of  bypass        gases. If no treatment is applied, indicate "none".
                                     Please        provide   the removal      efficiency    of the  technique   for each substance. This       can  be the
        Removal     efficiency (%)   design       value.
                     method for      Please select from           a  drop-down     list for  specifying   the method for    deriving  the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround           means a    unit  or plant  shutdown       required  for maintenance     or modifications of the
          Turnaround interval        unit    or  plant.    Please describe the turnaround interval and/or intervals for routine
                                     maintenance           activities, which    can   include    periodic inspections    and the   replacement     of
                                     Turnaround           means a unit     or plant  shutdown       required  for maintenance     or modifications to the
             Last turnaround         unit    or  plant.    Please describe the       month/year of the last turnaround         interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED        permit   sets  a minimum     operating      time  requirement   for the  technique, please
       Minimum     operating   time  indicate in hours per year (e.g. for a continuous process 24/365, the IED                       permit might
                   (hiyr)            require that the technique should work 90% of the time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                                     down at weekends but the equipment continues to operate because if it were switched off
         Operating time of the
                                     there would be          problems restarting        it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be         operated occasionally for a          few hours    only, for example in the case ofparticular
                                             ln
                                         dom
                                                emp emmlymd mam
            Do the waste gas         Typically,        the waste gas properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select Yes' to report upto 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e.   H20       content).  In the  case   of continuous       monitoring  of the  flow, please report the 95th
                                     Water vapour content emitted to atmosphere from ducts and stacks (see EN                              14790).   In the
                    Ce
               Humidity (%)          case of continuous monitoring of humidity, please report the 95th percentile.
                                     Temperature
                                              3            of the waste 9 gas. If the temperature
                                                                                               P          is monitored   continuously, Y: P please report
                                                                                                                                                      p
            Temperature (°C)         the 95th percentile.
     Operating temperature (°C) Temperature at which the equipment is designed to operate.
       Membrane replacement          Membranes have to be replaced periodically; please specify the replacement                            rate in months.
                    rate
                                                                                         Sheet 5. Endnotes
                                                                                                                                                                       0000000183
</pre>

====================================================================== Einde pagina 101 =================================================================

<br><br>====================================================================== Pagina 102 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                                    3.2. Reduction
                Substance              Please indicate          using      the   drop-down menu which pollutant(s) are removed by the technique.
                                                                                                                                                                   |Backte      |
                                                                                                                                                                    worksheet
                                       Please indicate          using      the drop-down menu if the main goal of the technique is to remove the
           Removal purpose             associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                       remove this substance but partial removal of the substance occurs all the same (abatement
                                       Please select from the drop-down                       menu (the options are generally taken from the CWW
                   Type                BREF).       If other, please provide information in the Comments cell.
           Last retrofit    (year)     According         to the IED       permit     or substantial      changes granted by the IED permit.
                                       Please describe how the                  operator      ensures     that the technique is running under       normal
          Control   parameters         operating       conditions        and that no significant pollution is caused.
                                       Conditions of the IED               permit under which the treatment equipment                 may be     bypassed (e.g.
           Bypass    conditions
                                       when the lower           explosion limit threshold is exceeded).
      Waste gas     treatment(s)    in When the technique is bypassed, please explain which                              treatment(s)   are  applied to the waste
             case  of  bypass          gases. If no treatment is applied, indicate "none".
                                       Please      provide      the removal          efficiency     of the  technique   for each substance. This      can  be the
        Removal     efficiency (%)     design      value.
                     method for        Please select from             a   drop-down        list for  specifying  the method for     deriving   the removal
          Deriving
           removal    efficiency       efficiency.
                                       Turnaround          means a        unit    or plant   shutdown       required  for maintenance     or  modifications of the
          Turnaround interval          unit  or   plant.    Please describe the turnaround interval and/or intervals for routine
                                                                                              include    periodic inspections    and the   replacement    of
                                       maintenance activities, which                   can
                                       Turnaroundmeans                 a  unit    or plant   shutdown       required  for maintenance     or  modifications to the
             Last turnaround           unit  or   plant.    Please describe the              month/year of the last turnaround         interval and/or intervals
                                       for routine maintenance activities.
                                       If the IED      permit     sets     a  minimum       operating      time requirement    for the  technique, please
       Minimum     operating     time
                                       indicate in hours per year (e.g. for a continuous process 24/365, the IED                              permit might
                   (hiyr)              require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                       This should be the time that the waste gas system is operating, e.g. a process may be shut
                      time of the      down at weekends but the equipment continues to operate because if it were switched off
         Operating
                                       there would be           problems restarting             it the following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                       may be                      occasionally for a            few hours only, for example in the case of particular
                                         mem
                                             lm     operatedpm
                                                 mignon)     Dm    me
                                                                      gm mm  mg
                                                                                gm
            Do the waste gas           Typically, the waste              gas   properties may vary in the case of multipurpose productions, batch
             properties vary           processes. Waste gas                  properties may also vary when an emission point receives emissions
                                       from both batch and continuous processes. In this case, select Yes' to                              report upto 12
      significantly under normal
                                       measurement values.
        operating conditions?
                                       The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)           temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                       (i.e. H20 content). In the               case    of continuous monitoring of the flow, please report the 95th
                    Ce
                                       Water      vapour content emitted to atmosphere from ducts and stacks (see EN 14790). In the
               Humidity (%)            case     of continuous         monitoring        of  humidity, please report       the 95th   percentile.
                                       Temperature of the waste $ gas. If the temperature              P         is monitored continuously, $:ip please report
                                                                                                                                                             P
            Temperature (°C)                 bP
                                       the 95th percentile.
          Permitted reference          Please      report     the referencen oxygen level                 according  to EN 147889.
       oxygen level     (if relevant)
                                                                                                 Sheet 5. Endnotes
                                                                                                                                                                              0000000184
</pre>

====================================================================== Einde pagina 102 =================================================================

<br><br>====================================================================== Pagina 103 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                        3.2. Th. oxidation
                Substance            Please indicate       using   the  drop-down       menu    which  pollutant(s) are removed by the technique.
                                                                                                                                                          |Backte       |
                                                                                                                                                            worksheet
                                     Please indicate       using   the  drop-down       menu if the main goal of the technique is to remove the
           Removal purpose           associated substance (i.e. abatement primary), or if the main goal of the technique is not to
                                     remove this substance but partial removal of the substance occurs all the same (abatement
                                     Please select the       type of thermal oxidiser.
                                     NB:    Recuperative thermal         oxidiser   means a      continuously operating heat exchanger           in which
                                     the thermal energy content of           a fluid is transferred via      a heat exchange surface to a         second
                                     fluid ofa lower temperature.
                   Type
                                     Regenerative thermal           oxidiser  means an       intermittently operating      heat exchanger     in which
                                     the thermal energy content of a fluid is alternatively stored and transferred to a second fluid
                                     with a lower temperature level for heating purposes. (e.g. waste gas preheating)
           Last retrofit  (year)     According      to the IED    permit or substantial changes granted by the IED permit.
                                     Please describe how the           operator ensures that the technique is running under normal
          Control    parameters      operating conditions and that no significant pollution is caused.
                                     Conditions of the IED permit under which the treatment equipment may be bypassed (e.g.
           Bypass    conditions
                                     when the lower explosion limit threshold is exceeded).
      Waste gas     treatment(s)  in When the technique is bypassed, please explain which                      treatment(s)    are  applied  to the waste
             case   of bypass        gases. If no treatment is applied, indicate "none".
                                     Please     provide   the removal      efficiency    of the  technique    for each substance. This       can  be the
        Removal     efficiency (%)   design    value.
                     method for      Please select from        a  drop-down     list for  specifying   the method for      deriving   the removal
          Deriving
           removal    efficiency     efficiency.
                                     Turnaround       means a     unit  or plant  shutdown       required   for maintenance      or  modifications of the
                                     unit  or  plant.  Please describe the turnaround interval and/or intervals for routine
          Turnaround interval
                                     maintenance        activities, which    can   include    periodic inspections      and the   replacement    of        |Backte      |
                                                                                                                                                            worksheet
                                     Turnaround       means    a unit   or plant shutdown        required for maintenance or modifications to the
             Last turnaround         unit  or  plant.  Please describe the        month/year of the last turnaround interval and/or intervals
                                     for routine maintenance activities.
                                     If the IED    permit   sets   a  minimum    operating      time  requirement     for the technique, please
       Minimum     operating   time  indicate in hours per year (e.g. for a continuous process 24/365, the IED                       permit might
                   (hiyr)            require that the technique should work 90% ofthe time, i.e. 7884 hours).
                                     This should be the time that the waste gas system is operating, e.g. a process may be shut
                                     down at weekends but the equipment continues to operate because if it were switched off
         Operating time of the
                                     there would be       problems restarting        it the  following week. Or, on the contrary, the equipment
            equipment (h/yr)
                                     may be     operated occasionally for a           few hours    only, for example in the case ofparticular
                                          Pl
                                       Pa     CrTET TPle
            Do the waste gas         Typically,    the waste gas properties may vary in the case of multipurpose productions, batch
             properties vary         processes. Waste gas properties may also vary when an emission point receives emissions
                                     from both batch and continuous processes. In this case, select "Yes' to report up to 12
      significantly under normal
                                     measurement values.
        operating conditions?
                                     The measured volume flow rate of the waste gas converted to standard conditions at a
              Flow   (Nm3/h)         temperature of 273.15 K, and a pressure of 101.3 kPa, subtracting the waste gas humidity
                                     (i.e. H20    content).    In the  case   of continuous       monitoring    of the  flow, please report the 95th
                     Ceo
                                     Water vapour content emitted to atmosphere from ducts and stacks (see EN                             14790).  In the
               Humidity (%)          case of continuous monitoring of humidity, please report the 95th percentile.
                                     Temperature of the waste 8 gas. If the temperature     2          is monitored continuously, Ys please report  i
            Temperature (°C)               Pp
                                     the 95th percentile.
          Permitted reference        Please     report   the referencen oxygen level           according   to EN 147889.
       oxygen level (if relevant)
                                     Liquid or gaseous fuels required in addition to the combustible waste gas constituents to
           Type   of fuel added
                                     maintain the minimum reaction temperature.
                                     Retention time of the waste gas to be treated in the reaction chamber of the thermal
           Residence time            oxidation    system. The residence time is the quotient of the reaction chamber volume of the
                              (s)
                                     thermal oxidation       system.
       Combustion                    Mean     temperature in the reaction chamber               at which the oxidation of the waste gas
                       temperature
                    (°C)             constituents      occurs.
                                                                                      Sheet 5. Endnotes
                                                                                                                                                                      0000000185
</pre>

====================================================================== Einde pagina 103 =================================================================

<br><br>====================================================================== Pagina 104 ======================================================================

<pre>30141731
     Drawing   up of the WGC BREF
                                                                           3.2. Waste gas info
                                                                                                                                       Back ¢
                                    Typically,  the waste gas             may vary in the case of
           Do the waste gas                                    properties                         multipurpose productions, batch     worksheet
            properties vary         processes. Waste gas properties may also vary when an emission point receives emissions
                                    from both batch and continuous processes. In this case, select Yes' to report upto 12
      significantly under normal
                                    The measured volume flow rate in the      waste-gas converted to standard conditions at a
             Flow  (Nm3/h)                         of 273.15 K, and
                                    temperature                      a pressure of 101.3 kPa, subtracting the waste-gas humidity
                                     Poem BLY mmpnbmimdh
                                    Water vapour content emitted to atmosphere from ducts and stacks (see EN         14790).   In the
              Humidity (%)          case of continuous monitoring of humidity, please report the 95th percentile.
                           "        Temperature of the    waste gas. If the temperature is monitored continuously, please report
           Temperature (°C)         the 95th percentile.
                                                                             3.3. Polyolefins                                          Back |
                                    Please specify the polymer process that is being carried out using the drop-down list (which      worksheet
             Process                js taken from the POL BREF). If your process is not included in the drop-down list please
                        type
                                    specify  in the ‘comments’ field.
                                    A technique that prevents or reduces the final emissions or consumption levels      by changing
          Process-integrated        the design or operation of the process, or the choice of raw materials.
               techniques
                                                                 is the removal of the unconverted monomer, solvent
                           applied Devolatilisation/degassing                                                              by-
                                                                                                                        or
      What treatment is
          to emissions from         product from the crude product.
     degassing/devolatilisation?
                                    Monomer residue contained in the polymer at the transition    point between the closed     system
      Monomer concentration in and the treatment or
                                                           drying in the open system.
       the product (g VOC/kg)
         Recovery techniques        [Techniques applied to reuse the solvent and/or    monomer.
           Emissions to air         Mass of pollutant released per mass of product     manufactured  or mass  of raw  material used.
     (channelled and diffuse)    as
             specific loads
                                                                           Sheet 5. Endnotes
                                                                                                                                                0000000186
</pre>

====================================================================== Einde pagina 104 =================================================================

<br><br>====================================================================== Pagina 105 ======================================================================

<pre>30141731
     Drawing  up of the WGC BREF
                                                                                  3.3. PVC
                                                                                                                                       Back ¢
                                    Please   specify the polymer process that is being carried out using the drop-down list (which    worksheet
             Process                is taken from the  POL BREF). If your process is not included in the drop-down list please
                       type
                                    specify  in the ‘comments’ field.
                                    A  technique that prevents or reduces the final emissions or consumption     levels by changing
         Process-integrated         the design or operation of the process, or the choice of raw materials.
              techniques
                                                                 is the removal of the unconverted monomer, solvent
                           applied Devolatilisation/degassing                                                              by-
                                                                                                                        or
      What treatment is
          to emissions from         product from the crude product.
     degassing/devolatilisation?
                                    Monomer residue contained in the polymer at the transition     point between the closed    system
      VCM concentration in the nd the treatment or
                                                           drying in the open system.
         product (g VOC/kg)
        Recovery techniques         [Techniques applied to reuse the solvent and/or     monomer.
           Emissions to air         Mass of pollutant released per mass of product      manufactured  or mass of  raw material used.
     (channelled and diffuse)    as
            specific loads
                                                                          3.3. Sol. Pol. Rubbers
                                                                                                                                       Back {
                                    Please   specify the polymer process that is being carried out using the drop-down list (which    worksheet
             Process                is taken from the  POL BREF). If your process is not included in the drop-down list please
                       type
                                    specify  in the ‘comments’ field.
                                    A  technique that prevents or reduces the final emissions or consumption     levels by changing
         Process-integrated         the
              techniques                 design or operation of the process, or the choice of raw materials.
                                                                 is the removal of the unconverted monomer, solvent
                           applied Devolatilisation/degassing                                                              by-
                                                                                                                        or
      What treatment is
          to emissions from         product from the crude product.
     degassing/devolatilisation?
                                    Monomer residue contained in the polymer at the transition     point between the closed    system
      Monomer concentration in and the treatment or
                                                           drying in the open system.
       the product (g VOC/kg)
        Recovery techniques         [Techniques applied to reuse the solvent and/or     monomer.
           Emissions to air         Mass of pollutant released per mass of product      manufactured  or mass of raw  material used.
     (channelled and diffuse)    as
            specific loads
                                                                                3.3. Viscose
                                                                                                                                       Back |
                                    Please   specify the polymer process that is being carried out using the drop-down list (which    worksheet
             Process                is taken from the  POL BREF). If your process is not included in the drop-down list please
                       type
                                    specify  in the ‘comments’ field.
                                    A  technique that prevents or reduces the final emissions or consumption     levels by changing
         Process-integrated         the design or operation of the process, or the choice of raw materials.
              techniques
                                                                 is the removal of the unconverted monomer, solvent
                           applied Devolatilisation/degassing                                                              by-
                                                                                                                        or
      What treatment is
          to emissions from         product from the crude product.
     degassing/devolatilisation?
        Recovery techniques         [Techniques applied to reuse the solvent and/or     monomer.
           Emissions to air         Mass of pollutant released per mass of product      manufactured  or mass of  raw material used.
     (channelled  and   diffuse) as
            specific  loads
                                                                           Sheet 5. Endnotes
                                                                                                                                                0000000187
</pre>

====================================================================== Einde pagina 105 =================================================================

<br><br>====================================================================== Pagina 106 ======================================================================

<pre>30141731
     Drawing  up of the WGC BREF
                                                                               3.3. Process f-h
                                  Please describe      by using the drop-down menu. In order to better understand the
                                                                                                                                             |Backte      |
          Product                                                                                                                             worksheet
                    category      production/process, you may provide further information on the type of product.
                                  Indicate the combustion       optimisation (mixing   of fuel and combustion       air) by using  the drop-
                                  down   menu.
                                  a. air
                                  b. oxygen enrichment
        Combustion scenario       c. oxy-fuel burner
                                  Oxy-fuel combustion is a process of burning a fuel using             pure oxygen instead of air as the
                                  primary oxidising agent. Oxygen enrichment combustion                is a process of burning a fuel using
                                  pure oxygen/air.
                                  Some chemical processes have electrical heaters but most process furnaces/heaters                    are
                                  combustion units that provide heat and/or raw materials to the chemical process.
                                  Some furnaces/heaters carry out direct heating, in which the flue-gases are in direct contact
                                  with the material to be heated, e.g. processes for drying mineral products.
                                  Some furnaces/heaters carry out indirect heating, in which the heat from the                flue-gases is
                                  transferred to the material to be heated through a solid wall (without using an              intermediary
      Type  of process furnace/   heat transfer   fluid), e.g. cracker furnaces in which the material to be          heated  is pumped
                heater            through pipes which pass through the furnace combustion chamber.
                                  All electrical heaters    are indirect heaters. Some furnaces/heaters          are  dual-use in which the
                                  flue-gases provide both heat and a raw material to the process, e.g. when the flue-gas
                                  contains a high proportion of carbon monoxide or hydrogen. Some combustion unit
                                  furnaces/heaters may use some of the heat to generate steam and/or electricity.
                                  Please select the main fuel from the       drop-down    list. If ‘other’ is selected specify the main fuel
                    of fuel       in the ‘comments’ cell. If several fuels     are  used specify the other fuels in the ‘comments’ cell.
             Type
                                  In the  case  of coal, cil and other fuels   please provide the nitrogen and sulphur content of the
      Process  temperature (°C) Mean     temperature in the      reactor.
                                  Permitted total rated thermal      input of all process furnaces/heaters connected to the stack
      Total rated thermal   input where emissions       occur.
         Permitted reference      Please   report  the referencen oxygen level      according    to EN 147889.
      oxygen level (if relevant)
                                                                            Sheet 5. Endnotes
                                                                                                                                                        0000000188
</pre>

====================================================================== Einde pagina 106 =================================================================

<br><br>====================================================================== Pagina 107 ======================================================================

<pre>30141731
     Drawing    up of the WGC BREF
                                                                                               4. Diffuse emissions
                                      Please         explain the reason for monitoring the                 substance: e.g. compliance monitoring,
                                                                                                                                                               |Backte      |
                     of                                                                                                                                         worksheet
        Purpose         monitoring    operator self-monitoring, operational control,                       other regulation (e.g. health and safety).
                                      For the purpose of this question, unit means an installation or a part of an installation for
        Number of units where         which diffuse emissions should be monitored, as required by the IED permit or any other
                                      hational        regulation or standard.
         diffuse emissions       are
                 monitored            For     example, if the permit requires                  to monitor diffuse emissions from       a tank farm   or a
                                      particular production unit, this tank                    farm   or production  unit could be described     as a  unit.
                                      Diffuse emissions can be monitored using:
         Monitoring of diffuse        -
                                         measurement methods, e.g. using direct measurement at source or optical gas imaging
      emissions (measurement
                                      methods:
     and calculation/estimation) calculation/estimation
                                      -
                                                                                 methods, e.g. based on design values of the equipment or emission
                                      Select the chemical                   activity specified    in the environmental    permit using the drop-down list
                                      (which        is taken from Annex | to Directive                 2010/75/EU). In the case of stand-alone waste gas
        Main chemical       activity                                  that
                                      treatment           plants              are  not  permitted as chemical installations, indicate the chemical
                                      acitvity       of the main contributor to the waste gas flow.
                                      Production capacity of the unit. The aim ofthis field is to differentiate between small-,
      Production      capacity (t/yr) medium-, large- and very large-scale processes. The exact production capacity is not
       Process      operating time    The time           during which          the   production    process is  operating  and waste gases      are  generated.
                                      If the waste gas treatment system treats emissions from the production of polyolefins, PVC,
                                      solution-polymerised rubbers or viscose, please indicate which one by using the drop-down
           Particular    polymer      list. This will generate a specific worksheet (numbered 3.3). The generic information about
                production            the measurement of emission recovery techniques, abatement techniques and monitoring of
                                      emissions should be reported using the generic worksheets (numbered 3.1 and 3.2).
                                      Fugitive        emissions           are   emissions    resulting   from looseness of   equipment and piping systems
        Are              emissions    that    are     designed         to be     tight. The most     common    emission   points are valve stems, flanges,
              fugitive
                monitored?            pump shafts and open ends. Internal leaks of safety valves discharging to atmosphere are
                                      included in fugitive emissions and can lead to significant emissions if undetected.
     Are   non-fugitive    emissions  INon-fugitive emissions are diffuse emissions other than fugitive emissions (storage tanks,
                monitored?            loading/unloading of mobile containers, sewers, sampling points etc.).
                                      Mass balances are one basis for understanding the processes                              on a   site and the
                                      development of improvement strategies. For a complete mass                               balance, the inputs    must
           Number of solvent          equal the outputs.                 Not every      output path is relevant in every    case   (e.g. heavy   metals cannot
                                      be destroyed).
     management plan(s) (mass         The solvent
            balance exercise)                                  management plan (SMP) is generally used by operators to justify the
                                      compliance with the emission limit values in the permit, identify future reduction options,
                                      enable provision of information on solvent consumption and solvent emissions.
                                      Enter the number of Solvent Management Plan(s) that applies to the unit concerned.
                                      "Volatile organic compound’ (VOC) means any organic compound as well as the fraction of
           Are VOCs used        or
                                      creosote, having at 293.15 K a vapour pressure of 0.01 kPa or more, or having a                                          |Backte      |
        produced      in the  plant?                                                                                                                            worksheet
                                      corresponding volatility                   under the   particular   conditions of use  [Definition   from the  IED].
          Are VOCs with CMR           Volatile organic compound classified as carcinogenic, mutagenic or toxic for reproduction
           properties used or         according to the classification criteria of Regulation (EC) No 1272/2008 on classification,
        produced in the plant?        labelling and packaging of substances and mixtures (CLP).
                                      Process design (parameters such as the process temperature and pressure, and the vapour
      Is there   a  condition in the
                                      pressure of the process fluid) can influence the level of diffuse emissions. However, these
        permit for process and        parameters are not chosen independently, and may also depend on other parameters (e.g.
     plant design? If yes, please catalyst activity).
                   specify            Plant design: the                selection of      plant components,     and the  manner    in which   they are
                                        |
                                             firn 1 rad
      What are the main factors Example of factors which may influence the monitoring of diffuse emisssions to air: health
            that influence the        and safety regulations to reduce worker exposure to CMR substances or environmental
         monitoring      of diffuse   regulations or specific permit requirements to protect sensitive local habitats.
           emisssions to air?
                                      If  possible,           choose the        same    representative    year  as the one  for which channelled emissions
            Year of reference
                                      have been              reported.
                                      All VOC substances                     including    VOCs classified    as  carcinogenic, mutagenic      or toxic for
                Total VOCs            reproduction (CMR)                    of  category 1A, 1B under Part 3 of Annex IV to Regulation (EC) No
                                         272/2008             on   classification, labelling and packaging of substances and mixtures (CLP).
                                      VOCs classified                 as   carcinogenic, mutagenic or toxic for reproduction (CMR) of category 1A,
       VOCs classified       as CMR   1B under Part 3 of Annex IV to                       Regulation (EC) No 1272/2008 on classification, labelling
                    1AM1B
                                      and     packaging of substances and mixtures (CLP).
                                      VOCs classified                 as   carcinogenic, mutagenic or toxic for reproduction (CMR) of category 2
      VOCs classified       as CMR 2 under Part 3 of Annex |V to Regulation                          (EC) No 1272/2008 on classification, labelling and
                                      packaging of substances and mixtures                          (CLP).
     To which                         Please report here the requirements of the [ED permit, the requirements of national
                  type of substance
            do the   monitoring       regulation or standards. For example: do the requirements apply to all VOC substances?
         requirements apply?          Only VOCs classified as carcinogenic, mutagenic or toxic for reproduction? Only to
                                         mpbiomy glom         bnemdom
                                                      pe  myn         pm
                                                                          mem
                                                                                                Sheet 5. Endnotes
                                                                                                                                                                          0000000189
</pre>

====================================================================== Einde pagina 107 =================================================================

<br><br>====================================================================== Pagina 108 ======================================================================

<pre>30141731
     Drawing up ofthe WGC BREF
                               Sheet 5. Endnotes
                                                 0000000190
</pre>

====================================================================== Einde pagina 108 =================================================================

<br><br>====================================================================== Pagina 109 ======================================================================

<pre>30141731
     Drawing   up of the WGC BREF
                                                                               4.1. Fug. emissions
                                                                                                                                                Back to
                                   An    inventory of fugitive emission sources consists of the compilation of relevant basic data             worksheet
        Is there an  inventory  of on the composition and quantity of gas streams, and/or pieces of equipment in contact with
      fugitive  emission   sources these streams. The emitted streams are listed respective to their source, i.e. the production
                    2
                                   process from which they originate.
         Number of accessible      Equipment/source         other than inaccessible     equipment/sources (see below).        Please   provide
                 sources           the number if available.
      Number of non-accessible     Equipment/source requiring special measures to be monitored,                  e.g. scaffolding,  removal of
                 sources           equipment's insulation. Please provide the number if available.
                                   Fugitive VOC emissions can be reduced by the detection and subsequent repair or
                                   replacement of leaking components. This is achieved by adopting a structured approach,
      Does the unit   apply a leak commonly known as a leak detection and repair (LDAR) programme. An LDAR programme
          detection and   repair   is usually risk-based and includes two fundamental steps:
              programme?           -
                                      identification of the leaking components;
                                   -
                                      repair of these leaks in order to minimise losses.
                                   Y ou may select one or several types of          high-integrity equipment      per category. High-integrity
                                   equipment includes for example:
                                   -
                                      valves with double      packing seals;
         Type of high-integrity    -
                                      magnetically driven pumps/compressors/agitators;
          equipment installed      -
                                      pumps/compressors/agitators fitted with mechanical seals instead of packing;
                                   -
                                      high-integrity gaskets (such as spiral wound, ring joints) for critical applications;
                                   -
                                      corrosion-resistant equipment.
                                   A   representative    value that    attempts  to relate the  quantity  ofa pollutant released to the
            Emission factors                        with  an  activity associated with the release     ofthat pollutant. Such factors
                                   pnosihers
                                       cilitate estimation of emissions from various        sources   of air pollution.
                                   If  possible,   choose the    same    representative  year   as the one   for which channelled emissions
            Year of reference
                                   have been      reported.
                                   All VOC substances          including  VOCs classified    as  carcinogenic, mutagenic      or toxic for
               Total VOCs          reproduction (CMR)         of category 1A, 1B under Part 3 of Annex |V to Regulation (EC) No
                                   1272/2008       on  classification, labelling and packaging of substances and mixtures (CLP).
                                   VOCs classified       as  carcinogenic, mutagenic or toxic for reproduction (CMR) of category 1A,
       VOCs classified    as CMR
                                   1B under Part 3 of Annex IV to          Regulation (EC) No 1272/2008 on classification, labelling
                  1AMB             and    packaging of substances and mixtures (CLP).
                                   VOCs classified       as  carcinogenic, mutagenic or toxic for reproduction (CMR) of category 2
      VOCs classified    as CMR 2 under Part 3 of Annex IV to Regulation            (EC) No 1272/2008 on classification, labelling and
                                   packaging of substances and mixtures             (CLP).
                                                                                Sheet 5. Endnotes
                                                                                                                                                        0000000191
</pre>

====================================================================== Einde pagina 109 =================================================================

<br><br>====================================================================== Pagina 110 ======================================================================

<pre>30141731
     Drawing  up of the WGC BREF
                                                                          4.1. Non-fug.     emissions
                                                                                                                                                 Back to
                                  An   inventory of non-fugitive emission      sources    consists of  the compilation    of relevant basic
                                                                                                                                                worksheet
     Is there an inventory of the data on the composition and quantity         of gas streams, and/or pieces of equipment in contact
                                  with these streams. The emitted streams are listed respective to their source, i.e. the
        equipment on the site?
                                  production    process from which     they originate.
                                  These include process emissions and purging emissions if these                 discharge  to  atmosphere,
                                  whether or not the discharge is through an abatement device.
          Atmospheric vents       Excluded: tank vent      emissions, loading vent emissions, emissions resulting from opening of
                                  process   vessels, whether resulting from operations or from maintenance activities.
                                  Loading/unloading      of ships, barges, trucks,    railcars   or other mobile    containers, whether
          Loading/unloading       fitted with  a vapour abatement device       or  not.
                 of vessels and   Opening    of process vessels, whether resulting from operations             (e.g. batch OFC    process)  or
       Opening
                 tanks            from maintenance activities (e.g. cleaning, inspection).
                                  Action of   sampling   and   emptying   of the sampling vessels      which from which emissions may
               Sampling
                                  Open    waste water collection     system, excluding emissions from          waste water treatment     plant
                Sewers
                                  equipment.
                        .         Vents of storage tanks, vents from cone roof tanks and pressure vacuum vent (PVV) from
             Tank  venting        tanks with nitrogen blanketing. Excluded: emissions from pressurised vessels and tank
        Waste water treatment     Waste water treatment       units, e.g. tanks, separators, dissolved air flotation.
                 plant
                                  If possible,   choose the   same   representative     year  as  the one  for which channelled emissions
           Year of reference
                                  have been     reported.
                                  All VOC substances       including  VOCs classified      as  carcinogenic, mutagenic      or toxic for
              Total VOCs          reproduction (CMR)       of category 1A, 1B under Part 3 of Annex [IV to Regulation (EC) No
                                  1272/2008      on classification, labelling and packaging of substances and mixtures (CLP).
                                  VOCs classified     as  carcinogenic, mutagenic or toxic for reproduction (CMR) of category 1A,
       VOCs classified    as CMR
                                  1B under Part 3 of Annex IV to       Regulation (EC) No 1272/2008 on classification, labelling
                 1AMB             and   packaging of substances and mixtures (CLP).
                                  VOCs classified     as  carcinogenic, mutagenic or toxic for reproduction (CMR) of category 2
      VOCs classified    as CMR 2 under Part 3 of Annex IV to Regulation         (EC) No 1272/2008 on classification, labelling and
                                  packaging of substances and mixtures           (CLP).
                                                                                    4.2. SMP
           Year of reference      Please   report the data of the SMP for the year considered            a  representative   year.
                                                                                                                                               |Backte      |
                                                                                                                                                worksheet
                                                                             Sheet 5. Endnotes
                                                                                                                                                          0000000192
</pre>

====================================================================== Einde pagina 110 =================================================================

<br><br>